Public Attributes | List of all members
iso_req_peer_sca_cmpl_evt_t Struct Reference
BLE » Core Isochronous Channels » Structures

The parameter for request peer sca complete event. More...

`#include <ble_iso.h>`

## Public Attributes
uint8_t | status
| 0x00: The SCA parameter received successfully.0x01-0xFF: The reception of SCA parameter failed More...
uint16_t | acl_hdl
| Connection handle of the ACL, (Range: 0x0000 to 0x0EFF). More...
uint8_t | sca
| See iso_sca_type_t. More...

## Detailed Description

The parameter for request peer sca complete event.

Definition at line 555 of file ble_iso.h.

## Member Data Documentation

## ◆ acl_hdl

uint16_t iso_req_peer_sca_cmpl_evt_t::acl_hdl

Connection handle of the ACL, (Range: 0x0000 to 0x0EFF).

Definition at line 558 of file ble_iso.h.

## ◆ sca

uint8_t iso_req_peer_sca_cmpl_evt_t::sca

See iso_sca_type_t.

Definition at line 559 of file ble_iso.h.

## ◆ status

uint8_t iso_req_peer_sca_cmpl_evt_t::status

0x00: The SCA parameter received successfully.0x01-0xFF: The reception of SCA parameter failed

Definition at line 557 of file ble_iso.h.

The documentation for this struct was generated from the following file:

- ble_iso.h