Macros
Clock Selection defines
Peripheral Driver » LL Driver » DDVS » Defines
Collaboration diagram for Clock Selection defines:

## Macros
#define | LL_DDVS_CLK_SEL_XO_32M (0U)
| DDVS Clock Select XO_32M. More...
#define | LL_DDVS_CLK_SEL_XO_16M (1U)
| DDVS Clock Select XO_16M. More...
#define | LL_DDVS_CLK_SEL_SYS_32M (2U)
| DDVS Clock Select SYS_32M. More...
#define | LL_DDVS_CLK_SEL_SYS_16M (3U)
| DDVS Clock Select SYS_16M. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_DDVS_CLK_SEL_SYS_16M

#define LL_DDVS_CLK_SEL_SYS_16M (3U)

DDVS Clock Select SYS_16M.

Definition at line 105 of file gr55xx_ll_ddvs.h.

## ◆ LL_DDVS_CLK_SEL_SYS_32M

#define LL_DDVS_CLK_SEL_SYS_32M (2U)

DDVS Clock Select SYS_32M.

Definition at line 104 of file gr55xx_ll_ddvs.h.

## ◆ LL_DDVS_CLK_SEL_XO_16M

#define LL_DDVS_CLK_SEL_XO_16M (1U)

DDVS Clock Select XO_16M.

Definition at line 103 of file gr55xx_ll_ddvs.h.

## ◆ LL_DDVS_CLK_SEL_XO_32M

#define LL_DDVS_CLK_SEL_XO_32M (0U)

DDVS Clock Select XO_32M.

Definition at line 102 of file gr55xx_ll_ddvs.h.