Macros
QSPI Interrupts
Peripheral Driver » HAL Driver » QSPI » Defines » QSPI Exported Constants
Collaboration diagram for QSPI Interrupts:

## Macros
#define | QSPI_IT_TXU LL_QSPI_IS_TXU
| Transmit FIFO Underflow Interrupt flag More...
#define | QSPI_IT_XRXO LL_QSPI_IS_XRXO
| XIP Receive FIFO Overflow Interrupt flag. More...
#define | QSPI_IT_MST LL_QSPI_IS_MST
| Multi-Master Contention Interrupt flag. More...
#define | QSPI_IT_RXF LL_QSPI_IS_RXF
| Receive FIFO Full Interrupt flag. More...
#define | QSPI_IT_RXO LL_QSPI_IS_RXO
| Receive FIFO Overflow Interrupt flag. More...
#define | QSPI_IT_RXU LL_QSPI_IS_RXU
| Receive FIFO Underflow Interrupt flag. More...
#define | QSPI_IT_TXO LL_QSPI_IS_TXO
| Transmit FIFO Overflow Interrupt flag. More...
#define | QSPI_IT_TXE LL_QSPI_IS_TXE
| Transmit FIFO Empty Interrupt flag. More...
#define | QSPI_IT_ALL LL_QSPI_IS_ALL
| ALL QSPI Interrupts flag. More...

## Detailed Description

## Macro Definition Documentation

## ◆ QSPI_IT_ALL

#define QSPI_IT_ALL LL_QSPI_IS_ALL

ALL QSPI Interrupts flag.

Definition at line 556 of file gr55xx_hal_qspi.h.

## ◆ QSPI_IT_MST

#define QSPI_IT_MST LL_QSPI_IS_MST

Multi-Master Contention Interrupt flag.

Definition at line 550 of file gr55xx_hal_qspi.h.

## ◆ QSPI_IT_RXF

#define QSPI_IT_RXF LL_QSPI_IS_RXF

Receive FIFO Full Interrupt flag.

Definition at line 551 of file gr55xx_hal_qspi.h.

## ◆ QSPI_IT_RXO

#define QSPI_IT_RXO LL_QSPI_IS_RXO

Receive FIFO Overflow Interrupt flag.

Definition at line 552 of file gr55xx_hal_qspi.h.

## ◆ QSPI_IT_RXU

#define QSPI_IT_RXU LL_QSPI_IS_RXU

Receive FIFO Underflow Interrupt flag.

Definition at line 553 of file gr55xx_hal_qspi.h.

## ◆ QSPI_IT_TXE

#define QSPI_IT_TXE LL_QSPI_IS_TXE

Transmit FIFO Empty Interrupt flag.

Definition at line 555 of file gr55xx_hal_qspi.h.

## ◆ QSPI_IT_TXO

#define QSPI_IT_TXO LL_QSPI_IS_TXO

Transmit FIFO Overflow Interrupt flag.

Definition at line 554 of file gr55xx_hal_qspi.h.

## ◆ QSPI_IT_TXU

#define QSPI_IT_TXU LL_QSPI_IS_TXU

Transmit FIFO Underflow Interrupt flag

Definition at line 548 of file gr55xx_hal_qspi.h.

## ◆ QSPI_IT_XRXO

#define QSPI_IT_XRXO LL_QSPI_IS_XRXO

XIP Receive FIFO Overflow Interrupt flag.

Definition at line 549 of file gr55xx_hal_qspi.h.