Public Attributes | List of all members
ble_gap_peer_features_ind_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Structures

LE features info. More...

`#include <ble_gapc.h>`

## Public Attributes
uint8_t | features [BLE_GAP_FEATS_LEN]
| 8-byte array for LE features Feature Setting field's bit mapping to Controller Features (0: not support, 1: support) More...

## Detailed Description

LE features info.

Definition at line 426 of file ble_gapc.h.

## Member Data Documentation

## ◆ features

uint8_t ble_gap_peer_features_ind_t::features[BLE_GAP_FEATS_LEN]

8-byte array for LE features
Feature Setting field's bit mapping to Controller Features (0: not support, 1: support)

Bit position | Link Layer Feature
--- | ---
0 | LE Encryption
1 | Connection Parameters Request Procedure
2 | Extended Reject Indication
3 | Slave-initiated Features Exchange
4 | LE Ping
5 | LE Data Packet Length Extension
6 | LL Privacy
7 | Extended Scanner Filter Policies
8 | LE 2M PHY
9 | Stable Modulation Index - Transmitter
10 | Stable Modulation Index - Receiver
11 | LE Coded PHY
12 | LE Extended Advertising
13 | LE Periodic Advertising
14 | Channel Selection Algorithm #2
15 | LE Power Class 1
16 | Minimum Number of Used Channels Procedure
17 | Connection CTE Request
18 | Connection CTE Response
19 | Connectionless CTE Transmitter
20 | Connectionless CTE Receiver
21 | Antenna Switching During CTE Transmission(AoD)
22 | Antenna Switching During CTE Reception(AoA)
23 | Receiving Constant Tone Extensions
24 | Periodic Advertising Sync Transfer - Sender
25 | Periodic Advertising Sync Transfer - Recipient
26 | Sleep Clock Accuracy Updates
27 | Remote Public Key Validation
33 | LE Power Control Request
34 | LE Power Change Indication
35 | LE Path Loss Monitoring

|All other values |Reserved for Future Use|

Definition at line 428 of file ble_gapc.h.

The documentation for this struct was generated from the following file:

- ble_gapc.h