Public Attributes | List of all members
ble_gap_evt_sync_established_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Management » Structures

Sync established event for BLE_GAPM_EVT_SYNC_ESTABLISH. More...

`#include <ble_gapm.h>`

Collaboration diagram for ble_gap_evt_sync_established_t:
[legend]

## Public Attributes
uint8_t | phy
| PHY on which synchronization has been established. More...
uint16_t | intv
| Periodic advertising interval (in unit of 1.25ms, min is 7.5ms). More...
uint8_t | adv_sid
| Advertising SID. More...
uint8_t | clk_acc
| Advertiser clock accuracy. More...
ble_gap_bdaddr_t | bd_addr
| Advertiser address. More...
uint16_t | sync_hdl
| Sync handle. More...

## Detailed Description

Sync established event for BLE_GAPM_EVT_SYNC_ESTABLISH.

Definition at line 907 of file ble_gapm.h.

## Member Data Documentation

## ◆ adv_sid

uint8_t ble_gap_evt_sync_established_t::adv_sid

Advertising SID.

Definition at line 911 of file ble_gapm.h.

## ◆ bd_addr

ble_gap_bdaddr_t ble_gap_evt_sync_established_t::bd_addr

Advertiser address.

Definition at line 913 of file ble_gapm.h.

## ◆ clk_acc

uint8_t ble_gap_evt_sync_established_t::clk_acc

Advertiser clock accuracy.

Definition at line 912 of file ble_gapm.h.

## ◆ intv

uint16_t ble_gap_evt_sync_established_t::intv

Periodic advertising interval (in unit of 1.25ms, min is 7.5ms).

Definition at line 910 of file ble_gapm.h.

## ◆ phy

uint8_t ble_gap_evt_sync_established_t::phy

PHY on which synchronization has been established.

Definition at line 909 of file ble_gapm.h.

## ◆ sync_hdl

uint16_t ble_gap_evt_sync_established_t::sync_hdl

Sync handle.

Definition at line 914 of file ble_gapm.h.

The documentation for this struct was generated from the following file:

- ble_gapm.h