### - h -

- HAL_ADC_STATE_BUSY : gr55xx_hal_adc.h
- HAL_ADC_STATE_ERROR : gr55xx_hal_adc.h
- HAL_ADC_STATE_READY : gr55xx_hal_adc.h
- HAL_ADC_STATE_RESET : gr55xx_hal_adc.h
- HAL_AES_STATE_BUSY : gr55xx_hal_aes.h
- HAL_AES_STATE_ERROR : gr55xx_hal_aes.h
- HAL_AES_STATE_READY : gr55xx_hal_aes.h
- HAL_AES_STATE_RESET : gr55xx_hal_aes.h
- HAL_AES_STATE_SUSPENDED : gr55xx_hal_aes.h
- HAL_AES_STATE_TIMEOUT : gr55xx_hal_aes.h
- HAL_BUSY : gr55xx_hal_def.h
- HAL_COMP_STATE_BUSY : gr55xx_hal_comp.h
- HAL_COMP_STATE_ERROR : gr55xx_hal_comp.h
- HAL_COMP_STATE_READY : gr55xx_hal_comp.h
- HAL_COMP_STATE_RESET : gr55xx_hal_comp.h
- HAL_DMA_STATE_BUSY : gr55xx_hal_dma.h
- HAL_DMA_STATE_ERROR : gr55xx_hal_dma.h
- HAL_DMA_STATE_READY : gr55xx_hal_dma.h
- HAL_DMA_STATE_RESET : gr55xx_hal_dma.h
- HAL_DMA_STATE_TIMEOUT : gr55xx_hal_dma.h
- HAL_DMA_XFER_ABORT_CB_ID : gr55xx_hal_dma.h
- HAL_DMA_XFER_ALL_CB_ID : gr55xx_hal_dma.h
- HAL_DMA_XFER_BLK_CB_ID : gr55xx_hal_dma.h
- HAL_DMA_XFER_ERROR_CB_ID : gr55xx_hal_dma.h
- HAL_DMA_XFER_TFR_CB_ID : gr55xx_hal_dma.h
- HAL_DSPI_STATE_ABORT : gr55xx_hal_dspi.h
- HAL_DSPI_STATE_BUSY : gr55xx_hal_dspi.h
- HAL_DSPI_STATE_BUSY_INDIRECT_TX : gr55xx_hal_dspi.h
- HAL_DSPI_STATE_ERROR : gr55xx_hal_dspi.h
- HAL_DSPI_STATE_READY : gr55xx_hal_dspi.h
- HAL_DSPI_STATE_RESET : gr55xx_hal_dspi.h
- HAL_DUAL_TIMER_STATE_BUSY : gr55xx_hal_dual_tim.h
- HAL_DUAL_TIMER_STATE_ERROR : gr55xx_hal_dual_tim.h
- HAL_DUAL_TIMER_STATE_READY : gr55xx_hal_dual_tim.h
- HAL_DUAL_TIMER_STATE_RESET : gr55xx_hal_dual_tim.h
- HAL_EFUSE_STATE_BUSY : gr55xx_hal_efuse.h
- HAL_EFUSE_STATE_ERROR : gr55xx_hal_efuse.h
- HAL_EFUSE_STATE_READY : gr55xx_hal_efuse.h
- HAL_EFUSE_STATE_RESET : gr55xx_hal_efuse.h
- HAL_ERROR : gr55xx_hal_def.h
- HAL_EXFLASH_ENCRYPTED : gr55xx_hal_exflash.h
- HAL_EXFLASH_STATE_BUSY : gr55xx_hal_exflash.h
- HAL_EXFLASH_STATE_BUSY_ERASE : gr55xx_hal_exflash.h
- HAL_EXFLASH_STATE_BUSY_READ : gr55xx_hal_exflash.h
- HAL_EXFLASH_STATE_BUSY_WRITE : gr55xx_hal_exflash.h
- HAL_EXFLASH_STATE_ERROR : gr55xx_hal_exflash.h
- HAL_EXFLASH_STATE_READY : gr55xx_hal_exflash.h
- HAL_EXFLASH_STATE_RESET : gr55xx_hal_exflash.h
- HAL_EXFLASH_STATE_SUSPEND_ERASE : gr55xx_hal_exflash.h
- HAL_EXFLASH_STATE_SUSPEND_WRITE : gr55xx_hal_exflash.h
- HAL_EXFLASH_UNENCRYPTED : gr55xx_hal_exflash.h
- HAL_GDC_ABGR8888 : hal_gdc.h
- HAL_GDC_ABGR8888_CHK : hal_gdc_intern.h
- HAL_GDC_ARGB4444 : hal_gdc.h
- HAL_GDC_ARGB4444_CHK : hal_gdc_intern.h
- HAL_GDC_ARGB8888 : hal_gdc.h
- HAL_GDC_ARGB8888_CHK : hal_gdc_intern.h
- HAL_GDC_AXI_128BEAT : hal_gdc_intern.h
- HAL_GDC_AXI_16BEAT : hal_gdc_intern.h
- HAL_GDC_AXI_2BEAT : hal_gdc_intern.h
- HAL_GDC_AXI_32BEAT : hal_gdc_intern.h
- HAL_GDC_AXI_4BEAT : hal_gdc_intern.h
- HAL_GDC_AXI_64BEAT : hal_gdc_intern.h
- HAL_GDC_AXI_8BEAT : hal_gdc_intern.h
- HAL_GDC_AXI_FT_2B : hal_gdc_intern.h
- HAL_GDC_AXI_FT_4B : hal_gdc_intern.h
- HAL_GDC_AXI_FT_8B : hal_gdc_intern.h
- HAL_GDC_AXI_FT_HF : hal_gdc_intern.h
- HAL_GDC_BF_DSTALPHA : hal_gdc.h
- HAL_GDC_BF_GLBALPHA : hal_gdc.h
- HAL_GDC_BF_INVDSTALPHA : hal_gdc.h
- HAL_GDC_BF_INVGBLALPHA : hal_gdc.h
- HAL_GDC_BF_INVSRCALPHA : hal_gdc.h
- HAL_GDC_BF_INVSRCGBLALPHA : hal_gdc.h
- HAL_GDC_BF_ONE : hal_gdc.h
- HAL_GDC_BF_SRCALPHA : hal_gdc.h
- HAL_GDC_BF_SRCGBLALPHA : hal_gdc.h
- HAL_GDC_BF_ZERO : hal_gdc.h
- HAL_GDC_BGRA8888 : hal_gdc.h
- HAL_GDC_BGRA8888_CHK : hal_gdc_intern.h
- HAL_GDC_BL_ADD : hal_gdc.h
- HAL_GDC_BL_CLEAR : hal_gdc.h
- HAL_GDC_BL_DST_ATOP : hal_gdc.h
- HAL_GDC_BL_DST_IN : hal_gdc.h
- HAL_GDC_BL_DST_OUT : hal_gdc.h
- HAL_GDC_BL_DST_OVER : hal_gdc.h
- HAL_GDC_BL_SIMPLE : hal_gdc.h
- HAL_GDC_BL_SRC : hal_gdc.h
- HAL_GDC_BL_SRC_ATOP : hal_gdc.h
- HAL_GDC_BL_SRC_IN : hal_gdc.h
- HAL_GDC_BL_SRC_OUT : hal_gdc.h
- HAL_GDC_BL_SRC_OVER : hal_gdc.h
- HAL_GDC_BL_XOR : hal_gdc.h
- HAL_GDC_BLANK : hal_gdc.h
- HAL_GDC_BLOCK4X4_CHK : hal_gdc_intern.h
- HAL_GDC_BT656 : hal_gdc.h
- HAL_GDC_CFG_DBIB : hal_gdc.h
- HAL_GDC_CFG_DITHERING : hal_gdc.h
- HAL_GDC_CFG_FIXED_CURSOR : hal_gdc.h
- HAL_GDC_CFG_FORMAT : hal_gdc.h
- HAL_GDC_CFG_HiQ_YUV : hal_gdc.h
- HAL_GDC_CFG_L0_BLENDER : hal_gdc.h
- HAL_GDC_CFG_L0_ENABLED : hal_gdc.h
- HAL_GDC_CFG_L0_GAMMA : hal_gdc.h
- HAL_GDC_CFG_L0_SCALER : hal_gdc.h
- HAL_GDC_CFG_L0_YUVMEM : hal_gdc.h
- HAL_GDC_CFG_L1_BLENDER : hal_gdc.h
- HAL_GDC_CFG_L1_ENABLED : hal_gdc.h
- HAL_GDC_CFG_L1_GAMMA : hal_gdc.h
- HAL_GDC_CFG_L1_SCALER : hal_gdc.h
- HAL_GDC_CFG_L1_YUVMEM : hal_gdc.h
- HAL_GDC_CFG_L2_BLENDER : hal_gdc.h
- HAL_GDC_CFG_L2_ENABLED : hal_gdc.h
- HAL_GDC_CFG_L2_GAMMA : hal_gdc.h
- HAL_GDC_CFG_L2_SCALER : hal_gdc.h
- HAL_GDC_CFG_L2_YUVMEM : hal_gdc.h
- HAL_GDC_CFG_L3_BLENDER : hal_gdc.h
- HAL_GDC_CFG_L3_ENABLED : hal_gdc.h
- HAL_GDC_CFG_L3_GAMMA : hal_gdc.h
- HAL_GDC_CFG_L3_SCALER : hal_gdc.h
- HAL_GDC_CFG_PALETTE : hal_gdc.h
- HAL_GDC_CFG_PROGR_CURSOR : hal_gdc.h
- HAL_GDC_CFG_SPI : hal_gdc.h
- HAL_GDC_CFG_YUVOUT : hal_gdc.h
- hal_gdc_clkctrl_cg_bypass_clk : hal_gdc.h
- hal_gdc_clkctrl_cg_clk_en : hal_gdc.h
- hal_gdc_clkctrl_cg_clk_inv : hal_gdc.h
- hal_gdc_clkctrl_cg_clk_swap : hal_gdc.h
- hal_gdc_clkctrl_cg_l0_bus_clk : hal_gdc.h
- hal_gdc_clkctrl_cg_l0_pix_clk : hal_gdc.h
- hal_gdc_clkctrl_cg_l1_bus_clk : hal_gdc.h
- hal_gdc_clkctrl_cg_l1_pix_clk : hal_gdc.h
- hal_gdc_clkctrl_cg_l2_bus_clk : hal_gdc.h
- hal_gdc_clkctrl_cg_l2_pix_clk : hal_gdc.h
- hal_gdc_clkctrl_cg_l3_pix_clk : hal_gdc.h
- hal_gdc_clkctrl_cg_regfil_clk : hal_gdc.h
- hal_gdc_clkctrl_cg_rsrvd_10 : hal_gdc.h
- hal_gdc_clkctrl_cg_rsrvd_11 : hal_gdc.h
- hal_gdc_clkctrl_cg_rsrvd_12 : hal_gdc.h
- hal_gdc_clkctrl_cg_rsrvd_13 : hal_gdc.h
- hal_gdc_clkctrl_cg_rsrvd_14 : hal_gdc.h
- hal_gdc_clkctrl_cg_rsrvd_15 : hal_gdc.h
- hal_gdc_clkctrl_cg_rsrvd_16 : hal_gdc.h
- hal_gdc_clkctrl_cg_rsrvd_17 : hal_gdc.h
- hal_gdc_clkctrl_cg_rsrvd_18 : hal_gdc.h
- hal_gdc_clkctrl_cg_rsrvd_19 : hal_gdc.h
- hal_gdc_clkctrl_cg_rsrvd_20 : hal_gdc.h
- hal_gdc_clkctrl_cg_rsrvd_21 : hal_gdc.h
- hal_gdc_clkctrl_cg_rsrvd_3 : hal_gdc.h
- hal_gdc_clkctrl_cg_rsrvd_4 : hal_gdc.h
- hal_gdc_clkctrl_cg_rsrvd_5 : hal_gdc.h
- hal_gdc_clkctrl_cg_rsrvd_6 : hal_gdc.h
- hal_gdc_clkctrl_cg_rsrvd_7 : hal_gdc.h
- hal_gdc_clkctrl_cg_rsrvd_8 : hal_gdc.h
- hal_gdc_clkctrl_cg_rsrvd_9 : hal_gdc.h
- HAL_GDC_CLKOUTDIV : hal_gdc.h
- HAL_GDC_CURSOR : hal_gdc.h
- hal_gdc_DBI_cmd : hal_gdc_intern.h
- hal_gdc_DBI_ge : hal_gdc_intern.h
- hal_gdc_DBI_read : hal_gdc_intern.h
- HAL_GDC_DBIB_STALL_CHK : hal_gdc_intern.h
- HAL_GDC_DISABLE : hal_gdc.h
- HAL_GDC_DITHER : hal_gdc.h
- HAL_GDC_DITHER15 : hal_gdc.h
- HAL_GDC_DITHER16 : hal_gdc.h
- HAL_GDC_EN_CFCLK : hal_gdc.h
- HAL_GDC_EN_L0BUS : hal_gdc.h
- HAL_GDC_EN_L0PIX : hal_gdc.h
- HAL_GDC_EN_L1BUS : hal_gdc.h
- HAL_GDC_EN_L1PIX : hal_gdc.h
- HAL_GDC_EN_L2BUS : hal_gdc.h
- HAL_GDC_EN_L2PIX : hal_gdc.h
- HAL_GDC_EN_L3BUS : hal_gdc.h
- HAL_GDC_EN_PIXCLK : hal_gdc.h
- hal_gdc_ext_ctrl : hal_gdc_intern.h
- HAL_GDC_EXTRCTRL_CHK : hal_gdc_intern.h
- HAL_GDC_FORCE_A : hal_gdc.h
- HAL_GDC_GAMMA : hal_gdc.h
- HAL_GDC_GPI_CHK : hal_gdc_intern.h
- HAL_GDC_INTERLACE : hal_gdc.h
- HAL_GDC_INVPIXCLK : hal_gdc.h
- HAL_GDC_JDIMIP : hal_gdc.h
- HAL_GDC_JDIMIP_CHK : hal_gdc_intern.h
- HAL_GDC_L1 : hal_gdc.h
- HAL_GDC_L1_CHK : hal_gdc_intern.h
- HAL_GDC_L4 : hal_gdc.h
- HAL_GDC_L4_CHK : hal_gdc_intern.h
- HAL_GDC_L8 : hal_gdc.h
- HAL_GDC_L8_CHK : hal_gdc_intern.h
- HAL_GDC_LAYER_AHBLOCK : hal_gdc.h
- HAL_GDC_LAYER_DISABLE : hal_gdc.h
- HAL_GDC_LAYER_GAMMALUT_EN : hal_gdc.h
- HAL_GDC_LUT8 : hal_gdc.h
- HAL_GDC_LUT8_CHK : hal_gdc_intern.h
- HAL_GDC_LVDS_ISP68 : hal_gdc.h
- HAL_GDC_LVDS_ISP8 : hal_gdc.h
- HAL_GDC_LVDS_OFF : hal_gdc.h
- HAL_GDC_LVDSPADS : hal_gdc.h
- hal_gdc_mask_qspi : hal_gdc_intern.h
- HAL_GDC_MIPI_OFF : hal_gdc.h
- HAL_GDC_MODULATE_A : hal_gdc.h
- HAL_GDC_NEG_DE : hal_gdc.h
- HAL_GDC_NEG_H : hal_gdc.h
- HAL_GDC_NEG_V : hal_gdc.h
- HAL_GDC_ONE_FRAME : hal_gdc.h
- HAL_GDC_OPENLDI_CHK : hal_gdc_intern.h
- HAL_GDC_OUTP_OFF : hal_gdc.h
- HAL_GDC_P_RGB3 : hal_gdc.h
- HAL_GDC_P_RGB3_16B : hal_gdc.h
- HAL_GDC_P_RGB3_16B1 : hal_gdc.h
- HAL_GDC_P_RGB3_16B2 : hal_gdc.h
- HAL_GDC_P_RGB3_18B : hal_gdc.h
- HAL_GDC_P_RGB3_18B1 : hal_gdc.h
- HAL_GDC_PALETTE : hal_gdc.h
- hal_gdc_rcmd16 : hal_gdc_intern.h
- hal_gdc_rcmd24 : hal_gdc_intern.h
- hal_gdc_rcmd32 : hal_gdc_intern.h
- hal_gdc_read_2byte : hal_gdc_intern.h
- hal_gdc_read_3byte : hal_gdc_intern.h
- hal_gdc_read_4byte : hal_gdc_intern.h
- hal_gdc_read_byte : hal_gdc_intern.h
- HAL_GDC_RGB24 : hal_gdc.h
- HAL_GDC_RGB24_CHK : hal_gdc_intern.h
- HAL_GDC_RGB332 : hal_gdc.h
- HAL_GDC_RGB332_CHK : hal_gdc_intern.h
- HAL_GDC_RGB565 : hal_gdc.h
- HAL_GDC_RGB565_CHK : hal_gdc_intern.h
- HAL_GDC_RGBA4444 : hal_gdc.h
- HAL_GDC_RGBA4444_CHK : hal_gdc_intern.h
- HAL_GDC_RGBA5551 : hal_gdc.h
- HAL_GDC_RGBA5551_CHK : hal_gdc_intern.h
- HAL_GDC_RGBA8888 : hal_gdc.h
- HAL_GDC_RGBA8888_CHK : hal_gdc_intern.h
- HAL_GDC_S_12BIT : hal_gdc.h
- HAL_GDC_S_RGB3 : hal_gdc.h
- HAL_GDC_S_RGBX4 : hal_gdc.h
- HAL_GDC_SCALE_NN : hal_gdc.h
- HAL_GDC_SCANDOUBLE : hal_gdc.h
- HAL_GDC_SINGLEV : hal_gdc.h
- hal_gdc_sline_cmd : hal_gdc_intern.h
- hal_gdc_snapshot : hal_gdc_intern.h
- hal_gdc_store_base_addr : hal_gdc_intern.h
- HAL_GDC_T_16BIT : hal_gdc.h
- HAL_GDC_TESTMODE : hal_gdc.h
- HAL_GDC_TLYUV420 : hal_gdc.h
- HAL_GDC_TLYUV420_CHK : hal_gdc_intern.h
- HAL_GDC_TSC4 : hal_gdc.h
- HAL_GDC_TSC6 : hal_gdc.h
- HAL_GDC_TSC6_CHK : hal_gdc_intern.h
- HAL_GDC_TSC6A : hal_gdc.h
- HAL_GDC_TSC_CHK : hal_gdc_intern.h
- HAL_GDC_V_YUV420 : hal_gdc.h
- HAL_GDC_V_YUV420_CHK : hal_gdc_intern.h
- hal_gdc_wcmd16 : hal_gdc_intern.h
- hal_gdc_wcmd24 : hal_gdc_intern.h
- hal_gdc_wcmd32 : hal_gdc_intern.h
- HAL_GDC_YUVOUT : hal_gdc.h
- HAL_GDC_YUVV_CHK : hal_gdc_intern.h
- HAL_GDC_YUY2 : hal_gdc.h
- HAL_GDC_YUY2_CHK : hal_gdc_intern.h
- HAL_GDC_YUYV : hal_gdc.h
- HAL_GFX_CULL_ALL : hal_gfx_graphics.h
- HAL_GFX_CULL_CCW : hal_gfx_graphics.h
- HAL_GFX_CULL_CW : hal_gfx_graphics.h
- HAL_GFX_CULL_NONE : hal_gfx_graphics.h
- HAL_GFX_NOTEX : hal_gfx_graphics.h
- HAL_GFX_TEX0 : hal_gfx_graphics.h
- HAL_GFX_TEX1 : hal_gfx_graphics.h
- HAL_GFX_TEX2 : hal_gfx_graphics.h
- HAL_GFX_TEX3 : hal_gfx_graphics.h
- HAL_GFX_TRANS_COVER : hal_gfx_transitions.h
- HAL_GFX_TRANS_CUBE_H : hal_gfx_transitions.h
- HAL_GFX_TRANS_CUBE_V : hal_gfx_transitions.h
- HAL_GFX_TRANS_FADE : hal_gfx_transitions.h
- HAL_GFX_TRANS_FADE_ZOOM : hal_gfx_transitions.h
- HAL_GFX_TRANS_INNERCUBE_H : hal_gfx_transitions.h
- HAL_GFX_TRANS_INNERCUBE_V : hal_gfx_transitions.h
- HAL_GFX_TRANS_LINEAR_H : hal_gfx_transitions.h
- HAL_GFX_TRANS_LINEAR_V : hal_gfx_transitions.h
- HAL_GFX_TRANS_MAX : hal_gfx_transitions.h
- HAL_GFX_TRANS_NONE : hal_gfx_transitions.h
- HAL_GFX_TRANS_PUSHPULL_H : hal_gfx_transitions.h
- HAL_GFX_TRANS_PUSHPULL_V : hal_gfx_transitions.h
- HAL_GFX_TRANS_SPIN_H_L2R : hal_gfx_transitions.h
- HAL_GFX_TRANS_SPIN_H_R2L : hal_gfx_transitions.h
- HAL_GFX_TRANS_STACK_H : hal_gfx_transitions.h
- HAL_GFX_TRANS_STACK_V : hal_gfx_transitions.h
- HAL_HMAC_STATE_BUSY : gr55xx_hal_hmac.h
- HAL_HMAC_STATE_ERROR : gr55xx_hal_hmac.h
- HAL_HMAC_STATE_READY : gr55xx_hal_hmac.h
- HAL_HMAC_STATE_RESET : gr55xx_hal_hmac.h
- HAL_HMAC_STATE_SUSPENDED : gr55xx_hal_hmac.h
- HAL_HMAC_STATE_TIMEOUT : gr55xx_hal_hmac.h
- HAL_I2C_MODE_MASTER : gr55xx_hal_i2c.h
- HAL_I2C_MODE_NONE : gr55xx_hal_i2c.h
- HAL_I2C_MODE_SLAVE : gr55xx_hal_i2c.h
- HAL_I2C_STATE_ABORT : gr55xx_hal_i2c.h
- HAL_I2C_STATE_BUSY : gr55xx_hal_i2c.h
- HAL_I2C_STATE_BUSY_RX : gr55xx_hal_i2c.h
- HAL_I2C_STATE_BUSY_TX : gr55xx_hal_i2c.h
- HAL_I2C_STATE_ERROR : gr55xx_hal_i2c.h
- HAL_I2C_STATE_READY : gr55xx_hal_i2c.h
- HAL_I2C_STATE_RESET : gr55xx_hal_i2c.h
- HAL_I2C_STATE_TIMEOUT : gr55xx_hal_i2c.h
- HAL_I2S_STATE_ABORT : gr55xx_hal_i2s.h
- HAL_I2S_STATE_BUSY : gr55xx_hal_i2s.h
- HAL_I2S_STATE_BUSY_RX : gr55xx_hal_i2s.h
- HAL_I2S_STATE_BUSY_TX : gr55xx_hal_i2s.h
- HAL_I2S_STATE_BUSY_TX_RX : gr55xx_hal_i2s.h
- HAL_I2S_STATE_ERROR : gr55xx_hal_i2s.h
- HAL_I2S_STATE_READY : gr55xx_hal_i2s.h
- HAL_I2S_STATE_RESET : gr55xx_hal_i2s.h
- HAL_ISO7816_STATE_ABORT : gr55xx_hal_iso7816.h
- HAL_ISO7816_STATE_BUSY : gr55xx_hal_iso7816.h
- HAL_ISO7816_STATE_BUSY_RX : gr55xx_hal_iso7816.h
- HAL_ISO7816_STATE_BUSY_TX : gr55xx_hal_iso7816.h
- HAL_ISO7816_STATE_BUSY_TX_RX : gr55xx_hal_iso7816.h
- HAL_ISO7816_STATE_ERROR : gr55xx_hal_iso7816.h
- HAL_ISO7816_STATE_READY : gr55xx_hal_iso7816.h
- HAL_ISO7816_STATE_RESET : gr55xx_hal_iso7816.h
- HAL_ISO7816_STATE_TIMEOUT : gr55xx_hal_iso7816.h
- HAL_LOCKED : gr55xx_hal_def.h
- HAL_MMAPPED_STATE_ACTIVED : gr55xx_hal_qspi.h
- HAL_MMAPPED_STATE_DEACTIVED : gr55xx_hal_qspi.h
- HAL_MMAPPED_STATE_ERROR : gr55xx_hal_qspi.h
- HAL_OK : gr55xx_hal_def.h
- HAL_PDM_STATE_BUSY : gr55xx_hal_pdm.h
- HAL_PDM_STATE_ERROR : gr55xx_hal_pdm.h
- HAL_PDM_STATE_READY : gr55xx_hal_pdm.h
- HAL_PDM_STATE_RESET : gr55xx_hal_pdm.h
- HAL_PKC_STATE_BUSY : gr55xx_hal_pkc.h
- HAL_PKC_STATE_ERROR : gr55xx_hal_pkc.h
- HAL_PKC_STATE_READY : gr55xx_hal_pkc.h
- HAL_PKC_STATE_RESET : gr55xx_hal_pkc.h
- HAL_PKC_STATE_TIMEOUT : gr55xx_hal_pkc.h
- HAL_PWM_ACTIVE_CHANNEL_A : gr55xx_hal_pwm.h
- HAL_PWM_ACTIVE_CHANNEL_ALL : gr55xx_hal_pwm.h
- HAL_PWM_ACTIVE_CHANNEL_B : gr55xx_hal_pwm.h
- HAL_PWM_ACTIVE_CHANNEL_C : gr55xx_hal_pwm.h
- HAL_PWM_ACTIVE_CHANNEL_CLEARED : gr55xx_hal_pwm.h
- HAL_PWM_STATE_BUSY : gr55xx_hal_pwm.h
- HAL_PWM_STATE_ERROR : gr55xx_hal_pwm.h
- HAL_PWM_STATE_READY : gr55xx_hal_pwm.h
- HAL_PWM_STATE_RESET : gr55xx_hal_pwm.h
- HAL_QSPI_STATE_ABORT : gr55xx_hal_qspi.h
- HAL_QSPI_STATE_BUSY : gr55xx_hal_qspi.h
- HAL_QSPI_STATE_BUSY_INDIRECT_RX : gr55xx_hal_qspi.h
- HAL_QSPI_STATE_BUSY_INDIRECT_TX : gr55xx_hal_qspi.h
- HAL_QSPI_STATE_BUSY_MEM_MAPPED : gr55xx_hal_qspi.h
- HAL_QSPI_STATE_ERROR : gr55xx_hal_qspi.h
- HAL_QSPI_STATE_READY : gr55xx_hal_qspi.h
- HAL_QSPI_STATE_RESET : gr55xx_hal_qspi.h
- HAL_RNG_STATE_BUSY : gr55xx_hal_rng.h
- HAL_RNG_STATE_ERROR : gr55xx_hal_rng.h
- HAL_RNG_STATE_READY : gr55xx_hal_rng.h
- HAL_RNG_STATE_RESET : gr55xx_hal_rng.h
- HAL_RNG_STATE_TIMEOUT : gr55xx_hal_rng.h
- HAL_RTC_ERROR : gr55xx_hal_rtc.h
- HAL_RTC_READY : gr55xx_hal_rtc.h
- HAL_RTC_RESET : gr55xx_hal_rtc.h
- HAL_RTC_RUNNING : gr55xx_hal_rtc.h
- HAL_SPI_STATE_ABORT : gr55xx_hal_spi.h
- HAL_SPI_STATE_BUSY : gr55xx_hal_spi.h
- HAL_SPI_STATE_BUSY_RX : gr55xx_hal_spi.h
- HAL_SPI_STATE_BUSY_TX : gr55xx_hal_spi.h
- HAL_SPI_STATE_BUSY_TX_RX : gr55xx_hal_spi.h
- HAL_SPI_STATE_ERROR : gr55xx_hal_spi.h
- HAL_SPI_STATE_READY : gr55xx_hal_spi.h
- HAL_SPI_STATE_RESET : gr55xx_hal_spi.h
- HAL_TIMEOUT : gr55xx_hal_def.h
- HAL_TIMER_STATE_BUSY : gr55xx_hal_tim.h
- HAL_TIMER_STATE_ERROR : gr55xx_hal_tim.h
- HAL_TIMER_STATE_READY : gr55xx_hal_tim.h
- HAL_TIMER_STATE_RESET : gr55xx_hal_tim.h
- HAL_UART_STATE_BUSY : gr55xx_hal_uart.h
- HAL_UART_STATE_BUSY_RX : gr55xx_hal_uart.h
- HAL_UART_STATE_BUSY_TX : gr55xx_hal_uart.h
- HAL_UART_STATE_BUSY_TXRX : gr55xx_hal_uart.h
- HAL_UART_STATE_ERROR : gr55xx_hal_uart.h
- HAL_UART_STATE_READY : gr55xx_hal_uart.h
- HAL_UART_STATE_RESET : gr55xx_hal_uart.h
- HAL_UART_STATE_TIMEOUT : gr55xx_hal_uart.h
- HAL_UNLOCKED : gr55xx_hal_def.h
- HAL_USB_EP0 : gr55xx_hal_usb.h
- HAL_USB_EP1 : gr55xx_hal_usb.h
- HAL_USB_EP2 : gr55xx_hal_usb.h
- HAL_USB_EP3 : gr55xx_hal_usb.h
- HAL_USB_EP4 : gr55xx_hal_usb.h
- HAL_USB_EP5 : gr55xx_hal_usb.h
- HAL_USB_STATE_ABORT : gr55xx_hal_usb.h
- HAL_USB_STATE_BUSY : gr55xx_hal_usb.h
- HAL_USB_STATE_BUSY_ADDR : gr55xx_hal_usb.h
- HAL_USB_STATE_BUSY_CFG : gr55xx_hal_usb.h
- HAL_USB_STATE_BUSY_HOST_REST : gr55xx_hal_usb.h
- HAL_USB_STATE_ERROR : gr55xx_hal_usb.h
- HAL_USB_STATE_ERROR_BIT_STUFF : gr55xx_hal_usb.h
- HAL_USB_STATE_ERROR_BYTE : gr55xx_hal_usb.h
- HAL_USB_STATE_ERROR_CRC16 : gr55xx_hal_usb.h
- HAL_USB_STATE_ERROR_DMA_RX : gr55xx_hal_usb.h
- HAL_USB_STATE_ERROR_EP5_TIMER : gr55xx_hal_usb.h
- HAL_USB_STATE_ERROR_NSE : gr55xx_hal_usb.h
- HAL_USB_STATE_ERROR_PID_CKS : gr55xx_hal_usb.h
- HAL_USB_STATE_ERROR_PID_CRC : gr55xx_hal_usb.h
- HAL_USB_STATE_ERROR_SEQ : gr55xx_hal_usb.h
- HAL_USB_STATE_ERROR_SYNC : gr55xx_hal_usb.h
- HAL_USB_STATE_ERROR_TIMEOUT : gr55xx_hal_usb.h
- HAL_USB_STATE_ERROR_UPID : gr55xx_hal_usb.h
- HAL_USB_STATE_READY : gr55xx_hal_usb.h
- HAL_USB_STATE_RESET : gr55xx_hal_usb.h
- HAL_USB_STATE_SUSPEND : gr55xx_hal_usb.h
- HAL_XQSPI_STATE_ABORT : gr55xx_hal_xqspi.h
- HAL_XQSPI_STATE_BUSY : gr55xx_hal_xqspi.h
- HAL_XQSPI_STATE_BUSY_INDIRECT_RX : gr55xx_hal_xqspi.h
- HAL_XQSPI_STATE_BUSY_INDIRECT_TX : gr55xx_hal_xqspi.h
- HAL_XQSPI_STATE_ERROR : gr55xx_hal_xqspi.h
- HAL_XQSPI_STATE_READY : gr55xx_hal_xqspi.h
- HAL_XQSPI_STATE_RESET : gr55xx_hal_xqspi.h
- HIDS_EVT_BOOT_MODE_ENTERED : hids.h
- HIDS_EVT_HOST_EXIT_SUSP : hids.h
- HIDS_EVT_HOST_SUSP : hids.h
- HIDS_EVT_IN_REP_NOTIFY_DISABLED : hids.h
- HIDS_EVT_IN_REP_NOTIFY_ENABLED : hids.h
- HIDS_EVT_INVALID : hids.h
- HIDS_EVT_REP_CHAR_WRITE : hids.h
- HIDS_EVT_REPORT_MODE_ENTERED : hids.h
- HIDS_REPORT_TYPE_FEATURE : hids.h
- HIDS_REPORT_TYPE_IN1 : hids.h
- HIDS_REPORT_TYPE_IN2 : hids.h
- HIDS_REPORT_TYPE_IN3 : hids.h
- HIDS_REPORT_TYPE_KB_IN : hids.h
- HIDS_REPORT_TYPE_KB_OUT : hids.h
- HIDS_REPORT_TYPE_MOUSE_IN : hids.h
- HIDS_REPORT_TYPE_OUT : hids.h
- HIDS_REPORT_TYPE_RESERVED : hids.h
- HOST_TO_CONTROLLER : ble_iso.h
- HRRCPS_CTRL_PT_HRS_CONN_STA_REPORT : hrrcps.h
- HRRCPS_CTRL_PT_HRS_DISCONN : hrrcps.h
- HRRCPS_CTRL_PT_HRS_NTF_DISABLE : hrrcps.h
- HRRCPS_CTRL_PT_HRS_NTF_ENABLE : hrrcps.h
- HRRCPS_CTRL_PT_HRS_SEN_LOC_READ : hrrcps.h
- HRRCPS_CTRL_PT_RSCS_CONN_STA_REPORT : hrrcps.h
- HRRCPS_CTRL_PT_RSCS_DISCONN : hrrcps.h
- HRRCPS_CTRL_PT_RSCS_NTF_DISABLE : hrrcps.h
- HRRCPS_CTRL_PT_RSCS_NTF_ENABLE : hrrcps.h
- HRRCPS_CTRL_PT_RSCS_SEN_LOC_READ : hrrcps.h
- HRRCPS_CTRL_PT_RSP_CODE : hrrcps.h
- HRRCPS_CTRL_PT_SCAN_HRS : hrrcps.h
- HRRCPS_CTRL_PT_SCAN_RSCS : hrrcps.h
- HRRCPS_EVT_CTRL_PT_IND_DISABLE : hrrcps.h
- HRRCPS_EVT_CTRL_PT_IND_ENABLE : hrrcps.h
- HRRCPS_EVT_DISABLE_HRS_NTF : hrrcps.h
- HRRCPS_EVT_DISABLE_RSCS_NTF : hrrcps.h
- HRRCPS_EVT_DISCONN_HRS_LINK : hrrcps.h
- HRRCPS_EVT_DISCONN_RSCS_LINK : hrrcps.h
- HRRCPS_EVT_ENABLE_HRS_NTF : hrrcps.h
- HRRCPS_EVT_ENABLE_RSCS_NTF : hrrcps.h
- HRRCPS_EVT_HRS_SENSOR_LOC_READ : hrrcps.h
- HRRCPS_EVT_INVALID : hrrcps.h
- HRRCPS_EVT_RSCS_SENSOR_LOC_READ : hrrcps.h
- HRRCPS_EVT_SCAN_HRS : hrrcps.h
- HRRCPS_EVT_SCAN_RSCS : hrrcps.h
- HRRCPS_RSP_ID_ERROR : hrrcps.h
- HRRCPS_RSP_ID_OK : hrrcps.h
- HRS_C_BIT_ENERGY_EXPENDED_STATUS : hrs_c.h
- HRS_C_BIT_INTERVAL : hrs_c.h
- HRS_C_BIT_RATE_FORMAT : hrs_c.h
- HRS_C_BIT_SENSOR_CONTACT_DETECTED : hrs_c.h
- HRS_C_BIT_SENSOR_CONTACT_SUPPORTED : hrs_c.h
- HRS_C_EVT_CTRL_POINT_SET : hrs_c.h
- HRS_C_EVT_DISCOVERY_COMPLETE : hrs_c.h
- HRS_C_EVT_DISCOVERY_FAIL : hrs_c.h
- HRS_C_EVT_HR_MEAS_NTF_SET_SUCCESS : hrs_c.h
- HRS_C_EVT_HR_MEAS_VAL_RECEIVE : hrs_c.h
- HRS_C_EVT_INVALID : hrs_c.h
- HRS_C_EVT_SENSOR_LOC_READ_RSP : hrs_c.h
- HRS_C_EVT_WRITE_OP_ERR : hrs_c.h
- HRS_C_SENS_LOC_CHEST : hrs_c.h
- HRS_C_SENS_LOC_EARLOBE : hrs_c.h
- HRS_C_SENS_LOC_FINGER : hrs_c.h
- HRS_C_SENS_LOC_FOOT : hrs_c.h
- HRS_C_SENS_LOC_HAND : hrs_c.h
- HRS_C_SENS_LOC_OTHER : hrs_c.h
- HRS_C_SENS_LOC_WRIST : hrs_c.h
- HRS_EVT_NOTIFICATION_DISABLED : hrs.h
- HRS_EVT_NOTIFICATION_ENABLED : hrs.h
- HRS_EVT_READ_BODY_SEN_LOCATION : hrs.h
- HRS_EVT_RESET_ENERGY_EXPENDED : hrs.h
- HRS_SENS_LOC_CHEST : hrs.h
- HRS_SENS_LOC_EARLOBE : hrs.h
- HRS_SENS_LOC_FINGER : hrs.h
- HRS_SENS_LOC_FOOT : hrs.h
- HRS_SENS_LOC_HAND : hrs.h
- HRS_SENS_LOC_OTHER : hrs.h
- HRS_SENS_LOC_WRIST : hrs.h
- HTS_EVT_INTM_TEM_NOTIFICATION_DISABLE : hts.h
- HTS_EVT_INTM_TEM_NOTIFICATION_ENABLE : hts.h
- HTS_EVT_INVALID : hts.h
- HTS_EVT_MEAS_INTERVAL_INDICATION_DISABLE : hts.h
- HTS_EVT_MEAS_INTERVAL_UPDATE : hts.h
- HTS_EVT_MEAS_INTREVAL_INDICATION_ENABLE : hts.h
- HTS_EVT_READ_CHARACTERISTIC : hts.h
- HTS_EVT_TEM_MEAS_INDICATION_DISABLE : hts.h
- HTS_EVT_TEM_MEAS_INDICATION_ENABLE : hts.h
- HTS_MEAS_FLAG_TEM_TYPE_BIT : hts.h
- HTS_MEAS_FLAG_TEM_UINTS_BIT : hts.h
- HTS_MEAS_FLAG_TIME_STAMP_BIT : hts.h
- HTS_READ_CHAR_MEAS_INTL : hts.h
- HTS_READ_CHAR_TEMP_TYPE : hts.h
- HTS_TEMP_TYPE_ARMPIT : hts.h
- HTS_TEMP_TYPE_BODY : hts.h
- HTS_TEMP_TYPE_EAR : hts.h
- HTS_TEMP_TYPE_EAR_DRUM : hts.h
- HTS_TEMP_TYPE_FINGER : hts.h
- HTS_TEMP_TYPE_GI_TRACT : hts.h
- HTS_TEMP_TYPE_MOUTH : hts.h
- HTS_TEMP_TYPE_RECTUM : hts.h
- HTS_TEMP_TYPE_TOE : hts.h
- HTS_TEMPERATURE_CELCIUS : hts.h
- HTS_TEMPERATURE_FAHRENHEIT : hts.h
- HTS_TEMPERATURE_INTERMEDIATE : hts.h
- HTS_TEMPERATURE_STABLE : hts.h