Macros
USB Flags Definition
Peripheral Driver » HAL Driver » USB » Defines » USB Exported Constants
Collaboration diagram for USB Flags Definition:

## Macros
#define | USB_FLAG_SUSPEND LL_USB_INT_STAT_SUSPEND
| USB suspend status flag More...
#define | USB_FLAG_EP0_OUT_READY LL_USB_INT_STAT_EP0_OUT_READY
| USB ep0 data out ready flag More...
#define | USB_FLAG_EP1_OUT_READY LL_USB_INT_STAT_EP1_OUT_READY
| USB ep1 data out ready flag More...
#define | USB_FLAG_CRC16_ERR LL_USB_INT_STAT_CRC16_ERR
| USB receive CRC error data flag More...
#define | USB_FLAG_UPID_ERR LL_USB_INT_STAT_UPID_ERR
| USB receive unsupported PID flag More...
#define | USB_FLAG_TIMEOUT_ERR LL_USB_INT_STAT_TIMEOUT_ERR
| USB rx/tx timeout error flag More...
#define | USB_FLAG_SEQ_ERR LL_USB_INT_STAT_SEQ_ERR
| USB DATA0/DATA1 PID sequence error flag More...
#define | USB_FLAG_PID_CKS_ERR LL_USB_INT_STAT_PID_CKS_ERR
| USB PID checksum error flag More...
#define | USB_FLAG_PID_CRC_ERR LL_USB_INT_STAT_PID_CRC_ERR
| USB PID CRC error flag More...
#define | USB_FLAG_HOST_RESET LL_USB_INT_STAT_HOST_RESET
| USB host reset flag More...
#define | USB_FLAG_AHB_XFER_ERR LL_USB_INT_STAT_AHB_XFER_ERR
| USB ep3 and ep4 AHB master receive error flag More...
#define | USB_FLAG_NSE_ERR LL_USB_INT_STAT_NSE_ERR
| USB no such endpoint error flag More...
#define | USB_FLAG_EP3_AHB_XFER_DONE LL_USB_INT_STAT_EP3_AHB_XFER_DONE
| USB ep3 AHB master transfer done flag More...
#define | USB_FLAG_SYNC_ERR LL_USB_INT_STAT_SYNC_ERR
| USB SYNC error flag More...
#define | USB_FLAG_BIT_STUFF_ERR LL_USB_INT_STAT_BIT_STUFF_ERR
| USB bit stuff error flag More...
#define | USB_FLAG_BYTE_ERR LL_USB_INT_STAT_BYTE_ERR
| USB byte error flag More...
#define | USB_FLAG_SOF LL_USB_INT_STAT_SOF
| USB SOF flag More...
#define | USB_FLAG_EP0_TX_DONE LL_USB_INT_STAT_EP0_TX_DONE
| USB ep0 TX done flag More...
#define | USB_FLAG_EP2_TX_DONE LL_USB_INT_STAT_EP2_TX_DONE
| USB ep2 TX done flag More...
#define | USB_FLAG_EP3_TX_DONE LL_USB_INT_STAT_EP3_TX_DONE
| USB ep3 TX done flag More...
#define | USB_FLAG_INTO_CONFIG LL_USB_INT_STAT_INTO_CONFIG
| USB into cofig status flag More...
#define | USB_FLAG_EP5_OUT_READY LL_USB_INT_STAT_EP5_OUT_READY
| USB ep5 data out ready flag More...
#define | USB_FLAG_EP4_AHB_XFER_DONE LL_USB_INT_STAT_EP4_AHB_XFER_DONE
| USB ep4 AHB master transfer done flag More...
#define | USB_FLAG_EP4_TX_DONE LL_USB_INT_STAT_EP4_TX_DONE
| USB ep4 TX done flag More...
#define | USB_FLAG_EP5_AHB_XFER_DONE LL_USB_INT_STAT_EP5_AHB_XFER_DONE
| USB ep5 AHB master transfer done flag More...
#define | USB_FLAG_EP5_TIMER_OUT_ERR LL_USB_INT_STAT_EP5_TIMER_OUT_ERR
| USB ep5 timer out error flag More...

## Detailed Description

## Macro Definition Documentation

## ◆ USB_FLAG_AHB_XFER_ERR

#define USB_FLAG_AHB_XFER_ERR LL_USB_INT_STAT_AHB_XFER_ERR

USB ep3 and ep4 AHB master receive error flag

Definition at line 343 of file gr55xx_hal_usb.h.

## ◆ USB_FLAG_BIT_STUFF_ERR

#define USB_FLAG_BIT_STUFF_ERR LL_USB_INT_STAT_BIT_STUFF_ERR

USB bit stuff error flag

Definition at line 347 of file gr55xx_hal_usb.h.

## ◆ USB_FLAG_BYTE_ERR

#define USB_FLAG_BYTE_ERR LL_USB_INT_STAT_BYTE_ERR

USB byte error flag

Definition at line 348 of file gr55xx_hal_usb.h.

## ◆ USB_FLAG_CRC16_ERR

#define USB_FLAG_CRC16_ERR LL_USB_INT_STAT_CRC16_ERR

USB receive CRC error data flag

Definition at line 336 of file gr55xx_hal_usb.h.

## ◆ USB_FLAG_EP0_OUT_READY

#define USB_FLAG_EP0_OUT_READY LL_USB_INT_STAT_EP0_OUT_READY

USB ep0 data out ready flag

Definition at line 334 of file gr55xx_hal_usb.h.

## ◆ USB_FLAG_EP0_TX_DONE

#define USB_FLAG_EP0_TX_DONE LL_USB_INT_STAT_EP0_TX_DONE

USB ep0 TX done flag

Definition at line 350 of file gr55xx_hal_usb.h.

## ◆ USB_FLAG_EP1_OUT_READY

#define USB_FLAG_EP1_OUT_READY LL_USB_INT_STAT_EP1_OUT_READY

USB ep1 data out ready flag

Definition at line 335 of file gr55xx_hal_usb.h.

## ◆ USB_FLAG_EP2_TX_DONE

#define USB_FLAG_EP2_TX_DONE LL_USB_INT_STAT_EP2_TX_DONE

USB ep2 TX done flag

Definition at line 351 of file gr55xx_hal_usb.h.

## ◆ USB_FLAG_EP3_AHB_XFER_DONE

#define USB_FLAG_EP3_AHB_XFER_DONE LL_USB_INT_STAT_EP3_AHB_XFER_DONE

USB ep3 AHB master transfer done flag

Definition at line 345 of file gr55xx_hal_usb.h.

## ◆ USB_FLAG_EP3_TX_DONE

#define USB_FLAG_EP3_TX_DONE LL_USB_INT_STAT_EP3_TX_DONE

USB ep3 TX done flag

Definition at line 352 of file gr55xx_hal_usb.h.

## ◆ USB_FLAG_EP4_AHB_XFER_DONE

#define USB_FLAG_EP4_AHB_XFER_DONE LL_USB_INT_STAT_EP4_AHB_XFER_DONE

USB ep4 AHB master transfer done flag

Definition at line 355 of file gr55xx_hal_usb.h.

## ◆ USB_FLAG_EP4_TX_DONE

#define USB_FLAG_EP4_TX_DONE LL_USB_INT_STAT_EP4_TX_DONE

USB ep4 TX done flag

Definition at line 356 of file gr55xx_hal_usb.h.

## ◆ USB_FLAG_EP5_AHB_XFER_DONE

#define USB_FLAG_EP5_AHB_XFER_DONE LL_USB_INT_STAT_EP5_AHB_XFER_DONE

USB ep5 AHB master transfer done flag

Definition at line 357 of file gr55xx_hal_usb.h.

## ◆ USB_FLAG_EP5_OUT_READY

#define USB_FLAG_EP5_OUT_READY LL_USB_INT_STAT_EP5_OUT_READY

USB ep5 data out ready flag

Definition at line 354 of file gr55xx_hal_usb.h.

## ◆ USB_FLAG_EP5_TIMER_OUT_ERR

#define USB_FLAG_EP5_TIMER_OUT_ERR LL_USB_INT_STAT_EP5_TIMER_OUT_ERR

USB ep5 timer out error flag

Definition at line 358 of file gr55xx_hal_usb.h.

## ◆ USB_FLAG_HOST_RESET

#define USB_FLAG_HOST_RESET LL_USB_INT_STAT_HOST_RESET

USB host reset flag

Definition at line 342 of file gr55xx_hal_usb.h.

## ◆ USB_FLAG_INTO_CONFIG

#define USB_FLAG_INTO_CONFIG LL_USB_INT_STAT_INTO_CONFIG

USB into cofig status flag

Definition at line 353 of file gr55xx_hal_usb.h.

## ◆ USB_FLAG_NSE_ERR

#define USB_FLAG_NSE_ERR LL_USB_INT_STAT_NSE_ERR

USB no such endpoint error flag

Definition at line 344 of file gr55xx_hal_usb.h.

## ◆ USB_FLAG_PID_CKS_ERR

#define USB_FLAG_PID_CKS_ERR LL_USB_INT_STAT_PID_CKS_ERR

USB PID checksum error flag

Definition at line 340 of file gr55xx_hal_usb.h.

## ◆ USB_FLAG_PID_CRC_ERR

#define USB_FLAG_PID_CRC_ERR LL_USB_INT_STAT_PID_CRC_ERR

USB PID CRC error flag

Definition at line 341 of file gr55xx_hal_usb.h.

## ◆ USB_FLAG_SEQ_ERR

#define USB_FLAG_SEQ_ERR LL_USB_INT_STAT_SEQ_ERR

USB DATA0/DATA1 PID sequence error flag

Definition at line 339 of file gr55xx_hal_usb.h.

## ◆ USB_FLAG_SOF

#define USB_FLAG_SOF LL_USB_INT_STAT_SOF

USB SOF flag

Definition at line 349 of file gr55xx_hal_usb.h.

## ◆ USB_FLAG_SUSPEND

#define USB_FLAG_SUSPEND LL_USB_INT_STAT_SUSPEND

USB suspend status flag

Definition at line 333 of file gr55xx_hal_usb.h.

## ◆ USB_FLAG_SYNC_ERR

#define USB_FLAG_SYNC_ERR LL_USB_INT_STAT_SYNC_ERR

USB SYNC error flag

Definition at line 346 of file gr55xx_hal_usb.h.

## ◆ USB_FLAG_TIMEOUT_ERR

#define USB_FLAG_TIMEOUT_ERR LL_USB_INT_STAT_TIMEOUT_ERR

USB rx/tx timeout error flag

Definition at line 338 of file gr55xx_hal_usb.h.

## ◆ USB_FLAG_UPID_ERR

#define USB_FLAG_UPID_ERR LL_USB_INT_STAT_UPID_ERR

USB receive unsupported PID flag

Definition at line 337 of file gr55xx_hal_usb.h.