Macros
address size for concurrent xip mode
Peripheral Driver » HAL Driver » QSPI » Defines » QSPI Exported Constants
Collaboration diagram for address size for concurrent xip mode:

## Macros
#define | QSPI_CONCURRENT_XIP_ADDRSIZE_0BIT LL_QSPI_CONCURRENT_XIP_ADDRSIZE_0BIT
| Address length for QSPI XIP transfer: 0 bits. More...
#define | QSPI_CONCURRENT_XIP_ADDRSIZE_4BIT LL_QSPI_CONCURRENT_XIP_ADDRSIZE_4BIT
| Address length for QSPI XIP transfer: 4 bits. More...
#define | QSPI_CONCURRENT_XIP_ADDRSIZE_8BIT LL_QSPI_CONCURRENT_XIP_ADDRSIZE_8BIT
| Address length for QSPI XIP transfer: 8 bits. More...
#define | QSPI_CONCURRENT_XIP_ADDRSIZE_12BIT LL_QSPI_CONCURRENT_XIP_ADDRSIZE_12BIT
| Address length for QSPI XIP transfer: 12 bits. More...
#define | QSPI_CONCURRENT_XIP_ADDRSIZE_16BIT LL_QSPI_CONCURRENT_XIP_ADDRSIZE_16BIT
| Address length for QSPI XIP transfer: 16 bits. More...
#define | QSPI_CONCURRENT_XIP_ADDRSIZE_20BIT LL_QSPI_CONCURRENT_XIP_ADDRSIZE_20BIT
| Address length for QSPI XIP transfer: 20 bits. More...
#define | QSPI_CONCURRENT_XIP_ADDRSIZE_24BIT LL_QSPI_CONCURRENT_XIP_ADDRSIZE_24BIT
| Address length for QSPI XIP transfer: 24 bits. More...
#define | QSPI_CONCURRENT_XIP_ADDRSIZE_28BIT LL_QSPI_CONCURRENT_XIP_ADDRSIZE_28BIT
| Address length for QSPI XIP transfer: 28 bits. More...
#define | QSPI_CONCURRENT_XIP_ADDRSIZE_32BIT LL_QSPI_CONCURRENT_XIP_ADDRSIZE_32BIT
| Address length for QSPI XIP transfer: 32 bits. More...
#define | QSPI_CONCURRENT_XIP_ADDRSIZE_36BIT LL_QSPI_CONCURRENT_XIP_ADDRSIZE_36BIT
| Address length for QSPI XIP transfer: 36 bits. More...
#define | QSPI_CONCURRENT_XIP_ADDRSIZE_40BIT LL_QSPI_CONCURRENT_XIP_ADDRSIZE_40BIT
| Address length for QSPI XIP transfer: 40 bits. More...
#define | QSPI_CONCURRENT_XIP_ADDRSIZE_44BIT LL_QSPI_CONCURRENT_XIP_ADDRSIZE_44BIT
| Address length for QSPI XIP transfer: 44 bits. More...
#define | QSPI_CONCURRENT_XIP_ADDRSIZE_48BIT LL_QSPI_CONCURRENT_XIP_ADDRSIZE_48BIT
| Address length for QSPI XIP transfer: 48 bits. More...
#define | QSPI_CONCURRENT_XIP_ADDRSIZE_52BIT LL_QSPI_CONCURRENT_XIP_ADDRSIZE_52BIT
| Address length for QSPI XIP transfer: 52 bits. More...
#define | QSPI_CONCURRENT_XIP_ADDRSIZE_56BIT LL_QSPI_CONCURRENT_XIP_ADDRSIZE_56BIT
| Address length for QSPI XIP transfer: 56 bits. More...
#define | QSPI_CONCURRENT_XIP_ADDRSIZE_60BIT LL_QSPI_CONCURRENT_XIP_ADDRSIZE_60BIT
| Address length for QSPI XIP transfer: 60 bits. More...

## Detailed Description

## Macro Definition Documentation

## ◆ QSPI_CONCURRENT_XIP_ADDRSIZE_0BIT

#define QSPI_CONCURRENT_XIP_ADDRSIZE_0BIT LL_QSPI_CONCURRENT_XIP_ADDRSIZE_0BIT

Address length for QSPI XIP transfer: 0 bits.

Definition at line 609 of file gr55xx_hal_qspi.h.

## ◆ QSPI_CONCURRENT_XIP_ADDRSIZE_12BIT

#define QSPI_CONCURRENT_XIP_ADDRSIZE_12BIT LL_QSPI_CONCURRENT_XIP_ADDRSIZE_12BIT

Address length for QSPI XIP transfer: 12 bits.

Definition at line 612 of file gr55xx_hal_qspi.h.

## ◆ QSPI_CONCURRENT_XIP_ADDRSIZE_16BIT

#define QSPI_CONCURRENT_XIP_ADDRSIZE_16BIT LL_QSPI_CONCURRENT_XIP_ADDRSIZE_16BIT

Address length for QSPI XIP transfer: 16 bits.

Definition at line 613 of file gr55xx_hal_qspi.h.

## ◆ QSPI_CONCURRENT_XIP_ADDRSIZE_20BIT

#define QSPI_CONCURRENT_XIP_ADDRSIZE_20BIT LL_QSPI_CONCURRENT_XIP_ADDRSIZE_20BIT

Address length for QSPI XIP transfer: 20 bits.

Definition at line 614 of file gr55xx_hal_qspi.h.

## ◆ QSPI_CONCURRENT_XIP_ADDRSIZE_24BIT

#define QSPI_CONCURRENT_XIP_ADDRSIZE_24BIT LL_QSPI_CONCURRENT_XIP_ADDRSIZE_24BIT

Address length for QSPI XIP transfer: 24 bits.

Definition at line 615 of file gr55xx_hal_qspi.h.

## ◆ QSPI_CONCURRENT_XIP_ADDRSIZE_28BIT

#define QSPI_CONCURRENT_XIP_ADDRSIZE_28BIT LL_QSPI_CONCURRENT_XIP_ADDRSIZE_28BIT

Address length for QSPI XIP transfer: 28 bits.

Definition at line 616 of file gr55xx_hal_qspi.h.

## ◆ QSPI_CONCURRENT_XIP_ADDRSIZE_32BIT

#define QSPI_CONCURRENT_XIP_ADDRSIZE_32BIT LL_QSPI_CONCURRENT_XIP_ADDRSIZE_32BIT

Address length for QSPI XIP transfer: 32 bits.

Definition at line 617 of file gr55xx_hal_qspi.h.

## ◆ QSPI_CONCURRENT_XIP_ADDRSIZE_36BIT

#define QSPI_CONCURRENT_XIP_ADDRSIZE_36BIT LL_QSPI_CONCURRENT_XIP_ADDRSIZE_36BIT

Address length for QSPI XIP transfer: 36 bits.

Definition at line 618 of file gr55xx_hal_qspi.h.

## ◆ QSPI_CONCURRENT_XIP_ADDRSIZE_40BIT

#define QSPI_CONCURRENT_XIP_ADDRSIZE_40BIT LL_QSPI_CONCURRENT_XIP_ADDRSIZE_40BIT

Address length for QSPI XIP transfer: 40 bits.

Definition at line 619 of file gr55xx_hal_qspi.h.

## ◆ QSPI_CONCURRENT_XIP_ADDRSIZE_44BIT

#define QSPI_CONCURRENT_XIP_ADDRSIZE_44BIT LL_QSPI_CONCURRENT_XIP_ADDRSIZE_44BIT

Address length for QSPI XIP transfer: 44 bits.

Definition at line 620 of file gr55xx_hal_qspi.h.

## ◆ QSPI_CONCURRENT_XIP_ADDRSIZE_48BIT

#define QSPI_CONCURRENT_XIP_ADDRSIZE_48BIT LL_QSPI_CONCURRENT_XIP_ADDRSIZE_48BIT

Address length for QSPI XIP transfer: 48 bits.

Definition at line 621 of file gr55xx_hal_qspi.h.

## ◆ QSPI_CONCURRENT_XIP_ADDRSIZE_4BIT

#define QSPI_CONCURRENT_XIP_ADDRSIZE_4BIT LL_QSPI_CONCURRENT_XIP_ADDRSIZE_4BIT

Address length for QSPI XIP transfer: 4 bits.

Definition at line 610 of file gr55xx_hal_qspi.h.

## ◆ QSPI_CONCURRENT_XIP_ADDRSIZE_52BIT

#define QSPI_CONCURRENT_XIP_ADDRSIZE_52BIT LL_QSPI_CONCURRENT_XIP_ADDRSIZE_52BIT

Address length for QSPI XIP transfer: 52 bits.

Definition at line 622 of file gr55xx_hal_qspi.h.

## ◆ QSPI_CONCURRENT_XIP_ADDRSIZE_56BIT

#define QSPI_CONCURRENT_XIP_ADDRSIZE_56BIT LL_QSPI_CONCURRENT_XIP_ADDRSIZE_56BIT

Address length for QSPI XIP transfer: 56 bits.

Definition at line 623 of file gr55xx_hal_qspi.h.

## ◆ QSPI_CONCURRENT_XIP_ADDRSIZE_60BIT

#define QSPI_CONCURRENT_XIP_ADDRSIZE_60BIT LL_QSPI_CONCURRENT_XIP_ADDRSIZE_60BIT

Address length for QSPI XIP transfer: 60 bits.

Definition at line 624 of file gr55xx_hal_qspi.h.

## ◆ QSPI_CONCURRENT_XIP_ADDRSIZE_8BIT

#define QSPI_CONCURRENT_XIP_ADDRSIZE_8BIT LL_QSPI_CONCURRENT_XIP_ADDRSIZE_8BIT

Address length for QSPI XIP transfer: 8 bits.

Definition at line 611 of file gr55xx_hal_qspi.h.