Macros
USB Endpoint attribute setting
Peripheral Driver » HAL Driver » USB » Defines » USB Exported Constants
Collaboration diagram for USB Endpoint attribute setting:

## Macros
#define | USB_EP_ATTR_INT ((uint32_t)0x00000000UL)
| Endpoint attribute setting: interrupt More...
#define | USB_EP_ATTR_ISO ((uint32_t)0x00000001UL)
| Endpoint attribute setting: Isochronous More...
#define | USB_EP_ATTR_BULK ((uint32_t)0x00000002UL)
| Endpoint attribute setting: bulk More...

## Detailed Description

## Macro Definition Documentation

## ◆ USB_EP_ATTR_BULK

#define USB_EP_ATTR_BULK ((uint32_t)0x00000002UL)

Endpoint attribute setting: bulk

Definition at line 311 of file gr55xx_hal_usb.h.

## ◆ USB_EP_ATTR_INT

#define USB_EP_ATTR_INT ((uint32_t)0x00000000UL)

Endpoint attribute setting: interrupt

Definition at line 309 of file gr55xx_hal_usb.h.

## ◆ USB_EP_ATTR_ISO

#define USB_EP_ATTR_ISO ((uint32_t)0x00000001UL)

Endpoint attribute setting: Isochronous

Definition at line 310 of file gr55xx_hal_usb.h.