Macros
Instruction sent mode for concurrent xip mode
Peripheral Driver » HAL Driver » QSPI » Defines » QSPI Exported Constants
Collaboration diagram for Instruction sent mode for concurrent xip mode:

## Macros
#define | QSPI_CONCURRENT_XIP_INST_SENT_EVERY_ACCESS LL_QSPI_CONCURRENT_XIP_INST_SENT_EVERY_ACCESS
#define | QSPI_CONCURRENT_XIP_INST_SENT_ONLY_FIRST_ACCESS LL_QSPI_CONCURRENT_XIP_INST_SENT_ONLY_FIRST_ACCESS

## Detailed Description

## Macro Definition Documentation

## ◆ QSPI_CONCURRENT_XIP_INST_SENT_EVERY_ACCESS

#define QSPI_CONCURRENT_XIP_INST_SENT_EVERY_ACCESS LL_QSPI_CONCURRENT_XIP_INST_SENT_EVERY_ACCESS

Send instruction for every transaction

Definition at line 689 of file gr55xx_hal_qspi.h.

## ◆ QSPI_CONCURRENT_XIP_INST_SENT_ONLY_FIRST_ACCESS

#define QSPI_CONCURRENT_XIP_INST_SENT_ONLY_FIRST_ACCESS LL_QSPI_CONCURRENT_XIP_INST_SENT_ONLY_FIRST_ACCESS

Send instruction only for first transaction

Definition at line 690 of file gr55xx_hal_qspi.h.