Functions
IRQ Handler and Callbacks
Peripheral Driver » HAL Driver » DUAL TIMER » Functions

IRQ Handler and Callbacks functions. More...

Collaboration diagram for IRQ Handler and Callbacks:

## Functions
void | hal_dual_timer_irq_handler (dual_timer_handle_t *p_dual_timer)
| Handle DUAL TIMER interrupt request. More...
void | hal_dual_timer_period_elapsed_callback (dual_timer_handle_t *p_dual_timer)
| Period elapsed callback in non-blocking mode. More...

## Detailed Description

IRQ Handler and Callbacks functions.

## Function Documentation

## ◆ hal_dual_timer_irq_handler()

void hal_dual_timer_irq_handler | ( | dual_timer_handle_t * | p_dual_timer | ) |

Handle DUAL TIMER interrupt request.

Parameters

  [in] | p_dual_timer | Pointer to a DUAL_TIMER handle which contains the configuration information for the specified DUAL TIMER.

## ◆ hal_dual_timer_period_elapsed_callback()

void hal_dual_timer_period_elapsed_callback | ( | dual_timer_handle_t * | p_dual_timer | ) |

Period elapsed callback in non-blocking mode.

Note
  This function should not be modified. When the callback is needed, the hal_dual_timer_period_elapsed_callback can be implemented in the user file.

Parameters

  [in] | p_dual_timer | Pointer to a DUAL_TIMER handle which contains the configuration information for the specified DUAL TIMER.