Modules | Macros
Defines
BLE Services » Bond Management Service (BMS)
Collaboration diagram for Defines:

## Modules
| BMS Feature
| BMS feature.

## Macros
#define | BMS_CONNECTION_MAX 10
| Maximum number of BMS connections.The value is configurable. More...
#define | BMS_ERROR_OP_CODE_NOT_SUPPORTED 0x80
| Error code: Response if unsupported Op Code is received. More...
#define | BMS_ERROR_OPERATION_FAILED 0x81
| Error code: Response if unable to complete a procedure for any reason. More...
#define | BMS_AUTH_CODE_LEN_MAX 12

## Detailed Description

## Macro Definition Documentation

## ◆ BMS_AUTH_CODE_LEN_MAX

#define BMS_AUTH_CODE_LEN_MAX 12

Definition at line 74 of file bms.h.

## ◆ BMS_CONNECTION_MAX

#define BMS_CONNECTION_MAX 10

Maximum number of BMS connections.The value is configurable.

Definition at line 69 of file bms.h.

## ◆ BMS_ERROR_OP_CODE_NOT_SUPPORTED

#define BMS_ERROR_OP_CODE_NOT_SUPPORTED 0x80

Error code: Response if unsupported Op Code is received.

Definition at line 71 of file bms.h.

## ◆ BMS_ERROR_OPERATION_FAILED

#define BMS_ERROR_OPERATION_FAILED 0x81

Error code: Response if unable to complete a procedure for any reason.

Definition at line 72 of file bms.h.