Functions
FLAG_Management
Peripheral Driver » LL Driver » TIMER » Functions
Collaboration diagram for FLAG_Management:

## Functions
__STATIC_INLINE void | ll_timer_clear_flag_it (timer_regs_t *TIMERx)
| Clear the interrupt flag (INTSTAT). More...
__STATIC_INLINE uint32_t | ll_timer_is_active_flag_it (timer_regs_t *TIMERx)
| Indicate whether interrupt flag (INTSTAT) is set (interrupt is pending). More...

## Detailed Description

## Function Documentation

## ◆ ll_timer_clear_flag_it()

__STATIC_INLINE void ll_timer_clear_flag_it | ( | timer_regs_t * | TIMERx | ) |

Clear the interrupt flag (INTSTAT).

Register | BitsName
--- | ---
INTSTAT | INTSTAT

Parameters

  TIMERx | Timer instance

Return values

  None |

Definition at line 329 of file gr55xx_ll_tim.h.

## ◆ ll_timer_is_active_flag_it()

__STATIC_INLINE uint32_t ll_timer_is_active_flag_it | ( | timer_regs_t * | TIMERx | ) |

Indicate whether interrupt flag (INTSTAT) is set (interrupt is pending).

Register | BitsName
--- | ---
INTSTAT | INTSTAT

Parameters

  TIMERx | Timer instance

Return values

  State | of bit (1 or 0).

Definition at line 344 of file gr55xx_ll_tim.h.