Functions
Functions
Peripheral Driver » APP DRIVER » GPIO
Collaboration diagram for Functions:

## Functions
uint16_t | app_io_init (app_io_type_t type, app_io_init_t *p_init)
| Initialize the APP GPIO DRIVER according to the specified parameters in the app_io_type_t and app_io_init_t. More...
uint16_t | app_io_deinit (app_io_type_t type, uint32_t pin)
| De-initialize the GPIOx peripheral. More...
app_io_pin_state_t | app_io_read_pin (app_io_type_t type, uint32_t pin)
| Read the specified input port pin. More...
uint16_t | app_io_write_pin (app_io_type_t type, uint32_t pin, app_io_pin_state_t pin_state)
| Set or clear the selected data port bit. More...
uint16_t | app_io_toggle_pin (app_io_type_t type, uint32_t pin)
| Toggle the specified GPIO pin. More...
uint16_t | app_io_set_speed (app_io_type_t type, uint32_t pin, app_io_speed_t speed)
| Set the speed of the GPIO. More...
uint16_t | app_io_set_strength (app_io_type_t type, uint32_t pin, app_io_strength_t strength)
| Set the strength of the GPIO. More...
uint16_t | app_io_set_intput_type (app_io_type_t type, uint32_t pin, app_io_input_type_t input_type)
| Set the input type of the GPIO. More...
uint16_t | app_io_event_register_cb (app_io_type_t type, app_io_init_t *p_init, app_io_callback_t io_evt_cb, void *arg)
| Initialize GPIO to interrupt mode and register interrupt callback function. More...
uint16_t | app_io_event_unregister (app_io_type_t type, uint32_t pin)
| Deinitialize GPIO to normal mode and unregister interrupt. More...

## Detailed Description

## Function Documentation

## ◆ app_io_deinit()

uint16_t app_io_deinit | ( | app_io_type_t | type,
|  | uint32_t | pin
| ) |  |

De-initialize the GPIOx peripheral.

Parameters

  [in] | type | GPIO type, See app_io_type_t.
  [in] | pin | The pin want to De-initialization.

Returns
  Result of De-initialization.

## ◆ app_io_event_register_cb()

uint16_t app_io_event_register_cb | ( | app_io_type_t | type,
|  | app_io_init_t * | p_init,
|  | app_io_callback_t | io_evt_cb,
|  | void * | arg
| ) |  |

Initialize GPIO to interrupt mode and register interrupt callback function.

Parameters

  [in] | type | GPIO type, See app_io_type_t.
  [in] | p_init | Pointer to app_io_init_t parameter which contains the configuration information for the specified GPIO.
  [in] | io_evt_cb | Interrupt callback function.
  [in] | arg | User parameters.

Returns
  Result of register.

## ◆ app_io_event_unregister()

uint16_t app_io_event_unregister | ( | app_io_type_t | type,
|  | uint32_t | pin
| ) |  |

Deinitialize GPIO to normal mode and unregister interrupt.

Parameters

  [in] | type | GPIO type, See app_io_type_t.
  [in] | pin | The pin want to unregister.

Returns
  Result of unregister.

## ◆ app_io_init()

uint16_t app_io_init | ( | app_io_type_t | type,
|  | app_io_init_t * | p_init
| ) |  |

Initialize the APP GPIO DRIVER according to the specified parameters in the app_io_type_t and app_io_init_t.

Parameters

  [in] | type | GPIO type.
  [in] | p_init | Pointer to app_io_init_t parameter which contains the configuration information for the specified GPIO.

Returns
  Result of initialization.

## ◆ app_io_read_pin()

app_io_pin_state_t app_io_read_pin | ( | app_io_type_t | type,
|  | uint32_t | pin
| ) |  |

Read the specified input port pin.

Parameters

  [in] | type | GPIO type, See app_io_type_t.
  [in] | pin | The pin want to read.

Returns
  The GPIO state.

## ◆ app_io_set_intput_type()

uint16_t app_io_set_intput_type | ( | app_io_type_t | type,
|  | uint32_t | pin,
|  | app_io_input_type_t | input_type
| ) |  |

Set the input type of the GPIO.

Parameters

  [in] | type | GPIO type, See app_io_type_t.
  [in] | pin | The pin want to toggle.
  [in] | input_type | GPIO input type, See app_io_input_type_t.

Returns
  Result of setting.

## ◆ app_io_set_speed()

uint16_t app_io_set_speed | ( | app_io_type_t | type,
|  | uint32_t | pin,
|  | app_io_speed_t | speed
| ) |  |

Set the speed of the GPIO.

Parameters

  [in] | type | GPIO type, See app_io_type_t.
  [in] | pin | The pin want to set.
  [in] | speed | GPIO speed type, See app_io_speed_t.

Returns
  Result of setting.

## ◆ app_io_set_strength()

uint16_t app_io_set_strength | ( | app_io_type_t | type,
|  | uint32_t | pin,
|  | app_io_strength_t | strength
| ) |  |

Set the strength of the GPIO.

Parameters

  [in] | type | GPIO type, See app_io_type_t.
  [in] | pin | The pin want to set.
  [in] | strength | GPIO strength type, See app_io_strength_t.

Returns
  Result of setting.

## ◆ app_io_toggle_pin()

uint16_t app_io_toggle_pin | ( | app_io_type_t | type,
|  | uint32_t | pin
| ) |  |

Toggle the specified GPIO pin.

Parameters

  [in] | type | GPIO type, See app_io_type_t.
  [in] | pin | The pin want to toggle.

Returns
  Result of toggle.

## ◆ app_io_write_pin()

uint16_t app_io_write_pin | ( | app_io_type_t | type,
|  | uint32_t | pin,
|  | app_io_pin_state_t | pin_state
| ) |  |

Set or clear the selected data port bit.

Parameters

  [in] | type | GPIO type, See app_io_type_t.
  [in] | pin | The pin want to set or clear.
  [in] | pin_state | Specifies the value to be written to the selected bit.

Returns
  Result of write.