Public Attributes | List of all members
iso_disc_ann_t Struct Reference
BLE » Core Isochronous Channels » Structures

The parameter for discovery announcement. More...

`#include <ble_iso.h>`

## Public Attributes
uint16_t | interval
| Scan interval between 0x0004 and 0x4000 in 0.625 ms units(range: 2.5 ms to 10.24 s). More...
uint16_t | window
| Scan window between 0x0004 and 0x4000 in 0.625 ms units(range: 2.5 ms to 10.24 s). More...
uint16_t | timeout
| Scan timeout should be a value between 0x0001 and 0xFFFF(unit: 10 ms). More...

## Detailed Description

The parameter for discovery announcement.

Definition at line 243 of file ble_iso.h.

## Member Data Documentation

## ◆ interval

uint16_t iso_disc_ann_t::interval

Scan interval between 0x0004 and 0x4000 in 0.625 ms units(range: 2.5 ms to 10.24 s).

Definition at line 245 of file ble_iso.h.

## ◆ timeout

uint16_t iso_disc_ann_t::timeout

Scan timeout should be a value between 0x0001 and 0xFFFF(unit: 10 ms).

0x0000 indicates that the timeout have no effect.

Definition at line 247 of file ble_iso.h.

## ◆ window

uint16_t iso_disc_ann_t::window

Scan window between 0x0004 and 0x4000 in 0.625 ms units(range: 2.5 ms to 10.24 s).

Definition at line 246 of file ble_iso.h.

The documentation for this struct was generated from the following file:

- ble_iso.h