Public Attributes | List of all members
_dspi_init_t Struct Reference
Peripheral Driver » HAL Driver » DSPI » Structures » DSPI Configuration

QSPI init Structure definition. More...

`#include <gr55xx_hal_dspi.h>`

## Public Attributes
uint32_t | data_size
| Specifies the DSPI data width. More...
uint32_t | baud_rate
| Specifies the BaudRate prescaler value which will be used to configure the transmit and receive SCK clock. More...
uint32_t | dspi_mode
| Specifies the DSPI interface mode. More...

## Detailed Description

QSPI init Structure definition.

Definition at line 95 of file gr55xx_hal_dspi.h.

## Member Data Documentation

## ◆ baud_rate

uint32_t _dspi_init_t::baud_rate

Specifies the BaudRate prescaler value which will be used to configure the transmit and receive SCK clock.

This parameter can be one even value between 0 and 7 Clock Select Clock Select.

Definition at line 100 of file gr55xx_hal_dspi.h.

## ◆ data_size

uint32_t _dspi_init_t::data_size

Specifies the DSPI data width.

This parameter can be a value of Data Width Data Width.

Definition at line 97 of file gr55xx_hal_dspi.h.

## ◆ dspi_mode

uint32_t _dspi_init_t::dspi_mode

Specifies the DSPI interface mode.

This parameter can be a value of DSPI Interface mode DSPI Interface Mode.

Definition at line 103 of file gr55xx_hal_dspi.h.

The documentation for this struct was generated from the following file:

- gr55xx_hal_dspi.h