Macros
Address Size For Xip
Peripheral Driver » LL Driver » QSPI » Defines » QSPI Exported Constants

Address size for concurrent xip mode. More...

Collaboration diagram for Address Size For Xip:

## Macros
#define | LL_QSPI_CONCURRENT_XIP_ADDRSIZE_0BIT 0x0
| Address length for QSPI XIP transfer: 0 bits. More...
#define | LL_QSPI_CONCURRENT_XIP_ADDRSIZE_4BIT 0x1
| Address length for QSPI XIP transfer: 4 bits. More...
#define | LL_QSPI_CONCURRENT_XIP_ADDRSIZE_8BIT 0x2
| Address length for QSPI XIP transfer: 8 bits. More...
#define | LL_QSPI_CONCURRENT_XIP_ADDRSIZE_12BIT 0x3
| Address length for QSPI XIP transfer: 12 bits. More...
#define | LL_QSPI_CONCURRENT_XIP_ADDRSIZE_16BIT 0x4
| Address length for QSPI XIP transfer: 16 bits. More...
#define | LL_QSPI_CONCURRENT_XIP_ADDRSIZE_20BIT 0x5
| Address length for QSPI XIP transfer: 20 bits. More...
#define | LL_QSPI_CONCURRENT_XIP_ADDRSIZE_24BIT 0x6
| Address length for QSPI XIP transfer: 24 bits. More...
#define | LL_QSPI_CONCURRENT_XIP_ADDRSIZE_28BIT 0x7
| Address length for QSPI XIP transfer: 28 bits. More...
#define | LL_QSPI_CONCURRENT_XIP_ADDRSIZE_32BIT 0x8
| Address length for QSPI XIP transfer: 32 bits. More...
#define | LL_QSPI_CONCURRENT_XIP_ADDRSIZE_36BIT 0x9
| Address length for QSPI XIP transfer: 36 bits. More...
#define | LL_QSPI_CONCURRENT_XIP_ADDRSIZE_40BIT 0xA
| Address length for QSPI XIP transfer: 40 bits. More...
#define | LL_QSPI_CONCURRENT_XIP_ADDRSIZE_44BIT 0xB
| Address length for QSPI XIP transfer: 44 bits. More...
#define | LL_QSPI_CONCURRENT_XIP_ADDRSIZE_48BIT 0xC
| Address length for QSPI XIP transfer: 48 bits. More...
#define | LL_QSPI_CONCURRENT_XIP_ADDRSIZE_52BIT 0xD
| Address length for QSPI XIP transfer: 52 bits. More...
#define | LL_QSPI_CONCURRENT_XIP_ADDRSIZE_56BIT 0xE
| Address length for QSPI XIP transfer: 56 bits. More...
#define | LL_QSPI_CONCURRENT_XIP_ADDRSIZE_60BIT 0xF
| Address length for QSPI XIP transfer: 60 bits. More...

## Detailed Description

Address size for concurrent xip mode.

## Macro Definition Documentation

## ◆ LL_QSPI_CONCURRENT_XIP_ADDRSIZE_0BIT

#define LL_QSPI_CONCURRENT_XIP_ADDRSIZE_0BIT 0x0

Address length for QSPI XIP transfer: 0 bits.

Definition at line 610 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_ADDRSIZE_12BIT

#define LL_QSPI_CONCURRENT_XIP_ADDRSIZE_12BIT 0x3

Address length for QSPI XIP transfer: 12 bits.

Definition at line 613 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_ADDRSIZE_16BIT

#define LL_QSPI_CONCURRENT_XIP_ADDRSIZE_16BIT 0x4

Address length for QSPI XIP transfer: 16 bits.

Definition at line 614 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_ADDRSIZE_20BIT

#define LL_QSPI_CONCURRENT_XIP_ADDRSIZE_20BIT 0x5

Address length for QSPI XIP transfer: 20 bits.

Definition at line 615 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_ADDRSIZE_24BIT

#define LL_QSPI_CONCURRENT_XIP_ADDRSIZE_24BIT 0x6

Address length for QSPI XIP transfer: 24 bits.

Definition at line 616 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_ADDRSIZE_28BIT

#define LL_QSPI_CONCURRENT_XIP_ADDRSIZE_28BIT 0x7

Address length for QSPI XIP transfer: 28 bits.

Definition at line 617 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_ADDRSIZE_32BIT

#define LL_QSPI_CONCURRENT_XIP_ADDRSIZE_32BIT 0x8

Address length for QSPI XIP transfer: 32 bits.

Definition at line 618 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_ADDRSIZE_36BIT

#define LL_QSPI_CONCURRENT_XIP_ADDRSIZE_36BIT 0x9

Address length for QSPI XIP transfer: 36 bits.

Definition at line 619 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_ADDRSIZE_40BIT

#define LL_QSPI_CONCURRENT_XIP_ADDRSIZE_40BIT 0xA

Address length for QSPI XIP transfer: 40 bits.

Definition at line 620 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_ADDRSIZE_44BIT

#define LL_QSPI_CONCURRENT_XIP_ADDRSIZE_44BIT 0xB

Address length for QSPI XIP transfer: 44 bits.

Definition at line 621 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_ADDRSIZE_48BIT

#define LL_QSPI_CONCURRENT_XIP_ADDRSIZE_48BIT 0xC

Address length for QSPI XIP transfer: 48 bits.

Definition at line 622 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_ADDRSIZE_4BIT

#define LL_QSPI_CONCURRENT_XIP_ADDRSIZE_4BIT 0x1

Address length for QSPI XIP transfer: 4 bits.

Definition at line 611 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_ADDRSIZE_52BIT

#define LL_QSPI_CONCURRENT_XIP_ADDRSIZE_52BIT 0xD

Address length for QSPI XIP transfer: 52 bits.

Definition at line 623 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_ADDRSIZE_56BIT

#define LL_QSPI_CONCURRENT_XIP_ADDRSIZE_56BIT 0xE

Address length for QSPI XIP transfer: 56 bits.

Definition at line 624 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_ADDRSIZE_60BIT

#define LL_QSPI_CONCURRENT_XIP_ADDRSIZE_60BIT 0xF

Address length for QSPI XIP transfer: 60 bits.

Definition at line 625 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_ADDRSIZE_8BIT

#define LL_QSPI_CONCURRENT_XIP_ADDRSIZE_8BIT 0x2

Address length for QSPI XIP transfer: 8 bits.

Definition at line 612 of file gr55xx_ll_qspi.h.