Macros
Low Power Feature
Peripheral Driver » LL Driver » CGC » Defines » CGC Exported Constants
Collaboration diagram for Low Power Feature:

## Macros
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_AHB2APB_EN MCU_SUB_PERIPH_CG_LP_AHB2APB_ASYNC_EN
| Enable AHB2APB ASYNC low-power feature More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_AHB2APB_SYNC_EN MCU_SUB_PERIPH_CG_LP_AHB2APB_SYNC_EN
| Enable AHB2APB SYNC low-power feature More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_QSPIM_EN MCU_SUB_PERIPH_CG_LP_EN_QSPIM_EN
| Enable qspim low-power feature More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_AHB_BUS_LP_EN MCU_SUB_PERIPH_CG_LP_EN_AHB_BUS_LP_EN
| Enable AHB bus low-power feature More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_LP_SCLK_EN MCU_SUB_PERIPH_CG_LP_EN_I2C_LP_SCLK_EN
| Enable i2c sclk low-power feature More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_SPIS_LP_SCLK_EN MCU_SUB_PERIPH_CG_LP_EN_SPIS_LP_SCLK_EN
| Enable spis sclk low-power feature More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_SPIM_LP_SCLK_EN MCU_SUB_PERIPH_CG_LP_EN_SPIM_LP_SCLK_EN
| Enable spim sclk low-power feature More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_I2S_LP_EN MCU_SUB_PERIPH_CG_LP_EN_I2S_LP_EN
| Enable i2s master low-power feature More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_UART_LP_PCLK_EN MCU_SUB_PERIPH_CG_LP_EN_UART_LP_PCLK_EN
| Enable uart pclk low-power feature More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_UART_LP_SCLK_EN MCU_SUB_PERIPH_CG_LP_EN_UART_LP_SCLK_EN
| Enable uart sclk low-power feature More...
#define | LL_CGC_MCU_PERIPH_CG_LP ((uint32_t)0x00000F3FUL)
| All Low Power Feature More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_CGC_MCU_PERIPH_CG_LP

#define LL_CGC_MCU_PERIPH_CG_LP ((uint32_t)0x00000F3FUL)

All Low Power Feature

Definition at line 182 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_AHB2APB_EN

#define LL_CGC_MCU_PERIPH_CG_LP_EN_AHB2APB_EN MCU_SUB_PERIPH_CG_LP_AHB2APB_ASYNC_EN

Enable AHB2APB ASYNC low-power feature

Definition at line 171 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_AHB2APB_SYNC_EN

#define LL_CGC_MCU_PERIPH_CG_LP_EN_AHB2APB_SYNC_EN MCU_SUB_PERIPH_CG_LP_AHB2APB_SYNC_EN

Enable AHB2APB SYNC low-power feature

Definition at line 172 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_AHB_BUS_LP_EN

#define LL_CGC_MCU_PERIPH_CG_LP_EN_AHB_BUS_LP_EN MCU_SUB_PERIPH_CG_LP_EN_AHB_BUS_LP_EN

Enable AHB bus low-power feature

Definition at line 174 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_LP_SCLK_EN

#define LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_LP_SCLK_EN MCU_SUB_PERIPH_CG_LP_EN_I2C_LP_SCLK_EN

Enable i2c sclk low-power feature

Definition at line 175 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_I2S_LP_EN

#define LL_CGC_MCU_PERIPH_CG_LP_EN_I2S_LP_EN MCU_SUB_PERIPH_CG_LP_EN_I2S_LP_EN

Enable i2s master low-power feature

Definition at line 178 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_QSPIM_EN

#define LL_CGC_MCU_PERIPH_CG_LP_EN_QSPIM_EN MCU_SUB_PERIPH_CG_LP_EN_QSPIM_EN

Enable qspim low-power feature

Definition at line 173 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_SPIM_LP_SCLK_EN

#define LL_CGC_MCU_PERIPH_CG_LP_EN_SPIM_LP_SCLK_EN MCU_SUB_PERIPH_CG_LP_EN_SPIM_LP_SCLK_EN

Enable spim sclk low-power feature

Definition at line 177 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_SPIS_LP_SCLK_EN

#define LL_CGC_MCU_PERIPH_CG_LP_EN_SPIS_LP_SCLK_EN MCU_SUB_PERIPH_CG_LP_EN_SPIS_LP_SCLK_EN

Enable spis sclk low-power feature

Definition at line 176 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_UART_LP_PCLK_EN

#define LL_CGC_MCU_PERIPH_CG_LP_EN_UART_LP_PCLK_EN MCU_SUB_PERIPH_CG_LP_EN_UART_LP_PCLK_EN

Enable uart pclk low-power feature

Definition at line 179 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_UART_LP_SCLK_EN

#define LL_CGC_MCU_PERIPH_CG_LP_EN_UART_LP_SCLK_EN MCU_SUB_PERIPH_CG_LP_EN_UART_LP_SCLK_EN

Enable uart sclk low-power feature

Definition at line 180 of file gr55xx_ll_cgc.h.