Public Attributes | List of all members
iso_per_adv_sync_tran_t Struct Reference
BLE » Core Isochronous Channels » Structures

The parameter for periodic advertising synchronization transport. More...

`#include <ble_iso.h>`

## Public Attributes
uint16_t | sync_hdl
| identifying the periodic advertising, (Range: 0x0000 to 0x0EFF). More...
uint16_t | service_data
| The Service_Data parameter is a value provided by the Host to identify the periodic advertisement to the peer device. More...
uint16_t | conn_hdl
| Connection_Handle, (Range: 0x0000 to 0x0EFF) More...

## Detailed Description

The parameter for periodic advertising synchronization transport.

Definition at line 405 of file ble_iso.h.

## Member Data Documentation

## ◆ conn_hdl

uint16_t iso_per_adv_sync_tran_t::conn_hdl

Connection_Handle, (Range: 0x0000 to 0x0EFF)

Definition at line 410 of file ble_iso.h.

## ◆ service_data

uint16_t iso_per_adv_sync_tran_t::service_data

The Service_Data parameter is a value provided by the Host to identify the periodic advertisement to the peer device.

It is not used by the Controller.

Definition at line 408 of file ble_iso.h.

## ◆ sync_hdl

uint16_t iso_per_adv_sync_tran_t::sync_hdl

identifying the periodic advertising, (Range: 0x0000 to 0x0EFF).

Definition at line 407 of file ble_iso.h.

The documentation for this struct was generated from the following file:

- ble_iso.h