Macros
MSIO Exported Macros
Peripheral Driver » HAL Driver » MSIO » Defines
Collaboration diagram for MSIO Exported Macros:

## Macros
#define | __HAL_MSIO_IT_GET_IT(__MSIOX__, __MSIO_PIN__) ll_msio_read_flag_it(__MSIOX__, __MSIO_PIN__)
| Check whether the specified MSIO pin is asserted or not. More...
#define | __HAL_MSIO_IT_CLEAR_IT(__MSIOX__, __MSIO_PIN__) ll_msio_clear_flag_it(__MSIOX__, __MSIO_PIN__)
| Clear the MSIO pin pending bits. More...

## Detailed Description

## Macro Definition Documentation

## ◆ __HAL_MSIO_IT_CLEAR_IT

#define __HAL_MSIO_IT_CLEAR_IT | ( |  | __MSIOX__,
|  |  | __MSIO_PIN__
| ) |  | ll_msio_clear_flag_it(__MSIOX__, __MSIO_PIN__)

Clear the MSIO pin pending bits.

Parameters

  <strong>MSIOX</strong> | MSIOX: Must select the MSIOA port
  <strong>MSIO_PIN</strong> | Specifies the MSIO pins to clear. This parameter can be any combination of MSIO_PIN_x where x can be (0..7)

Return values

  None |

Definition at line 216 of file gr55xx_hal_msio.h.

## ◆ __HAL_MSIO_IT_GET_IT

#define __HAL_MSIO_IT_GET_IT | ( |  | __MSIOX__,
|  |  | __MSIO_PIN__
| ) |  | ll_msio_read_flag_it(__MSIOX__, __MSIO_PIN__)

Check whether the specified MSIO pin is asserted or not.

Parameters

  <strong>MSIOX</strong> | MSIOX: Must select the MSIOA port
  <strong>MSIO_PIN</strong> | Specifies the MSIO pin to check. This parameter can be MSIO_PIN_x where x can be (0..7)

Return values

  The | new state of MSIO_PIN (SET or RESET).

Definition at line 207 of file gr55xx_hal_msio.h.