Macros
transfer of inst & address for concurrent xip mode
Peripheral Driver » HAL Driver » QSPI » Defines » QSPI Exported Constants
Collaboration diagram for transfer of inst & address for concurrent xip mode:

## Macros
#define | QSPI_CONCURRENT_XIP_INST_ADDR_ALL_IN_SPI LL_QSPI_CONCURRENT_XIP_INST_ADDR_ALL_IN_SPI
| Instruction and address are sent in SPI mode. More...
#define | QSPI_CONCURRENT_XIP_INST_IN_SPI_ADDR_IN_SPIFRF LL_QSPI_CONCURRENT_XIP_INST_IN_SPI_ADDR_IN_SPIFRF
| Instruction is in sent in SPI mode and address is sent in Daul/Quad SPI mode. More...
#define | QSPI_CONCURRENT_XIP_INST_ADDR_ALL_IN_SPIFRF LL_QSPI_CONCURRENT_XIP_INST_ADDR_ALL_IN_SPIFRF
| Instruction and address are sent in Daul/Quad SPI mode. More...

## Detailed Description

## Macro Definition Documentation

## ◆ QSPI_CONCURRENT_XIP_INST_ADDR_ALL_IN_SPI

#define QSPI_CONCURRENT_XIP_INST_ADDR_ALL_IN_SPI LL_QSPI_CONCURRENT_XIP_INST_ADDR_ALL_IN_SPI

Instruction and address are sent in SPI mode.

Definition at line 630 of file gr55xx_hal_qspi.h.

## ◆ QSPI_CONCURRENT_XIP_INST_ADDR_ALL_IN_SPIFRF

#define QSPI_CONCURRENT_XIP_INST_ADDR_ALL_IN_SPIFRF LL_QSPI_CONCURRENT_XIP_INST_ADDR_ALL_IN_SPIFRF

Instruction and address are sent in Daul/Quad SPI mode.

Definition at line 632 of file gr55xx_hal_qspi.h.

## ◆ QSPI_CONCURRENT_XIP_INST_IN_SPI_ADDR_IN_SPIFRF

#define QSPI_CONCURRENT_XIP_INST_IN_SPI_ADDR_IN_SPIFRF LL_QSPI_CONCURRENT_XIP_INST_IN_SPI_ADDR_IN_SPIFRF

Instruction is in sent in SPI mode and address is sent in Daul/Quad SPI mode.

Definition at line 631 of file gr55xx_hal_qspi.h.