Functions
Low Power mode configuration functions
Peripheral Driver » HAL Driver » PWR » Functions
Collaboration diagram for Low Power mode configuration functions:

## Functions
void | hal_pwr_enter_chip_deepsleep (void)
| Enters DeepSleep mode. More...

## Detailed Description

## Function Documentation

## ◆ hal_pwr_enter_chip_deepsleep()

void hal_pwr_enter_chip_deepsleep | ( | void |  | ) |

Enters DeepSleep mode.

Note
  In DeepSleep mode, all I/O pins keep the same state as in Run mode.