Macros
Instruction And Address For Xip
Peripheral Driver » LL Driver » QSPI » Defines » QSPI Exported Constants

Transfer of inst & address for concurrent xip mode. More...

Collaboration diagram for Instruction And Address For Xip:

## Macros
#define | LL_QSPI_CONCURRENT_XIP_INST_ADDR_ALL_IN_SPI 0x0
| Instruction and address are sent in SPI mode. More...
#define | LL_QSPI_CONCURRENT_XIP_INST_IN_SPI_ADDR_IN_SPIFRF 0x1
| Instruction is in sent in SPI mode and address is sent in Daul/Quad SPI mode. More...
#define | LL_QSPI_CONCURRENT_XIP_INST_ADDR_ALL_IN_SPIFRF 0x2
| Instruction and address are sent in Daul/Quad SPI mode. More...

## Detailed Description

Transfer of inst & address for concurrent xip mode.

## Macro Definition Documentation

## ◆ LL_QSPI_CONCURRENT_XIP_INST_ADDR_ALL_IN_SPI

#define LL_QSPI_CONCURRENT_XIP_INST_ADDR_ALL_IN_SPI 0x0

Instruction and address are sent in SPI mode.

Definition at line 632 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_INST_ADDR_ALL_IN_SPIFRF

#define LL_QSPI_CONCURRENT_XIP_INST_ADDR_ALL_IN_SPIFRF 0x2

Instruction and address are sent in Daul/Quad SPI mode.

Definition at line 634 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_INST_IN_SPI_ADDR_IN_SPIFRF

#define LL_QSPI_CONCURRENT_XIP_INST_IN_SPI_ADDR_IN_SPIFRF 0x1

Instruction is in sent in SPI mode and address is sent in Daul/Quad SPI mode.

Definition at line 633 of file gr55xx_ll_qspi.h.