Macros
Mode Bits Length For Xip
Peripheral Driver » LL Driver » QSPI » Defines » QSPI Exported Constants

More...

Collaboration diagram for Mode Bits Length For Xip:

## Macros
#define | LL_QSPI_CONCURRENT_XIP_MBL_2 0x0 /* mode bits length equals to 2 bit */
#define | LL_QSPI_CONCURRENT_XIP_MBL_4 0x1 /* mode bits length equals to 4 bit */
#define | LL_QSPI_CONCURRENT_XIP_MBL_8 0x2 /* mode bits length equals to 8 bit */
#define | LL_QSPI_CONCURRENT_XIP_MBL_16 0x3 /* mode bits length equals to 16 bit */

## Detailed Description

Mode bits length for xip mode

## Macro Definition Documentation

## ◆ LL_QSPI_CONCURRENT_XIP_MBL_16

#define LL_QSPI_CONCURRENT_XIP_MBL_16 0x3 /* mode bits length equals to 16 bit */

Definition at line 593 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_MBL_2

#define LL_QSPI_CONCURRENT_XIP_MBL_2 0x0 /* mode bits length equals to 2 bit */

Definition at line 590 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_MBL_4

#define LL_QSPI_CONCURRENT_XIP_MBL_4 0x1 /* mode bits length equals to 4 bit */

Definition at line 591 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_CONCURRENT_XIP_MBL_8

#define LL_QSPI_CONCURRENT_XIP_MBL_8 0x2 /* mode bits length equals to 8 bit */

Definition at line 592 of file gr55xx_ll_qspi.h.