### - i -

- I2C_ADDRESSINGMODE_10BIT : gr55xx_hal_i2c.h
- I2C_ADDRESSINGMODE_7BIT : gr55xx_hal_i2c.h
- I2C_DEFAULT_CONFIG : gr55xx_hal_i2c.h
- I2C_FIRST_AND_LAST_FRAME : gr55xx_hal_i2c.h
- I2C_FIRST_AND_NEXT_FRAME : gr55xx_hal_i2c.h
- I2C_FIRST_FRAME : gr55xx_hal_i2c.h
- I2C_GENERALCALL_DISABLE : gr55xx_hal_i2c.h
- I2C_GENERALCALL_ENABLE : gr55xx_hal_i2c.h
- I2C_LAST_FRAME : gr55xx_hal_i2c.h
- I2C_MEM_ADD_LSB : gr55xx_hal_i2c.h
- I2C_MEM_ADD_MSB : gr55xx_hal_i2c.h
- I2C_MEMADD_SIZE_16BIT : gr55xx_hal_i2c.h
- I2C_MEMADD_SIZE_8BIT : gr55xx_hal_i2c.h
- I2C_NEXT_FRAME : gr55xx_hal_i2c.h
- I2C_SPEED_1000K : gr55xx_hal_i2c.h
- I2C_SPEED_100K : gr55xx_hal_i2c.h
- I2C_SPEED_2000K : gr55xx_hal_i2c.h
- I2C_SPEED_400K : gr55xx_hal_i2c.h
- I2C_TIMING_FS_SCL_HIGH : gr55xx_hal_i2c.h
- I2C_TIMING_FS_SCL_LOW : gr55xx_hal_i2c.h
- I2C_TIMING_FS_SPK : gr55xx_hal_i2c.h
- I2C_TIMING_HS_SCL_HIGH : gr55xx_hal_i2c.h
- I2C_TIMING_HS_SCL_LOW : gr55xx_hal_i2c.h
- I2C_TIMING_HS_SPK : gr55xx_hal_i2c.h
- I2C_TIMING_SDA_RX_HOLD : gr55xx_hal_i2c.h
- I2C_TIMING_SDA_TX_HOLD : gr55xx_hal_i2c.h
- I2C_TIMING_SS_SCL_HIGH : gr55xx_hal_i2c.h
- I2C_TIMING_SS_SCL_LOW : gr55xx_hal_i2c.h
- I2S_CLOCK_SRC_32M : gr55xx_hal_i2s.h
- I2S_CLOCK_SRC_64M : gr55xx_hal_i2s.h
- I2S_CLOCK_SRC_96M : gr55xx_hal_i2s.h
- I2S_DATASIZE_12BIT : gr55xx_hal_i2s.h
- I2S_DATASIZE_16BIT : gr55xx_hal_i2s.h
- I2S_DATASIZE_20BIT : gr55xx_hal_i2s.h
- I2S_DATASIZE_24BIT : gr55xx_hal_i2s.h
- I2S_DATASIZE_32BIT : gr55xx_hal_i2s.h
- I2S_DIRECTION_FULL_DUPLEX : gr55xx_hal_i2s.h
- I2S_DIRECTION_SIMPLEX_RX : gr55xx_hal_i2s.h
- I2S_DIRECTION_SIMPLEX_TX : gr55xx_hal_i2s.h
- I2S_FLAG_RXDA : gr55xx_hal_i2s.h
- I2S_FLAG_RXFO : gr55xx_hal_i2s.h
- I2S_FLAG_TXFE : gr55xx_hal_i2s.h
- I2S_FLAG_TXFO : gr55xx_hal_i2s.h
- I2S_IT_RXDA : gr55xx_hal_i2s.h
- I2S_IT_RXFO : gr55xx_hal_i2s.h
- I2S_IT_TXFE : gr55xx_hal_i2s.h
- I2S_IT_TXFO : gr55xx_hal_i2s.h
- I2S_RX_FIFO_LEVEL_MAX : gr55xx_hal_i2s.h
- I2S_TX_FIFO_LEVEL_MAX : gr55xx_hal_i2s.h
- I2S_WS_CYCLES_16 : gr55xx_hal_i2s.h
- I2S_WS_CYCLES_24 : gr55xx_hal_i2s.h
- I2S_WS_CYCLES_32 : gr55xx_hal_i2s.h
- IAS_C_CONNECTION_MAX : ias_c.h
- IS_ADC_CLOCK : gr55xx_hal_adc.h
- IS_ADC_INPUT : gr55xx_hal_adc.h
- IS_ADC_INPUT_MODE : gr55xx_hal_adc.h
- IS_ADC_REF : gr55xx_hal_adc.h
- IS_ADC_REF_VALUE : gr55xx_hal_adc.h
- IS_AES_CHAININGMODE : gr55xx_hal_aes.h
- IS_AES_KEY_SIZE : gr55xx_hal_aes.h
- IS_AES_OPERATION_MODE : gr55xx_hal_aes.h
- IS_AON_GPIO_MODE : gr55xx_hal_aon_gpio.h
- IS_AON_GPIO_PIN : gr55xx_hal_aon_gpio.h
- IS_AON_GPIO_PIN_ACTION : gr55xx_hal_aon_gpio.h
- IS_AON_GPIO_PULL : gr55xx_hal_aon_gpio.h
- IS_CALENDAR_ALARM_TYPE : gr55xx_hal_calendar.h
- IS_CALENDAR_DATE : gr55xx_hal_calendar.h
- IS_CALENDAR_LEAP_YEAR : gr55xx_hal_calendar.h
- IS_CALENDAR_WEEKDAY : gr55xx_hal_calendar.h
- IS_COMP_HYST_NEG : gr55xx_hal_comp.h
- IS_COMP_HYST_POS : gr55xx_hal_comp.h
- IS_COMP_INPUT : gr55xx_hal_comp.h
- IS_COMP_REF : gr55xx_hal_comp.h
- IS_COMP_RES_DEGENERATION_NEG : gr55xx_hal_comp.h
- IS_COMP_RES_DEGENERATION_POS : gr55xx_hal_comp.h
- IS_DMA_ALL_INSTANCE : gr55xx_hal_dma.h
- IS_DMA_ALL_P_INSTANCE : gr55xx_hal_dma.h
- IS_DMA_ALL_REQUEST : gr55xx_hal_dma.h
- IS_DMA_BUFFER_SIZE : gr55xx_hal_dma.h
- IS_DMA_DESTINATION_DATA_SIZE : gr55xx_hal_dma.h
- IS_DMA_DESTINATION_INC_STATE : gr55xx_hal_dma.h
- IS_DMA_DIRECTION : gr55xx_hal_dma.h
- IS_DMA_DST_SCATTER_EN : gr55xx_hal_dma.h
- IS_DMA_LLP_DST_EN : gr55xx_hal_dma.h
- IS_DMA_LLP_SRC_EN : gr55xx_hal_dma.h
- IS_DMA_MODE : gr55xx_hal_dma.h
- IS_DMA_PRIORITY : gr55xx_hal_dma.h
- IS_DMA_SOURCE_DATA_SIZE : gr55xx_hal_dma.h
- IS_DMA_SOURCE_INC_STATE : gr55xx_hal_dma.h
- IS_DMA_SRC_GATHER_EN : gr55xx_hal_dma.h
- IS_DSPI_CLOCK_PRESCALER : gr55xx_hal_dspi.h
- IS_DSPI_INSTRUCTION_SIZE : gr55xx_hal_dspi.h
- IS_DSPI_INTERFACE_MODE : gr55xx_hal_dspi.h
- IS_DUAL_TIMER_COUNTERMODE : gr55xx_hal_dual_tim.h
- IS_DUAL_TIMER_PRESCALER : gr55xx_hal_dual_tim.h
- IS_EXFLASH_ERASE_TYPE : gr55xx_hal_exflash.h
- IS_EXFLASH_LOCK_AREA : gr55xx_hal_exflash.h
- IS_GPIO_MODE : gr55xx_hal_gpio.h
- IS_GPIO_PIN : gr55xx_hal_gpio.h
- IS_GPIO_PIN_ACTION : gr55xx_hal_gpio.h
- IS_GPIO_PULL : gr55xx_hal_gpio.h
- IS_I2C_ADDRESSING_MODE : gr55xx_hal_i2c.h
- IS_I2C_GENERAL_CALL : gr55xx_hal_i2c.h
- IS_I2C_MEMADD_SIZE : gr55xx_hal_i2c.h
- IS_I2C_OWN_ADDRESS : gr55xx_hal_i2c.h
- IS_I2C_SLV_ADDRESS : gr55xx_hal_i2c.h
- IS_I2C_SPEED : gr55xx_hal_i2c.h
- IS_I2C_TRANSFER_OPTIONS_REQUEST : gr55xx_hal_i2c.h
- IS_I2S_AUDIO_FREQUENCY : gr55xx_hal_i2s.h
- IS_I2S_CPOL : gr55xx_hal_i2s.h
- IS_I2S_DATASIZE : gr55xx_hal_i2s.h
- IS_I2S_DIRECTION : gr55xx_hal_i2s.h
- IS_I2S_FIFO_THRESHOLD : gr55xx_hal_i2s.h
- IS_LAST : tsi_malloc_intern.h
- IS_MSIO_DIRECTION : gr55xx_hal_msio.h
- IS_MSIO_MODE : gr55xx_hal_msio.h
- IS_MSIO_PIN : gr55xx_hal_msio.h
- IS_MSIO_PIN_ACTION : gr55xx_hal_msio.h
- IS_MSIO_PULL : gr55xx_hal_msio.h
- IS_NVIC_DEVICE_IRQ : gr55xx_hal_cortex.h
- IS_NVIC_PREEMPTION_PRIORITY : gr55xx_hal_cortex.h
- IS_NVIC_PRIORITY_GROUP : gr55xx_hal_cortex.h
- IS_NVIC_SUB_PRIORITY : gr55xx_hal_cortex.h
- IS_PKC_BIGMULTI_BITS_LENGTH : gr55xx_hal_pkc.h
- IS_PKC_BITS_LENGTH : gr55xx_hal_pkc.h
- IS_PKC_OPERATION_MODE : gr55xx_hal_pkc.h
- IS_PKC_SECURE_MODE : gr55xx_hal_pkc.h
- IS_PWM_ALIGNMENT_MODE : gr55xx_hal_pwm.h
- IS_PWM_DRIVEPOLARITY : gr55xx_hal_pwm.h
- IS_PWM_MODE : gr55xx_hal_pwm.h
- IS_PWM_STOP_LVL : gr55xx_hal_pwm.h
- IS_PWR_MEM_BLOCK : gr55xx_hal_pwr.h
- IS_PWR_MEM_POWER_STAT : gr55xx_hal_pwr.h
- IS_PWR_PWR_TIMER_TYPE : gr55xx_hal_pwr.h
- IS_PWR_WAKEUP_CONDITION : gr55xx_hal_pwr.h
- IS_QSPI_ADDRESS_SIZE : gr55xx_hal_qspi.h
- IS_QSPI_CLOCK_MODE : gr55xx_hal_qspi.h
- IS_QSPI_CLOCK_PRESCALER : gr55xx_hal_qspi.h
- IS_QSPI_CONC_INST_ADDR_XFER_FORMAT : gr55xx_hal_qspi.h
- IS_QSPI_CONC_XIP_ADDR_SIZE : gr55xx_hal_qspi.h
- IS_QSPI_CONC_XIP_CONT_XFER_EN : gr55xx_hal_qspi.h
- IS_QSPI_CONC_XIP_CONT_XFER_TOC : gr55xx_hal_qspi.h
- IS_QSPI_CONC_XIP_DATA_FRF : gr55xx_hal_qspi.h
- IS_QSPI_CONC_XIP_DFS : gr55xx_hal_qspi.h
- IS_QSPI_CONC_XIP_DFS_HC_EN : gr55xx_hal_qspi.h
- IS_QSPI_CONC_XIP_DUMMY_CYCLES : gr55xx_hal_qspi.h
- IS_QSPI_CONC_XIP_ENDIAN_MODE : gr55xx_hal_qspi.h
- IS_QSPI_CONC_XIP_INST : gr55xx_hal_qspi.h
- IS_QSPI_CONC_XIP_INST_EN : gr55xx_hal_qspi.h
- IS_QSPI_CONC_XIP_INST_SIZE : gr55xx_hal_qspi.h
- IS_QSPI_CONC_XIP_MODE_BITS : gr55xx_hal_qspi.h
- IS_QSPI_CONC_XIP_MODE_BITS_EN : gr55xx_hal_qspi.h
- IS_QSPI_CONC_XIP_MODE_BITS_SIZE : gr55xx_hal_qspi.h
- IS_QSPI_CONC_XIP_PREFETCH_EN : gr55xx_hal_qspi.h
- IS_QSPI_CONC_XIP_SIOO_MODE : gr55xx_hal_qspi.h
- IS_QSPI_DATA_MODE : gr55xx_hal_qspi.h
- IS_QSPI_DUMMY_CYCLES : gr55xx_hal_qspi.h
- IS_QSPI_FIFO_THRESHOLD : gr55xx_hal_qspi.h
- IS_QSPI_INSTADDR_MODE : gr55xx_hal_qspi.h
- IS_QSPI_INSTRUCTION_SIZE : gr55xx_hal_qspi.h
- IS_QSPI_RX_SAMPLE_DLY : gr55xx_hal_qspi.h
- IS_QSPI_SUPPORTED_DATA_SIZE : gr55xx_hal_qspi.h
- IS_SK_BOARD : graphics_dc_lcd_drv.h
- IS_SPI_BAUDRATE_PRESCALER : gr55xx_hal_spi.h
- IS_SPI_CPHA : gr55xx_hal_spi.h
- IS_SPI_CPOL : gr55xx_hal_spi.h
- IS_SPI_DATASIZE : gr55xx_hal_spi.h
- IS_SPI_DIRECTION : gr55xx_hal_spi.h
- IS_SPI_FIFO_THRESHOLD : gr55xx_hal_spi.h
- IS_SPI_RX_SAMPLE_DLY : gr55xx_hal_spi.h
- IS_SPI_SLAVE : gr55xx_hal_spi.h
- IS_SPI_TIMODE : gr55xx_hal_spi.h
- IS_TRANSFER_REQUEST : gr55xx_hal_i2c.h
- IS_UART_BAUDRATE : gr55xx_hal_uart.h
- IS_UART_DATABITS : gr55xx_hal_uart.h
- IS_UART_HARDWARE_FLOW_CONTROL : gr55xx_hal_uart.h
- IS_UART_PARITY : gr55xx_hal_uart.h
- IS_UART_STOPBITS : gr55xx_hal_uart.h
- IS_USB_ENUM_TYPE : gr55xx_hal_usb.h
- IS_USB_PWR_MODE : gr55xx_hal_usb.h
- IS_USB_SPEED : gr55xx_hal_usb.h
- IS_WDT_RESET_MODE : gr55xx_hal_wdt.h
- IS_XQSPI_ADDRESS_SIZE : gr55xx_hal_xqspi.h
- IS_XQSPI_BAUD_RATE : gr55xx_hal_xqspi.h
- IS_XQSPI_CACHE_FLUSH : gr55xx_hal_xqspi.h
- IS_XQSPI_CACHE_MAPPING : gr55xx_hal_xqspi.h
- IS_XQSPI_CACHE_MODE : gr55xx_hal_xqspi.h
- IS_XQSPI_CLOCK_MODE : gr55xx_hal_xqspi.h
- IS_XQSPI_DATA_MODE : gr55xx_hal_xqspi.h
- IS_XQSPI_FIFO_THRESHOLD : gr55xx_hal_xqspi.h
- IS_XQSPI_INSTADDR_MODE : gr55xx_hal_xqspi.h
- IS_XQSPI_INSTRUCTION_SIZE : gr55xx_hal_xqspi.h
- IS_XQSPI_READ_CMD : gr55xx_hal_xqspi.h
- IS_XQSPI_WORK_MODE : gr55xx_hal_xqspi.h
- ISO7816_DEFAULT_CONFIG : gr55xx_hal_iso7816.h
- ISO_ADDR_LEN : ble_iso.h
- ISO_SYNC0_PULSE : ble_iso.h
- ISO_SYNC1_PULSE : ble_iso.h