Macros
SPI Interrupt Definition
Peripheral Driver » HAL Driver » SPI » Defines » SPI Exported Constants
Collaboration diagram for SPI Interrupt Definition:

## Macros
#define | SPI_IT_MST LL_SPI_IS_MST
| Multi-Master Contention Interrupt flag More...
#define | SPI_IT_RXF LL_SPI_IS_RXF
| Receive FIFO Full Interrupt flag More...
#define | SPI_IT_RXO LL_SPI_IS_RXO
| Receive FIFO Overflow Interrupt flag More...
#define | SPI_IT_RXU LL_SPI_IS_RXU
| Receive FIFO Underflow Interrupt flag More...
#define | SPI_IT_TXO LL_SPI_IS_TXO
| Transmit FIFO Overflow Interrupt flag More...
#define | SPI_IT_TXE LL_SPI_IS_TXE
| Transmit FIFO Empty Interrupt flag More...

## Detailed Description

## Macro Definition Documentation

## ◆ SPI_IT_MST

#define SPI_IT_MST LL_SPI_IS_MST

Multi-Master Contention Interrupt flag

Definition at line 397 of file gr55xx_hal_spi.h.

## ◆ SPI_IT_RXF

#define SPI_IT_RXF LL_SPI_IS_RXF

Receive FIFO Full Interrupt flag

Definition at line 398 of file gr55xx_hal_spi.h.

## ◆ SPI_IT_RXO

#define SPI_IT_RXO LL_SPI_IS_RXO

Receive FIFO Overflow Interrupt flag

Definition at line 399 of file gr55xx_hal_spi.h.

## ◆ SPI_IT_RXU

#define SPI_IT_RXU LL_SPI_IS_RXU

Receive FIFO Underflow Interrupt flag

Definition at line 400 of file gr55xx_hal_spi.h.

## ◆ SPI_IT_TXE

#define SPI_IT_TXE LL_SPI_IS_TXE

Transmit FIFO Empty Interrupt flag

Definition at line 402 of file gr55xx_hal_spi.h.

## ◆ SPI_IT_TXO

#define SPI_IT_TXO LL_SPI_IS_TXO

Transmit FIFO Overflow Interrupt flag

Definition at line 401 of file gr55xx_hal_spi.h.