Macros
Interrupt Defines
Peripheral Driver » LL Driver » I2S » Defines » I2S Exported Constants

Interrupt definitions which can be used with LL_I2S_ReadReg and LL_I2S_WriteReg functions. More...

Collaboration diagram for Interrupt Defines:

## Macros
#define | LL_I2S_INT_TXFO I2S_INT_MASK_TX_FOM
| TX FIFO write overflow interrupt More...
#define | LL_I2S_INT_TXFE I2S_INT_MASK_TX_FEM
| TX FIFO threshold level is not reached interrupt. More...
#define | LL_I2S_INT_RXFO I2S_INT_MASK_RX_FOM
| RX FIFO receive overflow interrupt More...
#define | LL_I2S_INT_RXDA I2S_INT_MASK_RX_DAM
| RX FIFO threshold level is reached interrupt More...

## Detailed Description

Interrupt definitions which can be used with LL_I2S_ReadReg and LL_I2S_WriteReg functions.

## Macro Definition Documentation

## ◆ LL_I2S_INT_RXDA

#define LL_I2S_INT_RXDA I2S_INT_MASK_RX_DAM

RX FIFO threshold level is reached interrupt

Definition at line 144 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_INT_RXFO

#define LL_I2S_INT_RXFO I2S_INT_MASK_RX_FOM

RX FIFO receive overflow interrupt

Definition at line 143 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_INT_TXFE

#define LL_I2S_INT_TXFE I2S_INT_MASK_TX_FEM

TX FIFO threshold level is not reached interrupt.

Definition at line 142 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_INT_TXFO

#define LL_I2S_INT_TXFO I2S_INT_MASK_TX_FOM

TX FIFO write overflow interrupt

Definition at line 141 of file gr55xx_ll_i2s.h.