Macros
Datawidth
Peripheral Driver » LL Driver » SPI » Defines » SPI Exported Constants
Collaboration diagram for Datawidth:

## Macros
#define | LL_SPI_DATASIZE_4BIT (3UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)
| Data length for SPI transfer: 4 bits. More...
#define | LL_SPI_DATASIZE_5BIT (4UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)
| Data length for SPI transfer: 5 bits. More...
#define | LL_SPI_DATASIZE_6BIT (5UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)
| Data length for SPI transfer: 6 bits. More...
#define | LL_SPI_DATASIZE_7BIT (6UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)
| Data length for SPI transfer: 7 bits. More...
#define | LL_SPI_DATASIZE_8BIT (7UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)
| Data length for SPI transfer: 8 bits. More...
#define | LL_SPI_DATASIZE_9BIT (8UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)
| Data length for SPI transfer: 9 bits. More...
#define | LL_SPI_DATASIZE_10BIT (9UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)
| Data length for SPI transfer: 10 bits. More...
#define | LL_SPI_DATASIZE_11BIT (10UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)
| Data length for SPI transfer: 11 bits. More...
#define | LL_SPI_DATASIZE_12BIT (11UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)
| Data length for SPI transfer: 12 bits. More...
#define | LL_SPI_DATASIZE_13BIT (12UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)
| Data length for SPI transfer: 13 bits. More...
#define | LL_SPI_DATASIZE_14BIT (13UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)
| Data length for SPI transfer: 14 bits. More...
#define | LL_SPI_DATASIZE_15BIT (14UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)
| Data length for SPI transfer: 15 bits. More...
#define | LL_SPI_DATASIZE_16BIT (15UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)
| Data length for SPI transfer: 16 bits. More...
#define | LL_SPI_DATASIZE_17BIT (16UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)
| Data length for SPI transfer: 17 bits. More...
#define | LL_SPI_DATASIZE_18BIT (17UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)
| Data length for SPI transfer: 18 bits. More...
#define | LL_SPI_DATASIZE_19BIT (18UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)
| Data length for SPI transfer: 19 bits. More...
#define | LL_SPI_DATASIZE_20BIT (19UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)
| Data length for SPI transfer: 20 bits. More...
#define | LL_SPI_DATASIZE_21BIT (20UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)
| Data length for SPI transfer: 21 bits. More...
#define | LL_SPI_DATASIZE_22BIT (21UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)
| Data length for SPI transfer: 22 bits. More...
#define | LL_SPI_DATASIZE_23BIT (22UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)
| Data length for SPI transfer: 23 bits. More...
#define | LL_SPI_DATASIZE_24BIT (23UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)
| Data length for SPI transfer: 24 bits. More...
#define | LL_SPI_DATASIZE_25BIT (24UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)
| Data length for SPI transfer: 25 bits. More...
#define | LL_SPI_DATASIZE_26BIT (25UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)
| Data length for SPI transfer: 26 bits. More...
#define | LL_SPI_DATASIZE_27BIT (26UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)
| Data length for SPI transfer: 27 bits. More...
#define | LL_SPI_DATASIZE_28BIT (27UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)
| Data length for SPI transfer: 28 bits. More...
#define | LL_SPI_DATASIZE_29BIT (28UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)
| Data length for SPI transfer: 29 bits. More...
#define | LL_SPI_DATASIZE_30BIT (29UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)
| Data length for SPI transfer: 30 bits. More...
#define | LL_SPI_DATASIZE_31BIT (30UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)
| Data length for SPI transfer: 31 bits. More...
#define | LL_SPI_DATASIZE_32BIT (31UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)
| Data length for SPI transfer: 32 bits. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_SPI_DATASIZE_10BIT

#define LL_SPI_DATASIZE_10BIT (9UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)

Data length for SPI transfer: 10 bits.

Definition at line 196 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_DATASIZE_11BIT

#define LL_SPI_DATASIZE_11BIT (10UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)

Data length for SPI transfer: 11 bits.

Definition at line 197 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_DATASIZE_12BIT

#define LL_SPI_DATASIZE_12BIT (11UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)

Data length for SPI transfer: 12 bits.

Definition at line 198 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_DATASIZE_13BIT

#define LL_SPI_DATASIZE_13BIT (12UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)

Data length for SPI transfer: 13 bits.

Definition at line 199 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_DATASIZE_14BIT

#define LL_SPI_DATASIZE_14BIT (13UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)

Data length for SPI transfer: 14 bits.

Definition at line 200 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_DATASIZE_15BIT

#define LL_SPI_DATASIZE_15BIT (14UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)

Data length for SPI transfer: 15 bits.

Definition at line 201 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_DATASIZE_16BIT

#define LL_SPI_DATASIZE_16BIT (15UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)

Data length for SPI transfer: 16 bits.

Definition at line 202 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_DATASIZE_17BIT

#define LL_SPI_DATASIZE_17BIT (16UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)

Data length for SPI transfer: 17 bits.

Definition at line 203 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_DATASIZE_18BIT

#define LL_SPI_DATASIZE_18BIT (17UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)

Data length for SPI transfer: 18 bits.

Definition at line 204 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_DATASIZE_19BIT

#define LL_SPI_DATASIZE_19BIT (18UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)

Data length for SPI transfer: 19 bits.

Definition at line 205 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_DATASIZE_20BIT

#define LL_SPI_DATASIZE_20BIT (19UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)

Data length for SPI transfer: 20 bits.

Definition at line 206 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_DATASIZE_21BIT

#define LL_SPI_DATASIZE_21BIT (20UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)

Data length for SPI transfer: 21 bits.

Definition at line 207 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_DATASIZE_22BIT

#define LL_SPI_DATASIZE_22BIT (21UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)

Data length for SPI transfer: 22 bits.

Definition at line 208 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_DATASIZE_23BIT

#define LL_SPI_DATASIZE_23BIT (22UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)

Data length for SPI transfer: 23 bits.

Definition at line 209 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_DATASIZE_24BIT

#define LL_SPI_DATASIZE_24BIT (23UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)

Data length for SPI transfer: 24 bits.

Definition at line 210 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_DATASIZE_25BIT

#define LL_SPI_DATASIZE_25BIT (24UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)

Data length for SPI transfer: 25 bits.

Definition at line 211 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_DATASIZE_26BIT

#define LL_SPI_DATASIZE_26BIT (25UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)

Data length for SPI transfer: 26 bits.

Definition at line 212 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_DATASIZE_27BIT

#define LL_SPI_DATASIZE_27BIT (26UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)

Data length for SPI transfer: 27 bits.

Definition at line 213 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_DATASIZE_28BIT

#define LL_SPI_DATASIZE_28BIT (27UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)

Data length for SPI transfer: 28 bits.

Definition at line 214 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_DATASIZE_29BIT

#define LL_SPI_DATASIZE_29BIT (28UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)

Data length for SPI transfer: 29 bits.

Definition at line 215 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_DATASIZE_30BIT

#define LL_SPI_DATASIZE_30BIT (29UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)

Data length for SPI transfer: 30 bits.

Definition at line 216 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_DATASIZE_31BIT

#define LL_SPI_DATASIZE_31BIT (30UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)

Data length for SPI transfer: 31 bits.

Definition at line 217 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_DATASIZE_32BIT

#define LL_SPI_DATASIZE_32BIT (31UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)

Data length for SPI transfer: 32 bits.

Definition at line 218 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_DATASIZE_4BIT

#define LL_SPI_DATASIZE_4BIT (3UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)

Data length for SPI transfer: 4 bits.

Definition at line 190 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_DATASIZE_5BIT

#define LL_SPI_DATASIZE_5BIT (4UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)

Data length for SPI transfer: 5 bits.

Definition at line 191 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_DATASIZE_6BIT

#define LL_SPI_DATASIZE_6BIT (5UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)

Data length for SPI transfer: 6 bits.

Definition at line 192 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_DATASIZE_7BIT

#define LL_SPI_DATASIZE_7BIT (6UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)

Data length for SPI transfer: 7 bits.

Definition at line 193 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_DATASIZE_8BIT

#define LL_SPI_DATASIZE_8BIT (7UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)

Data length for SPI transfer: 8 bits.

Definition at line 194 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_DATASIZE_9BIT

#define LL_SPI_DATASIZE_9BIT (8UL << SPI_CTRL0_DATA_FRAME_SIZE_POS)

Data length for SPI transfer: 9 bits.

Definition at line 195 of file gr55xx_ll_spi.h.