Macros
Alert Status BIT
BLE Services » Phone Alert Status Service Client (PASS_C) » Defines

PASS Alert Status bits. More...

Collaboration diagram for Alert Status BIT:

## Macros
#define | PASS_C_CONNECTION_MAX 10
| Maximum number of HRS Client connections. More...
#define | PASS_C_NO_STATE_ACTIVE (0x00)
| Bit for no state active. More...
#define | PASS_C_RINGER_ACTIVE (0x01 << 0)
| Bit for ringer State active. More...
#define | PASS_C_VIBRATE_ACTIVE (0x01 << 1)
| Bit for vibrate State active. More...
#define | PASS_C_DISPLAY_ALERT_ACTIVE (0x01 << 2)
| Bit for display Alert Status State active. More...
#define | PASS_C_ALL_STATE_ACTIVE (0x07)
| Bit for no state active. More...

## Detailed Description

PASS Alert Status bits.

## Macro Definition Documentation

## ◆ PASS_C_ALL_STATE_ACTIVE

#define PASS_C_ALL_STATE_ACTIVE (0x07)

Bit for no state active.

Definition at line 82 of file pass_c.h.

## ◆ PASS_C_CONNECTION_MAX

#define PASS_C_CONNECTION_MAX 10

Maximum number of HRS Client connections.

Definition at line 77 of file pass_c.h.

## ◆ PASS_C_DISPLAY_ALERT_ACTIVE

#define PASS_C_DISPLAY_ALERT_ACTIVE (0x01 << 2)

Bit for display Alert Status State active.

Definition at line 81 of file pass_c.h.

## ◆ PASS_C_NO_STATE_ACTIVE

#define PASS_C_NO_STATE_ACTIVE (0x00)

Bit for no state active.

Definition at line 78 of file pass_c.h.

## ◆ PASS_C_RINGER_ACTIVE

#define PASS_C_RINGER_ACTIVE (0x01 << 0)

Bit for ringer State active.

Definition at line 79 of file pass_c.h.

## ◆ PASS_C_VIBRATE_ACTIVE

#define PASS_C_VIBRATE_ACTIVE (0x01 << 1)

Bit for vibrate State active.

Definition at line 80 of file pass_c.h.