Public Attributes | List of all members
ble_gap_evt_conn_param_updated_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Structures

Connection parameter updated event for BLE_GAPC_EVT_CONN_PARAM_UPDATED. More...

`#include <ble_gapc.h>`

## Public Attributes
uint16_t | conn_interval
| Connection interval. More...
uint16_t | slave_latency
| Latency for the connection in number of connection events. More...
uint16_t | sup_timeout
| Supervision timeout for the LE link. More...

## Detailed Description

Connection parameter updated event for BLE_GAPC_EVT_CONN_PARAM_UPDATED.

Definition at line 765 of file ble_gapc.h.

## Member Data Documentation

## ◆ conn_interval

uint16_t ble_gap_evt_conn_param_updated_t::conn_interval

Connection interval.

Range: 0x0006 to 0x0C80. Unit: 1.25 ms. Time range: 7.5 ms to 4 s.

Definition at line 767 of file ble_gapc.h.

## ◆ slave_latency

uint16_t ble_gap_evt_conn_param_updated_t::slave_latency

Latency for the connection in number of connection events.

Range: 0x0000 to 0x01F3.

Definition at line 768 of file ble_gapc.h.

## ◆ sup_timeout

uint16_t ble_gap_evt_conn_param_updated_t::sup_timeout

Supervision timeout for the LE link.

Range: 0x000A to 0x0C80, unit: 10 ms, time range: 100 ms to 32 s.

Definition at line 769 of file ble_gapc.h.

The documentation for this struct was generated from the following file:

- ble_gapc.h