Macros
InitStrcut default configuartion
Peripheral Driver » LL Driver » I2S » Defines » I2S Exported Constants
Collaboration diagram for InitStrcut default configuartion:

## Macros
#define | LL_I2S_DEFAULT_CONFIG
| LL I2S InitStrcut default configuartion. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_I2S_DEFAULT_CONFIG

#define LL_I2S_DEFAULT_CONFIG

Value:
{ \
.rxdata_size = LL_I2S_DATASIZE_16BIT, \
.txdata_size = LL_I2S_DATASIZE_16BIT, \
.rx_threshold = LL_I2S_THRESHOLD_1FIFO, \
.tx_threshold = LL_I2S_THRESHOLD_9FIFO, \
.clock_source = LL_I2S_CLOCK_SRC_32M, \
.audio_freq = 48000 \
}

LL I2S InitStrcut default configuartion.

Definition at line 256 of file gr55xx_ll_i2s.h.

LL_I2S_CLOCK_SRC_32M
#define LL_I2S_CLOCK_SRC_32M
I2S clock source select: 32M
Definition: gr55xx_ll_i2s.h:152
LL_I2S_THRESHOLD_9FIFO
#define LL_I2S_THRESHOLD_9FIFO
Trigger level for FIFO: 9 depth.
Definition: gr55xx_ll_i2s.h:185
LL_I2S_DATASIZE_16BIT
#define LL_I2S_DATASIZE_16BIT
Data size for I2S transfer: 16 bits.
Definition: gr55xx_ll_i2s.h:160
LL_I2S_THRESHOLD_1FIFO
#define LL_I2S_THRESHOLD_1FIFO
Trigger level for FIFO: 1 depth.
Definition: gr55xx_ll_i2s.h:177