Macros
Peripherals Off During WFI/WFE
Peripheral Driver » LL Driver » CGC » Defines » CGC Exported Constants

Turn the peripherals off during WFI/WFE. More...

Collaboration diagram for Peripherals Off During WFI/WFE:

## Macros
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_UART_0_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_UART0
| Turn the uart0 off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_UART_1_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_UART1
| Turn the uart1 off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_UART_2_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_UART2
| Turn the uart2 off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_UART_3_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_UART3
| Turn the uart3 off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_UART_4_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_UART4
| Turn the uart4 off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_UART_5_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_UART5
| Turn the uart5 off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_I2S_M_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2SM
| Turn the i2s_m off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_I2S_S_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2SS
| Turn the i2s_s off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_SPI_M_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_SPIM
| Turn the spi_m off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_SPI_S_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_SPIS
| Turn the spi_s off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_PWM_0_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_PWM0
| Turn the pwm0 off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_PWM_1_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_PWM1
| Turn the pwm1 off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_QSPIM_0_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_QSPIM0
| Turn the qspim0 off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_QSPIM_1_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_QSPIM1
| Turn the qspim1 off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_QSPIM_2_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_QSPIM2
| Turn the qspim2 off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_DSPI_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_DSPI
| Turn the dspi off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_PDM_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_PDM
| Turn the pdm off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_0_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2C0
| Turn the i2c0 off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_1_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2C1
| Turn the i2c1 off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_2_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2C2
| Turn the i2c0 off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_3_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2C3
| Turn the i2c1 off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_4_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2C4
| Turn the i2c0 off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_5_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2C5
| Turn the i2c1 off during WFI/WFE More...
#define | LL_CGC_MCU_PERIPH_SERIALS_SLP_OFF ((uint32_t)0x01FC3FFFUL)
| Serial blocks More...
#define | LL_CGC_MCU_PERIPH_SERIALS_SLP_ALL ((uint32_t)0x03FFFF3FUL)
| Serial blocks More...

## Detailed Description

Turn the peripherals off during WFI/WFE.

## Macro Definition Documentation

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_DSPI_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_DSPI_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_DSPI

Turn the dspi off during WFI/WFE

Definition at line 204 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_0_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_0_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2C0

Turn the i2c0 off during WFI/WFE

Definition at line 206 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_1_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_1_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2C1

Turn the i2c1 off during WFI/WFE

Definition at line 207 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_2_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_2_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2C2

Turn the i2c0 off during WFI/WFE

Definition at line 208 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_3_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_3_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2C3

Turn the i2c1 off during WFI/WFE

Definition at line 209 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_4_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_4_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2C4

Turn the i2c0 off during WFI/WFE

Definition at line 210 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_5_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_5_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2C5

Turn the i2c1 off during WFI/WFE

Definition at line 211 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_I2S_M_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_I2S_M_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2SM

Turn the i2s_m off during WFI/WFE

Definition at line 195 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_I2S_S_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_I2S_S_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2SS

Turn the i2s_s off during WFI/WFE

Definition at line 196 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_PDM_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_PDM_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_PDM

Turn the pdm off during WFI/WFE

Definition at line 205 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_PWM_0_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_PWM_0_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_PWM0

Turn the pwm0 off during WFI/WFE

Definition at line 199 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_PWM_1_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_PWM_1_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_PWM1

Turn the pwm1 off during WFI/WFE

Definition at line 200 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_QSPIM_0_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_QSPIM_0_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_QSPIM0

Turn the qspim0 off during WFI/WFE

Definition at line 201 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_QSPIM_1_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_QSPIM_1_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_QSPIM1

Turn the qspim1 off during WFI/WFE

Definition at line 202 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_QSPIM_2_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_QSPIM_2_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_QSPIM2

Turn the qspim2 off during WFI/WFE

Definition at line 203 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_SPI_M_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_SPI_M_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_SPIM

Turn the spi_m off during WFI/WFE

Definition at line 197 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_SPI_S_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_SPI_S_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_SPIS

Turn the spi_s off during WFI/WFE

Definition at line 198 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_UART_0_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_UART_0_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_UART0

Turn the uart0 off during WFI/WFE

Definition at line 189 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_UART_1_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_UART_1_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_UART1

Turn the uart1 off during WFI/WFE

Definition at line 190 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_UART_2_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_UART_2_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_UART2

Turn the uart2 off during WFI/WFE

Definition at line 191 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_UART_3_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_UART_3_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_UART3

Turn the uart3 off during WFI/WFE

Definition at line 192 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_UART_4_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_UART_4_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_UART4

Turn the uart4 off during WFI/WFE

Definition at line 193 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_UART_5_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_UART_5_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_UART5

Turn the uart5 off during WFI/WFE

Definition at line 194 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_SERIALS_SLP_ALL

#define LL_CGC_MCU_PERIPH_SERIALS_SLP_ALL ((uint32_t)0x03FFFF3FUL)

Serial blocks

Definition at line 214 of file gr55xx_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_SERIALS_SLP_OFF

#define LL_CGC_MCU_PERIPH_SERIALS_SLP_OFF ((uint32_t)0x01FC3FFFUL)

Serial blocks

Definition at line 213 of file gr55xx_ll_cgc.h.