Macros
Defines
BLE Services » Heart Rate Service Client (HRS_C)
Collaboration diagram for Defines:

## Macros
#define | HRS_C_CONNECTION_MAX 10
| Maximum number of HRS Client connections. More...
#define | HRS_C_RR_INTERVALS_NUM_MAX 9
| Maximum number of RR intervals in HRS notifications. More...
#define | HRS_C_CTRL_POINT_ENERGY_EXP 0x01
| Value for control point characteristic. More...

## Detailed Description

## Macro Definition Documentation

## ◆ HRS_C_CONNECTION_MAX

#define HRS_C_CONNECTION_MAX 10

Maximum number of HRS Client connections.

Definition at line 71 of file hrs_c.h.

## ◆ HRS_C_CTRL_POINT_ENERGY_EXP

#define HRS_C_CTRL_POINT_ENERGY_EXP 0x01

Value for control point characteristic.

Definition at line 73 of file hrs_c.h.

## ◆ HRS_C_RR_INTERVALS_NUM_MAX

#define HRS_C_RR_INTERVALS_NUM_MAX 9

Maximum number of RR intervals in HRS notifications.

Definition at line 72 of file hrs_c.h.