Public Attributes | List of all members
ble_l2cap_evt_enh_reconfig_ind_t Struct Reference
BLE » Logical Link Control and Adaptation Protocol (L2CAP) » Structures

L2cap Reconfig Enhanced credit Indicate event for BLE_L2CAP_EVT_ENH_RECONFIG_IND. More...

`#include <ble_l2cap.h>`

## Public Attributes
uint16_t | peer_mtu
| It indicates the maximum SDU size (in octets) that the L2CAP layer entity of peer device can receive on these channels. More...
uint16_t | peer_mps
| It indicates the maximum payload size (in octets) that the L2CAP layer entity of peer device can receive on these channels. More...
uint16_t | chl_num
| It specifies the number of channel need to reconfigure, it shall not greater than 5. More...
uint16_t | local_cid [5]
| It represents the local channel endpoints need to reconfigure. More...

## Detailed Description

L2cap Reconfig Enhanced credit Indicate event for BLE_L2CAP_EVT_ENH_RECONFIG_IND.

Definition at line 262 of file ble_l2cap.h.

## Member Data Documentation

## ◆ chl_num

uint16_t ble_l2cap_evt_enh_reconfig_ind_t::chl_num

It specifies the number of channel need to reconfigure, it shall not greater than 5.

Definition at line 266 of file ble_l2cap.h.

## ◆ local_cid

uint16_t ble_l2cap_evt_enh_reconfig_ind_t::local_cid[5]

It represents the local channel endpoints need to reconfigure.

Definition at line 267 of file ble_l2cap.h.

## ◆ peer_mps

uint16_t ble_l2cap_evt_enh_reconfig_ind_t::peer_mps

It indicates the maximum payload size (in octets) that the L2CAP layer entity of peer device can receive on these channels.

Definition at line 265 of file ble_l2cap.h.

## ◆ peer_mtu

uint16_t ble_l2cap_evt_enh_reconfig_ind_t::peer_mtu

It indicates the maximum SDU size (in octets) that the L2CAP layer entity of peer device can receive on these channels.

Definition at line 264 of file ble_l2cap.h.

The documentation for this struct was generated from the following file:

- ble_l2cap.h