Macros
MicroWire CommandSize
Peripheral Driver » LL Driver » SPI » Defines » SPI Exported Constants
Collaboration diagram for MicroWire CommandSize:

## Macros
#define | LL_SPI_MW_CMDSIZE_1BIT 0x00000000UL
| CMD length for Microwire transfer: 1 bits. More...
#define | LL_SPI_MW_CMDSIZE_2BIT (1UL << SPI_CTRL0_CTRL_FRAME_SIZE_POS)
| CMD length for Microwire transfer: 2 bits. More...
#define | LL_SPI_MW_CMDSIZE_3BIT (2UL << SPI_CTRL0_CTRL_FRAME_SIZE_POS)
| CMD length for Microwire transfer: 3 bits. More...
#define | LL_SPI_MW_CMDSIZE_4BIT (3UL << SPI_CTRL0_CTRL_FRAME_SIZE_POS)
| CMD length for Microwire transfer: 4 bits. More...
#define | LL_SPI_MW_CMDSIZE_5BIT (4UL << SPI_CTRL0_CTRL_FRAME_SIZE_POS)
| CMD length for Microwire transfer: 5 bits. More...
#define | LL_SPI_MW_CMDSIZE_6BIT (5UL << SPI_CTRL0_CTRL_FRAME_SIZE_POS)
| CMD length for Microwire transfer: 6 bits. More...
#define | LL_SPI_MW_CMDSIZE_7BIT (6UL << SPI_CTRL0_CTRL_FRAME_SIZE_POS)
| CMD length for Microwire transfer: 7 bits. More...
#define | LL_SPI_MW_CMDSIZE_8BIT (7UL << SPI_CTRL0_CTRL_FRAME_SIZE_POS)
| CMD length for Microwire transfer: 8 bits. More...
#define | LL_SPI_MW_CMDSIZE_9BIT (8UL << SPI_CTRL0_CTRL_FRAME_SIZE_POS)
| CMD length for Microwire transfer: 9 bits. More...
#define | LL_SPI_MW_CMDSIZE_10BIT (9UL << SPI_CTRL0_CTRL_FRAME_SIZE_POS)
| CMD length for Microwire transfer: 10 bits. More...
#define | LL_SPI_MW_CMDSIZE_11BIT (10UL << SPI_CTRL0_CTRL_FRAME_SIZE_POS)
| CMD length for Microwire transfer: 11 bits. More...
#define | LL_SPI_MW_CMDSIZE_12BIT (11UL << SPI_CTRL0_CTRL_FRAME_SIZE_POS)
| CMD length for Microwire transfer: 12 bits. More...
#define | LL_SPI_MW_CMDSIZE_13BIT (12UL << SPI_CTRL0_CTRL_FRAME_SIZE_POS)
| CMD length for Microwire transfer: 13 bits. More...
#define | LL_SPI_MW_CMDSIZE_14BIT (13UL << SPI_CTRL0_CTRL_FRAME_SIZE_POS)
| CMD length for Microwire transfer: 14 bits. More...
#define | LL_SPI_MW_CMDSIZE_15BIT (14UL << SPI_CTRL0_CTRL_FRAME_SIZE_POS)
| CMD length for Microwire transfer: 15 bits. More...
#define | LL_SPI_MW_CMDSIZE_16BIT (15UL << SPI_CTRL0_CTRL_FRAME_SIZE_POS)
| CMD length for Microwire transfer: 16 bits. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_SPI_MW_CMDSIZE_10BIT

#define LL_SPI_MW_CMDSIZE_10BIT (9UL << SPI_CTRL0_CTRL_FRAME_SIZE_POS)

CMD length for Microwire transfer: 10 bits.

Definition at line 233 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_MW_CMDSIZE_11BIT

#define LL_SPI_MW_CMDSIZE_11BIT (10UL << SPI_CTRL0_CTRL_FRAME_SIZE_POS)

CMD length for Microwire transfer: 11 bits.

Definition at line 234 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_MW_CMDSIZE_12BIT

#define LL_SPI_MW_CMDSIZE_12BIT (11UL << SPI_CTRL0_CTRL_FRAME_SIZE_POS)

CMD length for Microwire transfer: 12 bits.

Definition at line 235 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_MW_CMDSIZE_13BIT

#define LL_SPI_MW_CMDSIZE_13BIT (12UL << SPI_CTRL0_CTRL_FRAME_SIZE_POS)

CMD length for Microwire transfer: 13 bits.

Definition at line 236 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_MW_CMDSIZE_14BIT

#define LL_SPI_MW_CMDSIZE_14BIT (13UL << SPI_CTRL0_CTRL_FRAME_SIZE_POS)

CMD length for Microwire transfer: 14 bits.

Definition at line 237 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_MW_CMDSIZE_15BIT

#define LL_SPI_MW_CMDSIZE_15BIT (14UL << SPI_CTRL0_CTRL_FRAME_SIZE_POS)

CMD length for Microwire transfer: 15 bits.

Definition at line 238 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_MW_CMDSIZE_16BIT

#define LL_SPI_MW_CMDSIZE_16BIT (15UL << SPI_CTRL0_CTRL_FRAME_SIZE_POS)

CMD length for Microwire transfer: 16 bits.

Definition at line 239 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_MW_CMDSIZE_1BIT

#define LL_SPI_MW_CMDSIZE_1BIT 0x00000000UL

CMD length for Microwire transfer: 1 bits.

Definition at line 224 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_MW_CMDSIZE_2BIT

#define LL_SPI_MW_CMDSIZE_2BIT (1UL << SPI_CTRL0_CTRL_FRAME_SIZE_POS)

CMD length for Microwire transfer: 2 bits.

Definition at line 225 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_MW_CMDSIZE_3BIT

#define LL_SPI_MW_CMDSIZE_3BIT (2UL << SPI_CTRL0_CTRL_FRAME_SIZE_POS)

CMD length for Microwire transfer: 3 bits.

Definition at line 226 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_MW_CMDSIZE_4BIT

#define LL_SPI_MW_CMDSIZE_4BIT (3UL << SPI_CTRL0_CTRL_FRAME_SIZE_POS)

CMD length for Microwire transfer: 4 bits.

Definition at line 227 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_MW_CMDSIZE_5BIT

#define LL_SPI_MW_CMDSIZE_5BIT (4UL << SPI_CTRL0_CTRL_FRAME_SIZE_POS)

CMD length for Microwire transfer: 5 bits.

Definition at line 228 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_MW_CMDSIZE_6BIT

#define LL_SPI_MW_CMDSIZE_6BIT (5UL << SPI_CTRL0_CTRL_FRAME_SIZE_POS)

CMD length for Microwire transfer: 6 bits.

Definition at line 229 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_MW_CMDSIZE_7BIT

#define LL_SPI_MW_CMDSIZE_7BIT (6UL << SPI_CTRL0_CTRL_FRAME_SIZE_POS)

CMD length for Microwire transfer: 7 bits.

Definition at line 230 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_MW_CMDSIZE_8BIT

#define LL_SPI_MW_CMDSIZE_8BIT (7UL << SPI_CTRL0_CTRL_FRAME_SIZE_POS)

CMD length for Microwire transfer: 8 bits.

Definition at line 231 of file gr55xx_ll_spi.h.

## ◆ LL_SPI_MW_CMDSIZE_9BIT

#define LL_SPI_MW_CMDSIZE_9BIT (8UL << SPI_CTRL0_CTRL_FRAME_SIZE_POS)

CMD length for Microwire transfer: 9 bits.

Definition at line 232 of file gr55xx_ll_spi.h.