Macros
Test Mode
Peripheral Driver » LL Driver » QSPI » Defines » QSPI Exported Constants
Collaboration diagram for Test Mode:

## Macros
#define | LL_QSPI_NORMAL_MODE 0x00000000UL
| Normal mode for SPI transfer More...
#define | LL_QSPI_TEST_MODE (1UL << QSPI_CTRL0_SRL_Pos)
| Test mode for SPI transfer: Rx and Tx connected inside. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_QSPI_NORMAL_MODE

#define LL_QSPI_NORMAL_MODE 0x00000000UL

Normal mode for SPI transfer

Definition at line 443 of file gr55xx_ll_qspi.h.

## ◆ LL_QSPI_TEST_MODE

#define LL_QSPI_TEST_MODE (1UL << QSPI_CTRL0_SRL_Pos)

Test mode for SPI transfer: Rx and Tx connected inside.

Definition at line 444 of file gr55xx_ll_qspi.h.