Functions
ISO7816 Initialization and de-initialization functions
Peripheral Driver » LL Driver » ISO7816 » Functions
Collaboration diagram for ISO7816 Initialization and de-initialization functions:

## Functions
error_status_t | ll_iso7816_init (iso7816_regs_t *ISO7816x, ll_iso7816_init_t *p_iso7816_init)
| Initialize the ISO7816 registers according to the specified parameters in p_iso7816_init. More...
error_status_t | ll_iso7816_deinit (iso7816_regs_t *ISO7816x)
| De-initialize the ISO7816 registers to their default reset values. More...

## Detailed Description

## Function Documentation

## ◆ ll_iso7816_deinit()

error_status_t ll_iso7816_deinit | ( | iso7816_regs_t * | ISO7816x | ) |

De-initialize the ISO7816 registers to their default reset values.

Parameters

  ISO7816x | ISO7816 instance.

Return values

  An | ErrorStatus enumeration value: SUCCESS: ISO7816 registers are de-initialized ERROR: ISO7816 registers are not de-initialized

## ◆ ll_iso7816_init()

error_status_t ll_iso7816_init | ( | iso7816_regs_t * | ISO7816x,
|  | ll_iso7816_init_t * | p_iso7816_init
| ) |  |

Initialize the ISO7816 registers according to the specified parameters in p_iso7816_init.

Parameters

  ISO7816x | ISO7816 instance.
  p_iso7816_init | pointer to a ll_iso7816_init_t structure.

Return values

  An | ErrorStatus enumeration value: SUCCESS: ISO7816 registers are initialized ERROR: Not applicable