Public Attributes | List of all members
ble_l2cap_evt_conn_req_t Struct Reference
BLE » Logical Link Control and Adaptation Protocol (L2CAP) » Structures

L2cap Connect Request event for BLE_L2CAP_EVT_ENH_CONN_REQ. More...

`#include <ble_l2cap.h>`

## Public Attributes
uint16_t | le_psm
| Le_psm number that should be registered by local device. More...
uint16_t | peer_cid
| It represents the channel endpoint on the device sending the request and receiving the response. More...
uint16_t | peer_mtu
| It indicates the maximum SDU size (in octets) that the L2CAP layer entity sending the LE Credit Based Connection Request can receive on this channel. More...
uint16_t | peer_mps
| It indicates the maximum payload size (in octets) that the L2CAP layer entity sending the LE Credit Based Connection Request is capable of receiving on this channe. More...

## Detailed Description

L2cap Connect Request event for BLE_L2CAP_EVT_ENH_CONN_REQ.

Definition at line 180 of file ble_l2cap.h.

## Member Data Documentation

## ◆ le_psm

uint16_t ble_l2cap_evt_conn_req_t::le_psm

Le_psm number that should be registered by local device.

Definition at line 182 of file ble_l2cap.h.

## ◆ peer_cid

uint16_t ble_l2cap_evt_conn_req_t::peer_cid

It represents the channel endpoint on the device sending the request and receiving the response.

Definition at line 183 of file ble_l2cap.h.

## ◆ peer_mps

uint16_t ble_l2cap_evt_conn_req_t::peer_mps

It indicates the maximum payload size (in octets) that the L2CAP layer entity sending the LE Credit Based Connection Request is capable of receiving on this channe.

Definition at line 186 of file ble_l2cap.h.

## ◆ peer_mtu

uint16_t ble_l2cap_evt_conn_req_t::peer_mtu

It indicates the maximum SDU size (in octets) that the L2CAP layer entity sending the LE Credit Based Connection Request can receive on this channel.

Definition at line 184 of file ble_l2cap.h.

The documentation for this struct was generated from the following file:

- ble_l2cap.h