Macros
Hardware Flow Control
Peripheral Driver » LL Driver » UART » Defines » UART Exported Constants
Collaboration diagram for Hardware Flow Control:

## Macros
#define | LL_UART_HWCONTROL_NONE 0x00000000U
| CTS and RTS hardware flow control disabled. More...
#define | LL_UART_HWCONTROL_RTS_CTS (UART_MCR_AFCE | UART_MCR_RTS)
| CTS and RTS hardware flow control enabled. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_UART_HWCONTROL_NONE

#define LL_UART_HWCONTROL_NONE 0x00000000U

CTS and RTS hardware flow control disabled.

Definition at line 184 of file gr55xx_ll_uart.h.

## ◆ LL_UART_HWCONTROL_RTS_CTS

#define LL_UART_HWCONTROL_RTS_CTS (UART_MCR_AFCE | UART_MCR_RTS)

CTS and RTS hardware flow control enabled.

Definition at line 185 of file gr55xx_ll_uart.h.