Enumerations
Enumerations
Graphics » HAL DC » GDC MIPI
Collaboration diagram for Enumerations:

## Enumerations
enum | hal_gdc_mipi_cmd_t { MIPI_enter_idle_mode = 0x39, MIPI_enter_invert_mode = 0x21, MIPI_enter_normal_mode = 0x13, MIPI_enter_partial_mode = 0x12, MIPI_enter_sleep_mode = 0x10, MIPI_exit_idle_mode = 0x38, MIPI_exit_invert_mode = 0x20, MIPI_exit_sleep_mode = 0x11, MIPI_get_3D_control = 0x3f, MIPI_get_address_mode = 0x0b, MIPI_get_blue_channel = 0x08, MIPI_get_diagnostic_result = 0x0f, MIPI_get_display_mode = 0x0d, MIPI_get_green_channel = 0x07, MIPI_get_pixel_format = 0x0c, MIPI_get_power_mode = 0x0a, MIPI_get_red_channel = 0x06, MIPI_get_scanline = 0x45, MIPI_get_signal_mode = 0x0e, MIPI_nop = 0x00, MIPI_read_DDB_continue = 0xa8, MIPI_read_DDB_start = 0xa1, MIPI_read_memory_continue = 0x3e, MIPI_read_memory_start = 0x2e, MIPI_set_3D_control = 0x3d, MIPI_set_address_mode = 0x36, MIPI_set_column_address = 0x2a, MIPI_set_display_off = 0x28, MIPI_set_display_on = 0x29, MIPI_set_gamma_curve = 0x26, MIPI_set_page_address = 0x2b, MIPI_set_partial_columns = 0x31, MIPI_set_partial_rows = 0x30, MIPI_set_pixel_format = 0x3a, MIPI_set_scroll_area = 0x33, MIPI_set_scroll_start = 0x37, MIPI_set_tear_off = 0x34, MIPI_set_tear_on = 0x35, MIPI_set_tear_scanline = 0x44, MIPI_set_vsync_timing = 0x40, MIPI_soft_reset = 0x01, MIPI_write_LUT = 0x2d, MIPI_write_memory_continue = 0x3c, MIPI_write_memory_start = 0x2c, MIPI_snapshot = 0xff, MIPI_DBIB_STORE_BASE_ADDR = (1 <<31), MIPI_DBIB_CMD = (1U<<30), MIPI_CMD08 = (0U<<28), MIPI_CMD16 = (1U<<28), MIPI_CMD24 = (1U<<29), MIPI_MASK_QSPI = (1U<<27) }
| MIPI Command List definition. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ hal_gdc_mipi_cmd_t

enum hal_gdc_mipi_cmd_t

MIPI Command List definition.

Enumerator
MIPI_enter_idle_mode | Enter idle mode.
MIPI_enter_invert_mode | Enter invert mode.
MIPI_enter_normal_mode | Enter normal mode.
MIPI_enter_partial_mode | Enter partial mode.
MIPI_enter_sleep_mode | Enter sleep mode.
MIPI_exit_idle_mode | Exit idle mode.
MIPI_exit_invert_mode | Exit invert mode.
MIPI_exit_sleep_mode | Exit sleep mode.
MIPI_get_3D_control | Get 3D control.
MIPI_get_address_mode | Get address mode.
MIPI_get_blue_channel | Get blue channel.
MIPI_get_diagnostic_result | Get diagnostic result.
MIPI_get_display_mode | Get display mode.
MIPI_get_green_channel | Get green channel.
MIPI_get_pixel_format | Get pixel format.
MIPI_get_power_mode | Get power mode.
MIPI_get_red_channel | Get red channel.
MIPI_get_scanline | Get scanline.
MIPI_get_signal_mode | Get signal mode.
MIPI_nop | MIPI nop.
MIPI_read_DDB_continue | Read DDB continue.
MIPI_read_DDB_start | Read DDB start.
MIPI_read_memory_continue | Read memory continue.
MIPI_read_memory_start | Read memory start.
MIPI_set_3D_control | Set 3D control.
MIPI_set_address_mode | Set address mode.
MIPI_set_column_address | Set column address.
MIPI_set_display_off | Set display off.
MIPI_set_display_on | Set display on.
MIPI_set_gamma_curve | Set gamma curve.
MIPI_set_page_address | Set page address.
MIPI_set_partial_columns | Set partial columns.
MIPI_set_partial_rows | Set partial rows.
MIPI_set_pixel_format | Set pixel format.
MIPI_set_scroll_area | Set scroll area.
MIPI_set_scroll_start | Set scroll start.
MIPI_set_tear_off | Set tear off.
MIPI_set_tear_on | Set tear on.
MIPI_set_tear_scanline | Set tear scanline.
MIPI_set_vsync_timing | Set vsync timing.
MIPI_soft_reset | Soft reset.
MIPI_write_LUT | Write LUT.
MIPI_write_memory_continue | Write memory continue.
MIPI_write_memory_start | Write memory start.
MIPI_snapshot | snapshot.
MIPI_DBIB_STORE_BASE_ADDR | DBIB store base addr.
MIPI_DBIB_CMD | DBIB CMD.
MIPI_CMD08 | Set cmd width to 8bit.
MIPI_CMD16 | Set cmd width to 16bit.
MIPI_CMD24 | Set cmd width to 24bit.
MIPI_MASK_QSPI | Qspi is forced to single line.

Definition at line 180 of file hal_gdc_mipi.h.