### - p -

- P : _ll_ecc_curve_init
- p_A : _pkc_big_number_add , _pkc_big_number_multi , _pkc_modular_add , _pkc_modular_compare , _pkc_modular_shift , _pkc_modular_sub , _pkc_montgomery_inversion , _pkc_montgomery_multi , _pkc_rsa_modular_exponent
- p_B : _pkc_big_number_add , _pkc_big_number_multi , _pkc_modular_add , _pkc_modular_sub , _pkc_montgomery_multi , _pkc_rsa_modular_exponent
- p_buf : link_node
- p_buffer : _adc_handle , _i2c_handle
- p_channel : ble_hci_rx_channel_t
- p_cmd : ams_c_cmd_list_t
- p_cryp_input_buffer : _aes_handle
- p_cryp_output_buffer : _aes_handle
- p_current_sample_node : adc_env_t
- p_data : ags_evt_t , ams_c_attr_info_t , ams_c_cplt_attr_data_t , cscs_evt_t , dis_c_string_t , gus_c_evt_t , gus_evt_t , hts_evt_t , lms_evt_t , lns_log_data_t , mlmr_c_evt_t , mlmr_evt_t , otas_c_evt_t , otas_evt_t , pcs_evt_t , prf_att_info_t , ras_c_ad_read_ntf_ind_data_t , ras_c_ad_write_req_t , ras_c_write_req_t , rscs_evt_t , samples_evt_t , ths_c_evt_t , ths_evt_t , thscps_setting_t , wechat_data_t
- p_dev_mac : wechat_init_t
- p_digest : _hmac_handle
- p_dma : _adc_handle , _pdm_handle , _qspi_handle
- p_dmarx : _i2c_handle , _i2s_handle , _spi_handle , _uart_handle
- p_dmatx : _dspi_handle , _i2c_handle , _i2s_handle , _spi_handle , _uart_handle
- p_ecc_curve : _ll_pkc_init , pkc_init_t
- p_ecc_point : _pkc_ecc_point_multi
- p_hash : _ll_hmac_init_t
- p_init_vector : _aes_init , _ll_aes_init
- p_instance : _aes_handle , _dma_handle , _dspi_handle , _dual_timer_handle , _efuse_handle , _hmac_handle , _i2c_handle , _i2s_handle , _iso7816_handle_t , _pdm_handle , _pkc_handle , _qspi_handle , _rng_handle , _rtc_handle_t , _spi_handle , _timer_handle , _uart_handle , _usb_handle , _wdt_handle , _xqspi_handle_t , app_dma_params_t , pwm_handle_t
- p_K : _pkc_ecc_point_multi
- p_key : _aes_init , _hmac_init , _ll_aes_init , _ll_hmac_init_t
- p_kout : app_pkc_params_t
- p_list : dis_c_reg_cert_data_list_t , dis_reg_cert_data_list_t
- p_lli : dma_block_config
- p_map : hids_report_map_t
- p_message : _hmac_handle
- p_noti_multiple : ble_gatts_noti_multiple_t
- p_nvds_del : nvds_func_t
- p_nvds_flash_erase : nvds_drv_func_t
- p_nvds_flash_get_info : nvds_drv_func_t
- p_nvds_flash_get_security : nvds_drv_func_t
- p_nvds_flash_read : nvds_drv_func_t
- p_nvds_flash_set_security : nvds_drv_func_t
- p_nvds_flash_write_r : nvds_drv_func_t
- p_nvds_get : nvds_func_t
- p_nvds_init : nvds_func_t
- p_nvds_put : nvds_func_t
- p_nvds_tag_length : nvds_func_t
- p_P : _pkc_handle , _pkc_modular_add , _pkc_modular_compare , _pkc_modular_shift , _pkc_modular_sub , _pkc_montgomery_inversion , _pkc_montgomery_multi , _pkc_rsa_modular_exponent
- p_P_R2 : _pkc_rsa_modular_exponent
- p_parent : _dma_handle
- p_pin_cfg : comp_env_t , dspi_env_t , i2c_env_t , i2s_env_t , iso7816_env_t , pdm_env_t , pwm_env_t , qspi_env_t , spi_env_t , uart_env_t
- p_pnp_id : dis_init_t
- p_read_multiple : ble_gattc_read_multiple_t
- p_result : _pkc_handle , app_pkc_params_t
- p_rx_buffer : _i2s_handle , _qspi_handle , _spi_handle , _uart_handle , _xqspi_handle_t
- p_seed : _aes_init , _ll_aes_init
- p_sram_addr : hw_enum_parm
- p_str : dis_string_t
- p_subevt_data : ras_c_subevt_report_t
- p_sys_id : dis_init_t
- p_tx_buffer : _dspi_handle , _i2s_handle , _qspi_handle , _spi_handle , _uart_handle , _xqspi_handle_t
- p_tx_rx_buffer : _iso7816_handle_t
- p_user_hash : _hmac_init
- p_uuid : ble_gattc_cache_char_t , ble_gattc_cache_desc_t , ble_gattc_cache_include_t , ble_gattc_cache_service_t , ble_gattc_char_t , ble_gattc_desc_t , ble_gattc_disc_char_t , ble_gattc_include_t , ble_gattc_read_by_uuid_t , ble_gattc_service_t
- p_value : ble_gattc_evt_enh_ntf_ind_t , ble_gattc_evt_ntf_ind_t , ble_gattc_read_value_t , ble_gattc_write_attr_value_t , ble_gattc_write_no_resp_t , esls_c_evt_t
- p_xqspi : _exflash_handle
- pa_evt_cnt : ble_gap_connless_iq_report_t , ble_gap_evt_connless_iq_report_t
- package : _efuse_trim0_t
- packets_val : thscps_test_info_t
- packing : iso_create_big_t , iso_set_cig_param_t
- param : ams_c_evt_t , ble_gatts_evt_enh_cccd_rec_t , ble_gatts_evt_enh_multi_ntf_t , ble_gatts_evt_enh_ntf_ind_t , ble_gatts_evt_enh_prep_write_t , ble_gatts_evt_enh_read_t , ble_gatts_evt_enh_write_t , cgms_cp_cmd_req_t , cgms_cp_cmd_rsp_t , thscps_evt_t , wechat_evt_t
- params : ble_gapc_evt_t , ble_gapm_evt_t , ble_gatt_common_evt_t , ble_gattc_evt_t , ble_gatts_evt_t , ble_l2cap_evt_t , ble_sec_evt_t , iso_create_cis_t
- parity : _ll_uart_init_t , _uart_init
- pass_alert_status_cccd_handle : pass_c_handles_t
- pass_alert_status_handle : pass_c_handles_t
- pass_ringer_ctrl_pt_handle : pass_c_handles_t
- pass_ringer_set_cccd_handle : pass_c_handles_t
- pass_ringer_set_handle : pass_c_handles_t
- pass_srvc_end_handle : pass_c_handles_t
- pass_srvc_start_handle : pass_c_handles_t
- path_loss_threshold_reoprt : ble_gapc_evt_t
- patient_high_alert_level : cgms_cp_cmd_req_t , cgms_cp_cmd_rsp_t
- patient_low_alert_level : cgms_cp_cmd_req_t , cgms_cp_cmd_rsp_t
- pattern : _efuse_trim0_t , dfu_image_info_t
- payload_length : ags_ack_packet_t , ags_header_first_ext_t , ags_header_first_t , ags_header_subs_ext_t , ags_header_subs_t
- pdm_dma_blk_callback : _hal_pdm_callback
- pdm_dma_cplt_callback : _hal_pdm_callback
- pdm_dma_error_callback : _hal_pdm_callback
- pdm_env : app_pdm_params_t
- pdm_left_overflow_callback : _hal_pdm_callback
- pdm_msp_deinit : _hal_pdm_callback
- pdm_msp_init : _hal_pdm_callback
- pdm_right_overflow_callback : _hal_pdm_callback
- pdm_state : pdm_env_t
- pdu : thscps_test_conn_info_t
- pedo_target : wechat_evt_t
- peer_add_type : iso_start_target_ann_t
- peer_added_credits : ble_l2cap_evt_add_credits_ind_t
- peer_addr : ble_gap_adv_param_t , ble_gap_evt_connected_t , ble_gap_evt_peer_name_get_t , ble_gap_evt_scan_req_t , ble_gap_ext_adv_param_t , ble_gap_ext_init_param_t , ble_gap_init_param_t , ble_gatts_evt_cccd_rec_t , iso_start_target_ann_t , iso_sync_ann_t
- peer_addr_type : ble_gap_evt_connected_t , iso_sync_ann_t
- peer_cid : ble_l2cap_enh_lecb_cfm_conn_t , ble_l2cap_evt_conn_req_t , ble_l2cap_evt_enh_conn_req_t , ble_l2cap_lecb_cfm_conn_t
- peer_credits : ble_l2cap_evt_conn_ind_t , ble_l2cap_evt_enh_conn_ind_t
- peer_features : ble_gap_peer_info_t
- peer_info : ble_gap_evt_peer_info_t , ble_gapc_evt_t
- peer_irk : ble_gap_ral_dev_info_t
- peer_mps : ble_l2cap_evt_conn_ind_t , ble_l2cap_evt_conn_req_t , ble_l2cap_evt_enh_conn_ind_t , ble_l2cap_evt_enh_conn_req_t , ble_l2cap_evt_enh_reconfig_ind_t
- peer_mtu : ble_l2cap_evt_conn_ind_t , ble_l2cap_evt_conn_req_t , ble_l2cap_evt_enh_conn_ind_t , ble_l2cap_evt_enh_conn_req_t , ble_l2cap_evt_enh_reconfig_ind_t
- peer_name : ble_gapc_evt_t
- peer_version : ble_gap_peer_info_t
- per_adv_idx : iso_create_big_t
- per_sync_idx : ble_gap_evt_adv_report_t , ble_gap_ext_adv_report_ind_t , iso_big_info_report_evt_t , iso_create_big_sync_t
- period : ble_gap_ext_scan_param_t
- period_adv_intv : ble_gap_evt_adv_report_t , ble_gap_ext_adv_report_ind_t
- period_cfg : ble_gap_ext_adv_param_t
- perm : ble_gatts_attm_desc_128_t , ble_gatts_attm_desc_t
- phy : ble_gap_adv_prim_cfg_t , ble_gap_adv_second_cfg_t , ble_gap_conn_info_t , ble_gap_evt_local_tx_pwr_read_ind_t , ble_gap_evt_remote_tx_pwr_read_ind_t , ble_gap_evt_sync_established_t , ble_gap_evt_tx_pwr_change_report_t , ble_gap_local_tx_pwr_read_ind_t , ble_gap_remote_tx_pwr_read_ind_t , ble_gap_sync_established_ind_t , ble_gap_tx_pwr_change_report_t , iso_big_info_report_evt_t , iso_create_big_cmpl_evt_t , iso_create_big_t , thscps_adv_param_t
- phy_delay : app_graphics_ospi_params_t
- phy_m2s : iso_cis_est_evt_t , iso_cis_param_t
- phy_prim : ble_gap_evt_adv_report_t , ble_gap_ext_adv_report_ind_t
- phy_s2m : iso_cis_est_evt_t , iso_cis_param_t
- phy_second : ble_gap_evt_adv_report_t , ble_gap_ext_adv_report_ind_t
- phy_update : ble_gapc_evt_t
- pin : _aon_gpio_init , _gpio_init , _ll_gpio_init , _msio_init , app_adc_pin_t , app_comp_pin_t , app_dspi_pin_t , app_gpiote_param_t , app_i2c_pin_t , app_i2s_pin_t , app_io_evt_t , app_io_init_t , app_iso7816_pin_t , app_pdm_pin_t , app_pwm_pin_t , app_qspi_pin_t , app_spi_pin_t , app_uart_pin_t
- pin_cfg : app_adc_params_t , app_comp_params_t , app_dspi_params_t , app_i2c_params_t , app_i2s_params_t , app_iso7816_params_t , app_pdm_params_t , app_pwm_params_t , app_qspi_params_t , app_spi_params_t , app_uart_params_t
- pins_cfg : app_graphics_dc_params_t
- pkc_done_callback : _hal_pkc_callback
- pkc_env : app_pkc_params_t
- pkc_error_callback : _hal_pkc_callback
- pkc_msp_deinit : _hal_pkc_callback
- pkc_msp_init : _hal_pkc_callback
- pkc_overflow_callback : _hal_pkc_callback
- pkc_state : pkc_env_t
- pkt_seq_num : iso_read_iso_tx_sync_cmpl_evt_t
- pkt_status : ble_gap_conn_iq_report_t , ble_gap_connless_iq_report_t , ble_gap_evt_conn_iq_report_t , ble_gap_evt_connless_iq_report_t
- pll_lock : boot_timing_params_t
- pll_prep : boot_timing_params_t
- pnp_id : ble_dis_c_read_rsp_t
- positive_action : ancs_ntf_flags_t
- post_mode : _ll_rng_init , _rng_init
- power_lvl : ble_gap_dev_adv_tx_power_t
- pre_count : _calendar_handle
- pre_existing : ancs_ntf_flags_t
- prep_wr_req : ble_gatts_evt_t
- prescaler : _dual_timer_init , _ll_dual_timer_init , _ll_pwm_init_t
- prescaler_div : _rtc_init_t
- presence : app_iso7816_pin_cfg_t
- present_mcu_mask : _keyram_mask
- present_xip_mask : _keyram_mask
- previous_action : _iso7816_handle_t
- previous_state : _i2c_handle
- prf_buf : stack_heaps_table_t
- prf_index : ble_gatt_common_evt_prf_reg_t
- prf_reg : ble_gatt_common_evt_t
- prim_cfg : ble_gap_ext_adv_param_t
- prim_srvc_disc : ble_gattc_evt_t
- priority : _dma_init , _ll_dma_init
- priv_mode : ble_gap_ral_dev_info_t
- product_id : __attribute__ , dis_c_pnp_id_t , dis_pnp_id_t
- product_version : dis_c_pnp_id_t , dis_pnp_id_t
- prog_delay : ble_sch_config_t
- prop : ble_gap_ext_adv_param_t , ble_gap_ext_init_param_t , ble_gap_ext_scan_param_t , ble_gattc_browse_attr_char_t , ble_gattc_cache_char_t , ble_gattc_char_t
- PRSquare : _ll_ecc_curve_init
- pto : iso_big_create_sync_est_evt_t , iso_big_info_report_evt_t , iso_create_big_cmpl_evt_t
- pull : _aon_gpio_init , _gpio_init , _ll_gpio_init , _msio_init , app_dspi_pin_t , app_gpiote_param_t , app_graphics_dc_pin_t , app_i2c_pin_t , app_i2s_pin_t , app_io_init_t , app_iso7816_pin_t , app_pdm_pin_t , app_pwm_pin_t , app_qspi_pin_t , app_spi_pin_t , app_uart_pin_t
- pulse_rate : bps_meas_t
- pulse_rate_present : bps_meas_t
- put_cb : esls_nvds_cb_t
- pwm_env : app_pwm_params_t
- pwm_module_state : pwm_env_t
- pwm_msp_deinit : _hal_pwm_callback
- pwm_msp_init : _hal_pwm_callback
- pwm_state : pwm_env_t
- pwr_ble_ths : pwr_table_t
- pwr_delay_hslot : pwr_table_t
- pwr_delay_hus : pwr_table_t
- pwr_dur : pwr_table_t
- pwr_ext : pwr_table_t
- pwr_mgmt_app_timer_thrd : pwr_mgmt_var_box_t
- pwr_mgmt_ble_core_thrd : pwr_mgmt_var_box_t
- pwr_mgmt_rtc_timer_thrd : pwr_mgmt_var_box_t
- pwr_mgmt_wdt_timer_thrd : pwr_mgmt_var_box_t
- pwr_osc : pwr_table_t
- pwr_push_hus : pwr_table_t
- pwr_slp_elapsed_hander : _pwr_handler
- pwr_sw_prep : boot_timing_params_t
- pwr_timer_ths : pwr_table_t