Macros
TX FIFO Threshold
Peripheral Driver » LL Driver » I2C » Defines » I2C Exported Constants
Collaboration diagram for TX FIFO Threshold:

## Macros
#define | LL_I2C_TX_FIFO_TH_EMPTY 0x00000000U
| TX FIFO empty. More...
#define | LL_I2C_TX_FIFO_TH_CHAR_1 0x00000001U
| 1 character in TX FIFO More...
#define | LL_I2C_TX_FIFO_TH_CHAR_2 0x00000002U
| 2 characters in TX FIFO More...
#define | LL_I2C_TX_FIFO_TH_CHAR_3 0x00000003U
| 3 characters in TX FIFO More...
#define | LL_I2C_TX_FIFO_TH_CHAR_4 0x00000004U
| 4 characters in TX FIFO More...
#define | LL_I2C_TX_FIFO_TH_CHAR_5 0x00000005U
| 5 characters in TX FIFO More...
#define | LL_I2C_TX_FIFO_TH_CHAR_6 0x00000006U
| 6 characters in TX FIFO More...
#define | LL_I2C_TX_FIFO_TH_CHAR_7 0x00000007U
| 7 characters in TX FIFO More...
#define | LL_I2C_TX_FIFO_TH_CHAR_8 0x00000008U
| 9 character in TX FIFO More...
#define | LL_I2C_TX_FIFO_TH_CHAR_9 0x00000009U
| 9 characters in TX FIFO More...
#define | LL_I2C_TX_FIFO_TH_CHAR_10 0x0000000AU
| 10 characters in TX FIFO More...
#define | LL_I2C_TX_FIFO_TH_CHAR_11 0x0000000BU
| 11 characters in TX FIFO More...
#define | LL_I2C_TX_FIFO_TH_CHAR_12 0x0000000CU
| 12 characters in TX FIFO More...
#define | LL_I2C_TX_FIFO_TH_CHAR_13 0x0000000DU
| 13 characters in TX FIFO More...
#define | LL_I2C_TX_FIFO_TH_CHAR_14 0x0000000EU
| 14 characters in TX FIFO More...
#define | LL_I2C_TX_FIFO_TH_CHAR_15 0x0000000FU
| 15 character in TX FIFO More...
#define | LL_I2C_TX_FIFO_TH_CHAR_16 0x00000010U
| 16 characters in TX FIFO More...
#define | LL_I2C_TX_FIFO_TH_CHAR_17 0x00000011U
| 17 characters in TX FIFO More...
#define | LL_I2C_TX_FIFO_TH_CHAR_18 0x00000012U
| 18 characters in TX FIFO More...
#define | LL_I2C_TX_FIFO_TH_CHAR_19 0x00000013U
| 19 characters in TX FIFO More...
#define | LL_I2C_TX_FIFO_TH_CHAR_20 0x00000014U
| 20 characters in TX FIFO More...
#define | LL_I2C_TX_FIFO_TH_CHAR_21 0x00000015U
| 21 characters in TX FIFO More...
#define | LL_I2C_TX_FIFO_TH_CHAR_22 0x00000016U
| 22 character in TX FIFO More...
#define | LL_I2C_TX_FIFO_TH_CHAR_23 0x00000017U
| 23 characters in TX FIFO More...
#define | LL_I2C_TX_FIFO_TH_CHAR_24 0x00000018U
| 24 characters in TX FIFO More...
#define | LL_I2C_TX_FIFO_TH_CHAR_25 0x00000019U
| 25 characters in TX FIFO More...
#define | LL_I2C_TX_FIFO_TH_CHAR_26 0x0000001AU
| 26 characters in TX FIFO More...
#define | LL_I2C_TX_FIFO_TH_CHAR_27 0x0000001BU
| 27 characters in TX FIFO More...
#define | LL_I2C_TX_FIFO_TH_CHAR_28 0x0000001CU
| 28 characters in TX FIFO More...
#define | LL_I2C_TX_FIFO_TH_CHAR_29 0x0000001DU
| 29 characters in TX FIFO More...
#define | LL_I2C_TX_FIFO_TH_CHAR_30 0x0000001EU
| 30 characters in TX FIFO More...
#define | LL_I2C_TX_FIFO_TH_CHAR_31 0x0000001FU
| 31 characters in TX FIFO More...
#define | LL_I2C_TX_FIFO_TH_CHAR_32 0x00000020U
| 32 characters in TX FIFO More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_I2C_TX_FIFO_TH_CHAR_1

#define LL_I2C_TX_FIFO_TH_CHAR_1 0x00000001U

1 character in TX FIFO

Definition at line 215 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_CHAR_10

#define LL_I2C_TX_FIFO_TH_CHAR_10 0x0000000AU

10 characters in TX FIFO

Definition at line 224 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_CHAR_11

#define LL_I2C_TX_FIFO_TH_CHAR_11 0x0000000BU

11 characters in TX FIFO

Definition at line 225 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_CHAR_12

#define LL_I2C_TX_FIFO_TH_CHAR_12 0x0000000CU

12 characters in TX FIFO

Definition at line 226 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_CHAR_13

#define LL_I2C_TX_FIFO_TH_CHAR_13 0x0000000DU

13 characters in TX FIFO

Definition at line 227 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_CHAR_14

#define LL_I2C_TX_FIFO_TH_CHAR_14 0x0000000EU

14 characters in TX FIFO

Definition at line 228 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_CHAR_15

#define LL_I2C_TX_FIFO_TH_CHAR_15 0x0000000FU

15 character in TX FIFO

Definition at line 229 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_CHAR_16

#define LL_I2C_TX_FIFO_TH_CHAR_16 0x00000010U

16 characters in TX FIFO

Definition at line 230 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_CHAR_17

#define LL_I2C_TX_FIFO_TH_CHAR_17 0x00000011U

17 characters in TX FIFO

Definition at line 231 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_CHAR_18

#define LL_I2C_TX_FIFO_TH_CHAR_18 0x00000012U

18 characters in TX FIFO

Definition at line 232 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_CHAR_19

#define LL_I2C_TX_FIFO_TH_CHAR_19 0x00000013U

19 characters in TX FIFO

Definition at line 233 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_CHAR_2

#define LL_I2C_TX_FIFO_TH_CHAR_2 0x00000002U

2 characters in TX FIFO

Definition at line 216 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_CHAR_20

#define LL_I2C_TX_FIFO_TH_CHAR_20 0x00000014U

20 characters in TX FIFO

Definition at line 234 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_CHAR_21

#define LL_I2C_TX_FIFO_TH_CHAR_21 0x00000015U

21 characters in TX FIFO

Definition at line 235 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_CHAR_22

#define LL_I2C_TX_FIFO_TH_CHAR_22 0x00000016U

22 character in TX FIFO

Definition at line 236 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_CHAR_23

#define LL_I2C_TX_FIFO_TH_CHAR_23 0x00000017U

23 characters in TX FIFO

Definition at line 237 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_CHAR_24

#define LL_I2C_TX_FIFO_TH_CHAR_24 0x00000018U

24 characters in TX FIFO

Definition at line 238 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_CHAR_25

#define LL_I2C_TX_FIFO_TH_CHAR_25 0x00000019U

25 characters in TX FIFO

Definition at line 239 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_CHAR_26

#define LL_I2C_TX_FIFO_TH_CHAR_26 0x0000001AU

26 characters in TX FIFO

Definition at line 240 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_CHAR_27

#define LL_I2C_TX_FIFO_TH_CHAR_27 0x0000001BU

27 characters in TX FIFO

Definition at line 241 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_CHAR_28

#define LL_I2C_TX_FIFO_TH_CHAR_28 0x0000001CU

28 characters in TX FIFO

Definition at line 242 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_CHAR_29

#define LL_I2C_TX_FIFO_TH_CHAR_29 0x0000001DU

29 characters in TX FIFO

Definition at line 243 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_CHAR_3

#define LL_I2C_TX_FIFO_TH_CHAR_3 0x00000003U

3 characters in TX FIFO

Definition at line 217 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_CHAR_30

#define LL_I2C_TX_FIFO_TH_CHAR_30 0x0000001EU

30 characters in TX FIFO

Definition at line 244 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_CHAR_31

#define LL_I2C_TX_FIFO_TH_CHAR_31 0x0000001FU

31 characters in TX FIFO

Definition at line 245 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_CHAR_32

#define LL_I2C_TX_FIFO_TH_CHAR_32 0x00000020U

32 characters in TX FIFO

Definition at line 246 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_CHAR_4

#define LL_I2C_TX_FIFO_TH_CHAR_4 0x00000004U

4 characters in TX FIFO

Definition at line 218 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_CHAR_5

#define LL_I2C_TX_FIFO_TH_CHAR_5 0x00000005U

5 characters in TX FIFO

Definition at line 219 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_CHAR_6

#define LL_I2C_TX_FIFO_TH_CHAR_6 0x00000006U

6 characters in TX FIFO

Definition at line 220 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_CHAR_7

#define LL_I2C_TX_FIFO_TH_CHAR_7 0x00000007U

7 characters in TX FIFO

Definition at line 221 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_CHAR_8

#define LL_I2C_TX_FIFO_TH_CHAR_8 0x00000008U

9 character in TX FIFO

Definition at line 222 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_CHAR_9

#define LL_I2C_TX_FIFO_TH_CHAR_9 0x00000009U

9 characters in TX FIFO

Definition at line 223 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_TX_FIFO_TH_EMPTY

#define LL_I2C_TX_FIFO_TH_EMPTY 0x00000000U

TX FIFO empty.

Definition at line 214 of file gr55xx_ll_i2c.h.