Public Attributes | List of all members
ble_gap_bdaddr_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Structures

The struct of broadcast address with broadcast type. More...

`#include <ble_gapc.h>`

Collaboration diagram for ble_gap_bdaddr_t:
[legend]

## Public Attributes
ble_gap_addr_t | gap_addr
| Device BD Address. More...
uint8_t | addr_type
| Address type of the device: 0=public/1=random. More...

## Detailed Description

The struct of broadcast address with broadcast type.

Definition at line 276 of file ble_gapc.h.

## Member Data Documentation

## ◆ addr_type

uint8_t ble_gap_bdaddr_t::addr_type

Address type of the device: 0=public/1=random.

please ble_gap_addr_type_t.

Definition at line 279 of file ble_gapc.h.

## ◆ gap_addr

ble_gap_addr_t ble_gap_bdaddr_t::gap_addr

Device BD Address.

Definition at line 278 of file ble_gapc.h.

The documentation for this struct was generated from the following file:

- ble_gapc.h