Here is a list of all file members with links to the files they belong to:

### - g -

- g_devices_renew : gr55xx_hal_pwr_mgmt.h
- g_devices_sleep : gr55xx_hal_pwr_mgmt.h
- g_devices_state : gr55xx_hal_pwr_mgmt.h
- g_extra_devices_renew : gr55xx_hal_pwr_mgmt.h
- g_extra_devices_state : gr55xx_hal_pwr_mgmt.h
- gap_per_adv_sync_info_rec_mode : ble_gapm.h
- GAP_PHY_ANY : ble_gapc.h
- GAP_PHY_LE_1MBPS : ble_gapc.h
- GAP_PHY_LE_2MBPS : ble_gapc.h
- GAP_PHY_LE_CODED : ble_gapc.h
- gap_sec_lvl_type : ble_gapm.h
- gap_slot_dur_type : ble_gapm.h
- gap_switch_sampling_rate : ble_gapm.h
- gap_sync_cte_type : ble_gapm.h
- gatt_serv_type_t : ble_gattc.h
- gattc_cache_attr_t : ble_gattc_cache.h
- GDC_ACCESS_TYPE_ASYNC : app_graphics_dc.h
- GDC_ACCESS_TYPE_SYNC : app_graphics_dc.h
- GDC_CLOCK_FREQ_12MHz : app_graphics_dc.h
- GDC_CLOCK_FREQ_24MHz : app_graphics_dc.h
- GDC_CLOCK_FREQ_3MHz : app_graphics_dc.h
- GDC_CLOCK_FREQ_48MHz : app_graphics_dc.h
- GDC_CLOCK_FREQ_6MHz : app_graphics_dc.h
- GDC_CLOCK_MODE_0 : app_graphics_dc.h
- GDC_CLOCK_MODE_1 : app_graphics_dc.h
- GDC_CLOCK_MODE_2 : app_graphics_dc.h
- GDC_CLOCK_MODE_3 : app_graphics_dc.h
- GDC_DATA_FORMAT_ABGR8888 : app_graphics_dc.h
- GDC_DATA_FORMAT_ARGB8888 : app_graphics_dc.h
- GDC_DATA_FORMAT_BGRA8888 : app_graphics_dc.h
- GDC_DATA_FORMAT_RGB24 : app_graphics_dc.h
- GDC_DATA_FORMAT_RGB565 : app_graphics_dc.h
- GDC_DATA_FORMAT_RGBA8888 : app_graphics_dc.h
- GDC_DATA_FORMAT_TSC4 : app_graphics_dc.h
- GDC_DATA_FORMAT_TSC6 : app_graphics_dc.h
- GDC_DATA_FORMAT_TSC6A : app_graphics_dc.h
- GDC_DSPI_FRAME_TIMING_0 : app_graphics_dc.h
- GDC_FRAME_ADDRESS_WIDTH_08BIT : app_graphics_dc.h
- GDC_FRAME_ADDRESS_WIDTH_16BIT : app_graphics_dc.h
- GDC_FRAME_ADDRESS_WIDTH_24BIT : app_graphics_dc.h
- GDC_FRAME_ADDRESS_WIDTH_NONE : app_graphics_dc.h
- GDC_FRAME_RES_ASYNC_WAIT : app_graphics_dc.h
- GDC_FRAME_RES_FAIL : app_graphics_dc.h
- GDC_FRAME_RES_SUCCESS : app_graphics_dc.h
- GDC_FRAME_RES_UNSUPPORT : app_graphics_dc.h
- GDC_IRQ_EVT_CMD_TRANSMITION_END : app_graphics_dc.h
- GDC_IRQ_EVT_FRAME_TRANSMITION_END : app_graphics_dc.h
- GDC_MIPICFG_DSPI_RGB565_OPT0 : app_graphics_dc.h
- GDC_MIPICFG_DSPI_RGB888_OPT0 : app_graphics_dc.h
- GDC_MIPICFG_DSPI_RGB888_OPT1 : app_graphics_dc.h
- GDC_MIPICFG_QSPI_RGB565_OPT0 : app_graphics_dc.h
- GDC_MIPICFG_QSPI_RGB888_OPT0 : app_graphics_dc.h
- GDC_MIPICFG_SPI_RGB565_OPT0 : app_graphics_dc.h
- GDC_MIPICFG_SPI_RGB888_OPT0 : app_graphics_dc.h
- GDC_MODE_DSPI : app_graphics_dc.h
- GDC_MODE_QSPI : app_graphics_dc.h
- GDC_MODE_SPI : app_graphics_dc.h
- GDC_ONE_LAYER_MODE : app_graphics_dc.h
- GDC_OUT_PIXEL_BITS_16 : app_graphics_dc.h
- GDC_OUT_PIXEL_BITS_24 : app_graphics_dc.h
- GDC_OUT_PIXEL_BITS_NOT_SUPPORT : app_graphics_dc.h
- GDC_POWER_STATE_ACTIVE : app_graphics_dc.h
- GDC_POWER_STATE_SLEEP : app_graphics_dc.h
- GDC_QSPI_FRAME_TIMING_0 : app_graphics_dc.h
- GDC_QSPI_FRAME_TIMING_1 : app_graphics_dc.h
- GDC_SPI_FRAME_TIMING_0 : app_graphics_dc.h
- GDC_TCSU_CYCLE_0 : app_graphics_dc.h
- GDC_TCSU_CYCLE_1 : app_graphics_dc.h
- GDC_TCSU_CYCLE_2 : app_graphics_dc.h
- GDC_TCSU_CYCLE_3 : app_graphics_dc.h
- GDC_TCSU_CYCLE_4 : app_graphics_dc.h
- GDC_TWO_LAYER_MODE : app_graphics_dc.h
- gdx_lcp_channel_get() : ble_lcp.h
- gdx_lcp_channel_set() : ble_lcp.h
- gdx_lcp_data_tx() : ble_lcp.h
- gdx_lcp_deinit() : ble_lcp.h
- gdx_lcp_init() : ble_lcp.h
- gdx_lcp_rx_start() : ble_lcp.h
- gdx_lcp_rx_stop() : ble_lcp.h
- gdx_lcp_tx_power_get() : ble_lcp.h
- gdx_lcp_tx_power_set() : ble_lcp.h
- GGPU_IRQ_EVT_CMD_LIST_END : app_graphics_gpu.h
- GGPU_IRQ_EVT_DRAW_CMD_END : app_graphics_gpu.h
- GGPU_IRQ_EVT_IRQ_ID_CLEAR : app_graphics_gpu.h
- GGPU_IRQ_EVT_OTHER : app_graphics_gpu.h
- GLOBAL_EXCEPTION_DISABLE : gr55xx_hal.h
- GLOBAL_EXCEPTION_ENABLE : gr55xx_hal.h
- GLOBAL_INT_DISABLE : gr55xx_hal.h
- GLOBAL_INT_RESTORE : gr55xx_hal.h
- GPIO_ALTFUNCCLR_ADDR : gr55xx_ll_gpio.h
- GPIO_ALTFUNCSET_ADDR : gr55xx_ll_gpio.h
- GPIO_DATA_ADDR : gr55xx_ll_gpio.h
- GPIO_DATAOUT_ADDR : gr55xx_ll_gpio.h
- GPIO_DEFAULT_CONFIG : gr55xx_hal_gpio.h
- gpio_init_t : gr55xx_hal_gpio.h
- GPIO_INTDBECLR_ADDR : gr55xx_ll_gpio.h
- GPIO_INTDBESET_ADDR : gr55xx_ll_gpio.h
- GPIO_INTENCLR_ADDR : gr55xx_ll_gpio.h
- GPIO_INTENSET_ADDR : gr55xx_ll_gpio.h
- GPIO_INTPOLCLR_ADDR : gr55xx_ll_gpio.h
- GPIO_INTPOLSET_ADDR : gr55xx_ll_gpio.h
- GPIO_INTSTAT_ADDR : gr55xx_ll_gpio.h
- GPIO_INTTYPECLR_ADDR : gr55xx_ll_gpio.h
- GPIO_INTTYPESET_ADDR : gr55xx_ll_gpio.h
- GPIO_MODE_INPUT : gr55xx_hal_gpio.h
- GPIO_MODE_IT_BOTH_EDGE : gr55xx_hal_gpio.h
- GPIO_MODE_IT_FALLING : gr55xx_hal_gpio.h
- GPIO_MODE_IT_HIGH : gr55xx_hal_gpio.h
- GPIO_MODE_IT_LOW : gr55xx_hal_gpio.h
- GPIO_MODE_IT_RISING : gr55xx_hal_gpio.h
- GPIO_MODE_MUX : gr55xx_hal_gpio.h
- GPIO_MODE_OUTPUT : gr55xx_hal_gpio.h
- GPIO_MUX_0 : gr55xx_hal_gpio_ex.h
- GPIO_MUX_1 : gr55xx_hal_gpio_ex.h
- GPIO_MUX_2 : gr55xx_hal_gpio_ex.h
- GPIO_MUX_3 : gr55xx_hal_gpio_ex.h
- GPIO_MUX_4 : gr55xx_hal_gpio_ex.h
- GPIO_MUX_5 : gr55xx_hal_gpio_ex.h
- GPIO_MUX_6 : gr55xx_hal_gpio_ex.h
- GPIO_MUX_7 : gr55xx_hal_gpio_ex.h
- GPIO_MUX_8 : gr55xx_hal_gpio_ex.h
- GPIO_NOPULL : gr55xx_hal_gpio.h
- GPIO_OUTENCLR_ADDR : gr55xx_ll_gpio.h
- GPIO_OUTENSET_ADDR : gr55xx_ll_gpio.h
- GPIO_PIN_0 : gr55xx_hal_gpio.h
- GPIO_PIN_1 : gr55xx_hal_gpio.h
- GPIO_PIN_10 : gr55xx_hal_gpio.h
- GPIO_PIN_11 : gr55xx_hal_gpio.h
- GPIO_PIN_12 : gr55xx_hal_gpio.h
- GPIO_PIN_13 : gr55xx_hal_gpio.h
- GPIO_PIN_14 : gr55xx_hal_gpio.h
- GPIO_PIN_15 : gr55xx_hal_gpio.h
- GPIO_PIN_2 : gr55xx_hal_gpio.h
- GPIO_PIN_3 : gr55xx_hal_gpio.h
- GPIO_PIN_4 : gr55xx_hal_gpio.h
- GPIO_PIN_5 : gr55xx_hal_gpio.h
- GPIO_PIN_6 : gr55xx_hal_gpio.h
- GPIO_PIN_7 : gr55xx_hal_gpio.h
- GPIO_PIN_8 : gr55xx_hal_gpio.h
- GPIO_PIN_9 : gr55xx_hal_gpio.h
- GPIO_PIN_ALL : gr55xx_hal_gpio.h
- GPIO_PIN_MASK : gr55xx_hal_gpio.h
- GPIO_PIN_RESET : gr55xx_hal_gpio.h
- GPIO_PIN_SET : gr55xx_hal_gpio.h
- gpio_pin_state_t : gr55xx_hal_gpio.h
- GPIO_PULLDOWN : gr55xx_hal_gpio.h
- GPIO_PULLUP : gr55xx_hal_gpio.h
- GPU_POWER_STATE_ACTIVE : app_graphics_gpu.h
- GPU_POWER_STATE_SLEEP : app_graphics_gpu.h
- gr_assert_param : gr55xx_hal_conf.h
- graphics_dc_am139_qspi_lcd_init() : graphics_dc_lcd_drv.h
- graphics_dc_am139_qspi_lcd_set_show_area() : graphics_dc_lcd_drv.h
- graphics_dc_am139_qspi_send_frame() : graphics_dc_lcd_drv.h
- GRAPHICS_DC_BASEADDR : app_graphics_dc.h
- GRAPHICS_DC_CLK_PIN : app_graphics_dc.h
- GRAPHICS_DC_CLK_PIN_MUX : app_graphics_dc.h
- GRAPHICS_DC_CLK_PORT : app_graphics_dc.h
- graphics_dc_clock_freq_e : app_graphics_dc.h
- graphics_dc_clock_mode_e : app_graphics_dc.h
- GRAPHICS_DC_CSN_PIN : app_graphics_dc.h
- GRAPHICS_DC_CSN_PIN_MUX : app_graphics_dc.h
- GRAPHICS_DC_CSN_PORT : app_graphics_dc.h
- graphics_dc_data_format_e : app_graphics_dc.h
- GRAPHICS_DC_DCX_PIN : app_graphics_dc.h
- GRAPHICS_DC_DCX_PIN_MUX : app_graphics_dc.h
- GRAPHICS_DC_DCX_PORT : app_graphics_dc.h
- graphics_dc_deinit() : app_graphics_dc.h
- graphics_dc_init() : app_graphics_dc.h
- GRAPHICS_DC_IO0_PIN : app_graphics_dc.h
- GRAPHICS_DC_IO0_PIN_MUX : app_graphics_dc.h
- GRAPHICS_DC_IO0_PORT : app_graphics_dc.h
- GRAPHICS_DC_IO1_PIN : app_graphics_dc.h
- GRAPHICS_DC_IO1_PIN_MUX : app_graphics_dc.h
- GRAPHICS_DC_IO1_PORT : app_graphics_dc.h
- GRAPHICS_DC_IO2_PIN : app_graphics_dc.h
- GRAPHICS_DC_IO2_PIN_MUX : app_graphics_dc.h
- GRAPHICS_DC_IO2_PORT : app_graphics_dc.h
- GRAPHICS_DC_IO3_PIN : app_graphics_dc.h
- GRAPHICS_DC_IO3_PIN_MUX : app_graphics_dc.h
- GRAPHICS_DC_IO3_PORT : app_graphics_dc.h
- graphics_dc_irq_event_notify_cb : app_graphics_dc.h
- GRAPHICS_DC_LAYER_0 : app_graphics_dc.h
- GRAPHICS_DC_LAYER_1 : app_graphics_dc.h
- graphics_dc_layer_mode_e : app_graphics_dc.h
- graphics_dc_mipi_format_e : app_graphics_dc.h
- graphics_dc_mspi_e : app_graphics_dc.h
- graphics_dc_out_pixel_bits_e : app_graphics_dc.h
- graphics_dc_pins_reinit() : app_graphics_dc.h
- graphics_dc_power_state_e : app_graphics_dc.h
- graphics_dc_rm69330_qspi_lcd_init() : graphics_dc_lcd_drv.h
- graphics_dc_rm69330_qspi_lcd_set_show_area() : graphics_dc_lcd_drv.h
- graphics_dc_rm69330_qspi_lcd_test() : graphics_dc_lcd_drv.h
- graphics_dc_rm69330_qspi_send_frame() : graphics_dc_lcd_drv.h
- graphics_dc_rm69330_spi_lcd_init() : graphics_dc_lcd_drv.h
- graphics_dc_rm69330_spi_lcd_set_show_area() : graphics_dc_lcd_drv.h
- graphics_dc_set_refresh_area_cb : app_graphics_dc.h
- graphics_dc_st7789_dspi_lcd_init() : graphics_dc_lcd_drv.h
- graphics_dc_st7789_dspi_lcd_set_show_area() : graphics_dc_lcd_drv.h
- graphics_dc_tcsu_cycle_e : app_graphics_dc.h
- GRAPHICS_GPU_BASEADDR : app_graphics_gpu.h
- graphics_gpu_deinit() : app_graphics_gpu.h
- graphics_gpu_init() : app_graphics_gpu.h
- graphics_gpu_irq_event_notify : app_graphics_gpu.h
- graphics_gpu_power_state_e : app_graphics_gpu.h
- GRP_ID_MSK : esls.h
- GUS_C_CONNECTION_MAX : gus_c.h
- gus_c_disc_srvc_start() : gus_c.h
- GUS_C_EVT_DISCOVERY_COMPLETE : gus_c.h
- GUS_C_EVT_DISCOVERY_FAIL : gus_c.h
- GUS_C_EVT_FLOW_CTRL_NTF_SET_SUCCESS : gus_c.h
- gus_c_evt_handler_t : gus_c.h
- GUS_C_EVT_INVALID : gus_c.h
- GUS_C_EVT_PEER_DATA_RECEIVE : gus_c.h
- GUS_C_EVT_RX_FLOW_UPDATE_CPLT : gus_c.h
- GUS_C_EVT_TX_CPLT : gus_c.h
- GUS_C_EVT_TX_FLOW_OFF : gus_c.h
- GUS_C_EVT_TX_FLOW_ON : gus_c.h
- GUS_C_EVT_TX_NTF_SET_SUCCESS : gus_c.h
- gus_c_evt_type_t : gus_c.h
- GUS_C_EVT_WRITE_OP_ERR : gus_c.h
- gus_c_flow_ctrl_notify_set() : gus_c.h
- gus_c_flow_ctrl_state : gus_c.h
- GUS_C_FLOW_CTRL_STATE_OFF : gus_c.h
- GUS_C_FLOW_CTRL_STATE_ON : gus_c.h
- gus_c_flow_ctrl_state_t : gus_c.h
- gus_c_rx_flow_ctrl_set() : gus_c.h
- gus_c_tx_data_send() : gus_c.h
- gus_c_tx_notify_set() : gus_c.h
- gus_client_init() : gus_c.h
- GUS_CONNECTION_MAX : gus.h
- GUS_EVT_FLOW_CTRL_DISABLE : gus.h
- GUS_EVT_FLOW_CTRL_ENABLE : gus.h
- gus_evt_handler_t : gus.h
- GUS_EVT_INVALID : gus.h
- GUS_EVT_RX_DATA_RECEIVED : gus.h
- GUS_EVT_TX_DATA_SENT : gus.h
- GUS_EVT_TX_FLOW_OFF : gus.h
- GUS_EVT_TX_FLOW_ON : gus.h
- GUS_EVT_TX_PORT_CLOSED : gus.h
- GUS_EVT_TX_PORT_OPENED : gus.h
- gus_evt_type_t : gus.h
- GUS_FLOW_CTRL_LEN : gus.h
- gus_flow_ctrl_state : gus.h
- GUS_FLOW_CTRL_STATE_OFF : gus.h
- GUS_FLOW_CTRL_STATE_ON : gus.h
- gus_flow_ctrl_state_t : gus.h
- GUS_FLOW_CTRL_UUID : gus_c.h
- GUS_MAX_DATA_LEN : gus.h
- GUS_RX_CHAR_UUID : gus_c.h
- gus_rx_flow_ctrl_set() : gus.h
- gus_service_init() : gus.h
- gus_service_start_handle_get() : gus.h
- GUS_SERVICE_UUID : gus.h
- GUS_SVC_UUID : gus_c.h
- GUS_TX_CHAR_UUID : gus_c.h
- gus_tx_data_send() : gus.h