Public Attributes | List of all members
ble_gap_set_conn_cte_trans_param_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Structures

Set connection CTE transmit parameters info. More...

`#include <ble_gapc.h>`

## Public Attributes
uint8_t | cte_type
| The type of cte, see ble_gap_cte_type_t. More...
uint8_t | num_antenna
| The number of Antenna IDs in the pattern, range 0x02 to 0x4B. More...
uint8_t * | antenna_id
| List of Antenna IDs in the pattern. More...

## Detailed Description

Set connection CTE transmit parameters info.

Definition at line 543 of file ble_gapc.h.

## Member Data Documentation

## ◆ antenna_id

uint8_t* ble_gap_set_conn_cte_trans_param_t::antenna_id

List of Antenna IDs in the pattern.

Definition at line 547 of file ble_gapc.h.

## ◆ cte_type

uint8_t ble_gap_set_conn_cte_trans_param_t::cte_type

The type of cte, see ble_gap_cte_type_t.

Definition at line 545 of file ble_gapc.h.

## ◆ num_antenna

uint8_t ble_gap_set_conn_cte_trans_param_t::num_antenna

The number of Antenna IDs in the pattern, range 0x02 to 0x4B.

Definition at line 546 of file ble_gapc.h.

The documentation for this struct was generated from the following file:

- ble_gapc.h