Classes | Macros | Typedefs | Functions
gr55xx_ll_dma.h File Reference

Header file containing functions prototypes of DMA LL library. More...

`#include "gr55xx.h"`
Include dependency graph for gr55xx_ll_dma.h:
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Classes
struct | _ll_dma_init
| LL DMA init Structure definition. More...

## Macros
#define | LL_DMA_CHANNEL_0 ((uint32_t)0x00000000U)
| DMA Channel 0. More...
#define | LL_DMA_CHANNEL_1 ((uint32_t)0x00000001U)
| DMA Channel 1. More...
#define | LL_DMA_CHANNEL_2 ((uint32_t)0x00000002U)
| DMA Channel 2. More...
#define | LL_DMA_CHANNEL_3 ((uint32_t)0x00000003U)
| DMA Channel 3. More...
#define | LL_DMA_CHANNEL_4 ((uint32_t)0x00000004U)
| DMA Channel 4. More...
#define | LL_DMA_CHANNEL_5 ((uint32_t)0x00000005U)
| DMA Channel 5. More...
#define | LL_DMA_CHANNEL_6 ((uint32_t)0x00000006U)
| DMA Channel 6. More...
#define | LL_DMA_CHANNEL_7 ((uint32_t)0x00000007U)
| DMA Channel 7. More...
#define | LL_DMA_CHANNEL_ALL ((uint32_t)0xFFFF0000U)
| DMA Channel all (used only for function ll_dma_deinit(). More...
#define | LL_DMA_DIRECTION_MEMORY_TO_MEMORY DMA_CTLL_TT_FC_M2M
| Memory to memory direction More...
#define | LL_DMA_DIRECTION_MEMORY_TO_PERIPH DMA_CTLL_TT_FC_M2P
| Memory to peripheral direction. More...
#define | LL_DMA_DIRECTION_PERIPH_TO_MEMORY DMA_CTLL_TT_FC_P2M
| Peripheral to memory direction. More...
#define | LL_DMA_DIRECTION_PERIPH_TO_PERIPH DMA_CTLL_TT_FC_P2P
| Peripheral to Peripheral direction. More...
#define | LL_DMA_MODE_SINGLE_BLOCK ((uint32_t)0x00000000U)
| Single block. More...
#define | LL_DMA_MODE_MULTI_BLOCK_SRC_RELOAD DMA_CFGL_RELOAD_SRC
| Multi-block: src address reload, dst address contiguous. More...
#define | LL_DMA_MODE_MULTI_BLOCK_DST_RELOAD DMA_CFGL_RELOAD_DST
| Multi-block: src address contiguous, dst address reload. More...
#define | LL_DMA_MODE_MULTI_BLOCK_ALL_RELOAD (DMA_CFGL_RELOAD_SRC | DMA_CFGL_RELOAD_DST)
| Multi-block: src address reload, dst address reload. More...
#define | LL_DMA_LLP_DST_ENABLE DMA_CTLL_LLP_DST_EN_ENABLE
| Destination LLP Enable. More...
#define | LL_DMA_LLP_DST_DISABLE DMA_CTLL_LLP_DST_EN_DISABLE
| Destination LLP Disable. More...
#define | LL_DMA_LLP_SRC_ENABLE DMA_CTLL_LLP_SRC_EN_ENABLE
| Source LLP Enable. More...
#define | LL_DMA_LLP_SRC_DISABLE DMA_CTLL_LLP_SRC_EN_DISABLE
| Source LLP Disable. More...
#define | LL_DMA_SRC_STAT_UPDATE_ENABLE DMA_CFGH_SS_UPD_ENABLE
| Destination Status Update Enable. More...
#define | LL_DMA_SRC_STAT_UPDATE_DISABLE DMA_CFGH_SS_UPD_DISABLE
| Destination Status Update Enable. More...
#define | LL_DMA_DST_STAT_UPDATE_ENABLE DMA_CFGH_DS_UPD_ENABLE
| Source Status Update Enable. More...
#define | LL_DMA_DST_STAT_UPDATE_DISABLE DMA_CFGH_DS_UPD_DISABLE
| Source Status Update Enable. More...
#define | LL_DMA_DST_SCATTER_ENABLE DMA_CTLL_DST_SCATTER_EN_ENABLE
| Destination Scatter Enable. More...
#define | LL_DMA_DST_SCATTER_DISABLE DMA_CTLL_DST_SCATTER_EN_DISABLE
| Destination Scatter Disable. More...
#define | LL_DMA_SRC_GATHER_ENABLE DMA_CTLL_SRC_GATHER_EN_ENABLE
| Source Gather Enable. More...
#define | LL_DMA_SRC_GATHER_DISABLE DMA_CTLL_SRC_GATHER_EN_DISABLE
| Source Gather Disable. More...
#define | LL_DMA_SRC_INCREMENT DMA_CTLL_SINC_INC
| Source Address increment. More...
#define | LL_DMA_SRC_DECREMENT DMA_CTLL_SINC_DEC
| Source Address decrement. More...
#define | LL_DMA_SRC_NO_CHANGE DMA_CTLL_SINC_NO
| Source Address no change. More...
#define | LL_DMA_DST_INCREMENT DMA_CTLL_DINC_INC
| Destination Address increment. More...
#define | LL_DMA_DST_DECREMENT DMA_CTLL_DINC_DEC
| Destination Address decrement. More...
#define | LL_DMA_DST_NO_CHANGE DMA_CTLL_DINC_NO
| Destination Address no change. More...
#define | LL_DMA_SRC_BURST_LENGTH_1 DMA_CTLL_SRC_MSIZE_1
| Source Burst length: 1 word. More...
#define | LL_DMA_SRC_BURST_LENGTH_4 DMA_CTLL_SRC_MSIZE_4
| Source Burst length: 4 words. More...
#define | LL_DMA_SRC_BURST_LENGTH_8 DMA_CTLL_SRC_MSIZE_8
| Source Burst length: 8 words. More...
#define | LL_DMA_SRC_BURST_LENGTH_16 DMA_CTLL_SRC_MSIZE_16
| Source Burst length: 16 words. More...
#define | LL_DMA_SRC_BURST_LENGTH_32 DMA_CTLL_SRC_MSIZE_32
| Source Burst length: 32 words. More...
#define | LL_DMA_SRC_BURST_LENGTH_64 DMA_CTLL_SRC_MSIZE_64
| Source Burst length: 64 words. More...
#define | LL_DMA_DST_BURST_LENGTH_1 DMA_CTLL_DST_MSIZE_1
| Destination Burst length: 1 word. More...
#define | LL_DMA_DST_BURST_LENGTH_4 DMA_CTLL_DST_MSIZE_4
| Destination Burst length: 4 words. More...
#define | LL_DMA_DST_BURST_LENGTH_8 DMA_CTLL_DST_MSIZE_8
| Destination Burst length: 8 words. More...
#define | LL_DMA_DST_BURST_LENGTH_16 DMA_CTLL_DST_MSIZE_16
| Destination Burst length: 16 words. More...
#define | LL_DMA_DST_BURST_LENGTH_32 DMA_CTLL_DST_MSIZE_32
| Destination Burst length: 32 words. More...
#define | LL_DMA_DST_BURST_LENGTH_64 DMA_CTLL_DST_MSIZE_64
| Destination Burst length: 64 words. More...
#define | LL_DMA_SDATAALIGN_BYTE DMA_CTLL_SRC_TR_WIDTH_8
| Source data alignment : Byte More...
#define | LL_DMA_SDATAALIGN_HALFWORD DMA_CTLL_SRC_TR_WIDTH_16
| Source data alignment : HalfWord. More...
#define | LL_DMA_SDATAALIGN_WORD DMA_CTLL_SRC_TR_WIDTH_32
| Source data alignment : Word More...
#define | LL_DMA_DDATAALIGN_BYTE DMA_CTLL_DST_TR_WIDTH_8
| Destination data alignment : Byte More...
#define | LL_DMA_DDATAALIGN_HALFWORD DMA_CTLL_DST_TR_WIDTH_16
| Destination data alignment : HalfWord. More...
#define | LL_DMA_DDATAALIGN_WORD DMA_CTLL_DST_TR_WIDTH_32
| Destination data alignment : Word More...
#define | LL_DMA_PRIORITY_0 DMA_CFGL_CH_PRIOR_0
| Priority level : 0. More...
#define | LL_DMA_PRIORITY_1 DMA_CFGL_CH_PRIOR_1
| Priority level : 1. More...
#define | LL_DMA_PRIORITY_2 DMA_CFGL_CH_PRIOR_2
| Priority level : 2. More...
#define | LL_DMA_PRIORITY_3 DMA_CFGL_CH_PRIOR_3
| Priority level : 3. More...
#define | LL_DMA_PRIORITY_4 DMA_CFGL_CH_PRIOR_4
| Priority level : 4. More...
#define | LL_DMA_PRIORITY_5 DMA_CFGL_CH_PRIOR_5
| Priority level : 5. More...
#define | LL_DMA_PRIORITY_6 DMA_CFGL_CH_PRIOR_6
| Priority level : 6. More...
#define | LL_DMA_PRIORITY_7 DMA_CFGL_CH_PRIOR_7
| Priority level : 7. More...
#define | LL_DMA_SHANDSHAKING_HW ((uint32_t)0x00000000U)
| Source: hardware handshake. More...
#define | LL_DMA_SHANDSHAKING_SW DMA_CFGL_HS_SEL_SRC
| Source: software handshake. More...
#define | LL_DMA_DHANDSHAKING_HW ((uint32_t)0x00000000U)
| Destination: hardware handshake. More...
#define | LL_DMA_DHANDSHAKING_SW DMA_CFGL_HS_SEL_DST
| Destination: software handshake. More...
#define | LL_DMA0_PERIPH_MEM ((uint32_t)0x0000000BU)
| DMA peripheral type is Memory. More...
#define | LL_DMA0_PERIPH_QSPI0_TX ((uint32_t)0x00000000U)
| DMA Peripheral type is QSPIM0 TX. More...
#define | LL_DMA0_PERIPH_QSPI0_RX ((uint32_t)0x00000001U)
| DMA Peripheral type is QSPIM0 RX. More...
#define | LL_DMA0_PERIPH_SPIM_TX ((uint32_t)0x00000002U)
| DMA Peripheral type is SPIM TX More...
#define | LL_DMA0_PERIPH_SPIM_RX ((uint32_t)0x00000003U)
| DMA Peripheral type is SPIM RX More...
#define | LL_DMA0_PERIPH_SPIS_TX ((uint32_t)0x00000004U)
| DMA Peripheral type is SPIS TX More...
#define | LL_DMA0_PERIPH_SPIS_RX ((uint32_t)0x00000005U)
| DMA Peripheral type is SPIS RX More...
#define | LL_DMA0_PERIPH_UART0_TX ((uint32_t)0x00000006U)
| DMA Peripheral type is UART0 TX More...
#define | LL_DMA0_PERIPH_UART0_RX ((uint32_t)0x00000007U)
| DMA Peripheral type is UART0 RX More...
#define | LL_DMA0_PERIPH_UART1_TX ((uint32_t)0x00000008U)
| DMA Peripheral type is UART1 TX More...
#define | LL_DMA0_PERIPH_UART1_RX ((uint32_t)0x00000009U)
| DMA Peripheral type is UART1 RX More...
#define | LL_DMA0_PERIPH_SNSADC ((uint32_t)0x0000000AU)
| DMA peripheral type is SNSADC More...
#define | LL_DMA0_PERIPH_OSPI_TX ((uint32_t)0x0000000CU)
| DMA Peripheral type is OSPIM TX More...
#define | LL_DMA0_PERIPH_OSPI_RX ((uint32_t)0x0000000DU)
| DMA Peripheral type is OSPIM RX More...
#define | LL_DMA0_PERIPH_UART2_TX ((uint32_t)0x0000000EU)
| DMA Peripheral type is UART2 TX More...
#define | LL_DMA0_PERIPH_UART2_RX ((uint32_t)0x0000000FU)
| DMA Peripheral type is UART2 RX More...
#define | LL_DMA0_PERIPH_I2C2_TX ((uint32_t)0x00000012U)
| DMA Peripheral type is I2C2 TX More...
#define | LL_DMA0_PERIPH_I2C2_RX ((uint32_t)0x00000013U)
| DMA Peripheral type is I2C2 RX More...
#define | LL_DMA0_PERIPH_UART3_TX ((uint32_t)0x00000014U)
| DMA Peripheral type is UART3 TX More...
#define | LL_DMA0_PERIPH_UART3_RX ((uint32_t)0x00000015U)
| DMA Peripheral type is UART3 RX More...
#define | LL_DMA0_PERIPH_I2C5_TX ((uint32_t)0x00000016U)
| DMA Peripheral type is I2C5 TX More...
#define | LL_DMA0_PERIPH_I2C5_RX ((uint32_t)0x00000017U)
| DMA Peripheral type is I2C5 RX More...
#define | LL_DMA0_PERIPH_I2C4_TX ((uint32_t)0x00000018U)
| DMA Peripheral type is I2C4 TX More...
#define | LL_DMA0_PERIPH_I2C4_RX ((uint32_t)0x00000019U)
| DMA Peripheral type is I2C5 RX More...
#define | LL_DMA0_PERIPH_UART4_TX ((uint32_t)0x0000001AU)
| DMA Peripheral type is UART4 TX More...
#define | LL_DMA0_PERIPH_UART4_RX ((uint32_t)0x0000001BU)
| DMA Peripheral type is UART4 RX More...
#define | LL_DMA0_PERIPH_QSPI1_TX ((uint32_t)0x0000001CU)
| DMA Peripheral type is QSPIM1 TX. More...
#define | LL_DMA0_PERIPH_QSPI1_RX ((uint32_t)0x0000001DU)
| DMA Peripheral type is QSPIM1 RX. More...
#define | LL_DMA0_PERIPH_I2C3_TX ((uint32_t)0x0000001EU)
| DMA Peripheral type is I2C3 TX More...
#define | LL_DMA0_PERIPH_I2C3_RX ((uint32_t)0x0000001FU)
| DMA Peripheral type is I2C3 RX More...
#define | LL_DMA1_PERIPH_MEM ((uint32_t)0x00000009U)
| DMA peripheral type is Memory. More...
#define | LL_DMA1_PERIPH_OSPI_TX ((uint32_t)0x00000000U)
| DMA Peripheral type is OSPIM TX More...
#define | LL_DMA1_PERIPH_OSPI_RX ((uint32_t)0x00000001U)
| DMA Peripheral type is OSPIM RX More...
#define | LL_DMA1_PERIPH_QSPI2_TX ((uint32_t)0x00000002U)
| DMA Peripheral type is QSPIM2 TX. More...
#define | LL_DMA1_PERIPH_QSPI2_RX ((uint32_t)0x00000003U)
| DMA Peripheral type is QSPIM2 RX. More...
#define | LL_DMA1_PERIPH_I2S_M_TX ((uint32_t)0x00000004U)
| DMA Peripheral type is IIS_M TX More...
#define | LL_DMA1_PERIPH_I2S_M_RX ((uint32_t)0x00000005U)
| DMA Peripheral type is IIS_M RX More...
#define | LL_DMA1_PERIPH_I2S_S_TX ((uint32_t)0x00000006U)
| DMA Peripheral type is IIS_S TX More...
#define | LL_DMA1_PERIPH_I2S_S_RX ((uint32_t)0x00000007U)
| DMA Peripheral type is IIS_S RX More...
#define | LL_DMA1_PERIPH_PDM_TX ((uint32_t)0x00000008U)
| DMA Peripheral type is PDM TX More...
#define | LL_DMA1_PERIPH_QSPI1_TX ((uint32_t)0x0000000AU)
| DMA Peripheral type is QSPIM1 TX. More...
#define | LL_DMA1_PERIPH_QSPI1_RX ((uint32_t)0x0000000BU)
| DMA Peripheral type is QSPIM1 RX. More...
#define | LL_DMA1_PERIPH_I2C0_TX ((uint32_t)0x0000000CU)
| DMA Peripheral type is I2C0 TX More...
#define | LL_DMA1_PERIPH_I2C0_RX ((uint32_t)0x0000000DU)
| DMA Peripheral type is I2C0 RX More...
#define | LL_DMA1_PERIPH_I2C1_TX ((uint32_t)0x0000000EU)
| DMA Peripheral type is I2C1 TX More...
#define | LL_DMA1_PERIPH_I2C1_RX ((uint32_t)0x0000000FU)
| DMA Peripheral type is I2C1 RX More...
#define | LL_DMA1_PERIPH_SPIM_TX ((uint32_t)0x00000010U)
| DMA Peripheral type is SPIM TX More...
#define | LL_DMA1_PERIPH_SPIM_RX ((uint32_t)0x00000011U)
| DMA Peripheral type is SPIM RX More...
#define | LL_DMA1_PERIPH_DSPIM_TX ((uint32_t)0x00000012U)
| DMA Peripheral type is DSPIM TX More...
#define | LL_DMA1_PERIPH_DSPIM_RX ((uint32_t)0x00000013U)
| DMA Peripheral type is DSPIM RX More...
#define | LL_DMA1_PERIPH_QSPI1_TX_2 ((uint32_t)0x00000014U)
| DMA Peripheral type is QSPI1 TX More...
#define | LL_DMA1_PERIPH_QSPI1_RX_2 ((uint32_t)0x00000015U)
| DMA Peripheral type is QSPI1 RX More...
#define | LL_DMA1_PERIPH_UART3_TX ((uint32_t)0x00000016U)
| DMA Peripheral type is UART3 TX More...
#define | LL_DMA1_PERIPH_UART3_RX ((uint32_t)0x00000017U)
| DMA Peripheral type is UART3 RX More...
#define | LL_DMA1_PERIPH_UART4_TX ((uint32_t)0x00000018U)
| DMA Peripheral type is UART4 TX More...
#define | LL_DMA1_PERIPH_UART4_RX ((uint32_t)0x00000019U)
| DMA Peripheral type is UART4 RX More...
#define | LL_DMA1_PERIPH_UART5_TX ((uint32_t)0x0000001AU)
| DMA Peripheral type is UART5 TX More...
#define | LL_DMA1_PERIPH_UART5_RX ((uint32_t)0x0000001BU)
| DMA Peripheral type is UART5 RX More...
#define | LL_DMA1_PERIPH_UART0_TX ((uint32_t)0x0000001EU)
| DMA Peripheral type is UART0 TX More...
#define | LL_DMA1_PERIPH_UART0_RX ((uint32_t)0x0000001FU)
| DMA Peripheral type is UART0 RX More...
#define | LL_DMA_WriteReg(__instance__, __REG__, __VALUE__) WRITE_REG(__instance__.__REG__, (__VALUE__))
| Write a value in DMA register. More...
#define | LL_DMA_ReadReg(__instance__, __REG__) READ_REG(__instance__.__REG__)
| Read a value in DMA register. More...

## Typedefs
typedef struct _ll_dma_init | ll_dma_init_t
| LL DMA init Structure definition. More...

## Functions
__STATIC_INLINE void | ll_dma_enable (dma_regs_t *DMAx)
| Enable DMA Module. More...
__STATIC_INLINE void | ll_dma_disable (dma_regs_t *DMAx)
| Disable DMA Module. More...
__STATIC_INLINE uint32_t | ll_dma_is_enable (dma_regs_t *DMAx)
| Check if DMA Module is enabled or disabled. More...
__STATIC_INLINE void | ll_dma_enable_channel (dma_regs_t *DMAx, uint32_t channel)
| Enable DMA channel. More...
__STATIC_INLINE void | ll_dma_disable_channel (dma_regs_t *DMAx, uint32_t channel)
| Disable DMA channel. More...
__STATIC_INLINE uint32_t | ll_dma_is_enabled_channel (dma_regs_t *DMAx, uint32_t channel)
| Check if DMA channel is enabled or disabled. More...
__STATIC_INLINE void | ll_dma_suspend_channel (dma_regs_t *DMAx, uint32_t channel)
| Suspend a DMA channel transfer. More...
__STATIC_INLINE void | ll_dma_resume_channel (dma_regs_t *DMAx, uint32_t channel)
| Resume a DMA channel. More...
__STATIC_INLINE uint32_t | ll_dma_is_suspended (dma_regs_t *DMAx, uint32_t channel)
| Check if DMA channel is suspended or resumed. More...
__STATIC_INLINE uint32_t | ll_dma_is_empty_fifo (dma_regs_t *DMAx, uint32_t channel)
| Check if DMA channel FIFO is empty. More...
__STATIC_INLINE void | ll_dma_config_transfer (dma_regs_t *DMAx, uint32_t channel, uint32_t configuration)
| Configure all parameters link to DMA transfer. More...
__STATIC_INLINE void | ll_dma_set_data_transfer_direction (dma_regs_t *DMAx, uint32_t channel, uint32_t direction)
| Set Data transfer direction (read from peripheral or from memory). More...
__STATIC_INLINE uint32_t | ll_dma_get_data_transfer_direction (dma_regs_t *DMAx, uint32_t channel)
| Get Data transfer direction (read from peripheral or from memory). More...
__STATIC_INLINE void | ll_dma_set_mode (dma_regs_t *DMAx, uint32_t channel, uint32_t mode)
| Set DMA mode Single block or Multi block. More...
__STATIC_INLINE uint32_t | ll_dma_get_mode (dma_regs_t *DMAx, uint32_t channel)
| Get DMA mode circular or normal. More...
__STATIC_INLINE void | ll_dma_set_max_amba_burst (dma_regs_t *DMAx, uint32_t channel, uint32_t beats)
| Set Maximum AMBA Burst Length. More...
__STATIC_INLINE uint32_t | ll_dma_get_max_amba_burst (dma_regs_t *DMAx, uint32_t channel)
| Get source status after each block tranfer completed. More...
__STATIC_INLINE void | ll_dma_set_sstat (dma_regs_t *DMAx, uint32_t channel, uint32_t sstat)
| Set source status after each block tranfer completed. More...
__STATIC_INLINE uint32_t | ll_dma_get_sstat (dma_regs_t *DMAx, uint32_t channel)
| Get source status after each block tranfer completed. More...
__STATIC_INLINE void | ll_dma_set_dstat (dma_regs_t *DMAx, uint32_t channel, uint32_t dstat)
| Set deatination status after each block tranfer completed. More...
__STATIC_INLINE uint32_t | ll_dma_get_dstat (dma_regs_t *DMAx, uint32_t channel)
| Get deatination status after each block tranfer completed. More...
__STATIC_INLINE void | ll_dma_set_sstatar (dma_regs_t *DMAx, uint32_t channel, uint32_t sstatar)
| Set source status address after each block tranfer completed. More...
__STATIC_INLINE uint32_t | ll_dma_get_sstatar (dma_regs_t *DMAx, uint32_t channel)
| Get source status address after each block tranfer completed. More...
__STATIC_INLINE void | ll_dma_set_dstatar (dma_regs_t *DMAx, uint32_t channel, uint32_t dstatar)
| Set deatination status address after each block tranfer completed. More...
__STATIC_INLINE uint32_t | ll_dma_get_dstatar (dma_regs_t *DMAx, uint32_t channel)
| Get deatination status address after each block tranfer completed. More...
__STATIC_INLINE void | ll_dma_set_llp_loc (dma_regs_t *DMAx, uint32_t channel, uint32_t llp_loc)
| Set LLP loc. More...
__STATIC_INLINE uint32_t | ll_dma_get_llp_loc (dma_regs_t *DMAx, uint32_t channel)
| Get LLP loc. More...
__STATIC_INLINE void | ll_dma_set_llp_dst_en (dma_regs_t *DMAx, uint32_t channel, uint32_t llp_dst_en)
| Set destination LLP enable. More...
__STATIC_INLINE uint32_t | ll_dma_get_llp_dst_en (dma_regs_t *DMAx, uint32_t channel)
| Get destination LLP enable. More...
__STATIC_INLINE void | ll_dma_set_llp_src_en (dma_regs_t *DMAx, uint32_t channel, uint32_t llp_src_en)
| Set source LLP enable. More...
__STATIC_INLINE uint32_t | ll_dma_get_llp_src_en (dma_regs_t *DMAx, uint32_t channel)
| Get source LLP enable. More...
__STATIC_INLINE void | ll_dma_set_dst_scatter_en (dma_regs_t *DMAx, uint32_t channel, uint32_t dst_scatter_en)
| Set destination scatter enable. More...
__STATIC_INLINE uint32_t | ll_dma_get_dst_scatter_en (dma_regs_t *DMAx, uint32_t channel)
| Get destination scatter enable. More...
__STATIC_INLINE void | ll_dma_set_src_gather_en (dma_regs_t *DMAx, uint32_t channel, uint32_t src_gather_en)
| Set source gather enable. More...
__STATIC_INLINE uint32_t | ll_dma_get_src_gather_en (dma_regs_t *DMAx, uint32_t channel)
| Get source gather enable. More...
__STATIC_INLINE void | ll_dma_set_source_increment_mode (dma_regs_t *DMAx, uint32_t channel, uint32_t src_increment_mode)
| Set Source increment mode. More...
__STATIC_INLINE uint32_t | ll_dma_get_source_increment_mode (dma_regs_t *DMAx, uint32_t channel)
| Get Source increment mode. More...
__STATIC_INLINE void | ll_dma_set_destination_increment_mode (dma_regs_t *DMAx, uint32_t channel, uint32_t dst_increment_mode)
| Set Destination increment mode. More...
__STATIC_INLINE uint32_t | ll_dma_get_destination_increment_mode (dma_regs_t *DMAx, uint32_t channel)
| Get Destination increment mode. More...
__STATIC_INLINE void | ll_dma_set_source_width (dma_regs_t *DMAx, uint32_t channel, uint32_t src_width)
| Set Source transfer width. More...
__STATIC_INLINE uint32_t | ll_dma_get_source_width (dma_regs_t *DMAx, uint32_t channel)
| Get Source transfer width. More...
__STATIC_INLINE void | ll_dma_set_destination_width (dma_regs_t *DMAx, uint32_t channel, uint32_t dst_width)
| Set Destination transfer width. More...
__STATIC_INLINE uint32_t | ll_dma_get_destination_width (dma_regs_t *DMAx, uint32_t channel)
| Get Destination transfer width. More...
__STATIC_INLINE void | ll_dma_set_source_burst_length (dma_regs_t *DMAx, uint32_t channel, uint32_t burst_length)
| Set Source Burst Transaction Length. More...
__STATIC_INLINE uint32_t | ll_dma_get_source_burst_length (dma_regs_t *DMAx, uint32_t channel)
| Get Burst Transaction Length. More...
__STATIC_INLINE void | ll_dma_set_destination_burst_length (dma_regs_t *DMAx, uint32_t channel, uint32_t burst_length)
| Set Destination Burst Transaction Length. More...
__STATIC_INLINE uint32_t | ll_dma_get_destination_burst_length (dma_regs_t *DMAx, uint32_t channel)
| Get Destination Burst Transaction Length. More...
__STATIC_INLINE void | ll_dma_set_channel_priority_level (dma_regs_t *DMAx, uint32_t channel, uint32_t priority)
| Set Channel priority level. More...
__STATIC_INLINE uint32_t | ll_dma_get_channel_priority_level (dma_regs_t *DMAx, uint32_t channel)
| Get Channel priority level. More...
__STATIC_INLINE void | ll_dma_set_block_size (dma_regs_t *DMAx, uint32_t channel, uint32_t block_size)
| Set the block size of a transfer. More...
__STATIC_INLINE uint32_t | ll_dma_get_block_size (dma_regs_t *DMAx, uint32_t channel)
| Get the block size of a transfer. More...
__STATIC_INLINE void | ll_dma_config_address (dma_regs_t *DMAx, uint32_t channel, uint32_t src_address, uint32_t dst_address, uint32_t direction)
| Configure the Source and Destination addresses. More...
__STATIC_INLINE void | ll_dma_set_source_address (dma_regs_t *DMAx, uint32_t channel, uint32_t address)
| Set the Source address. More...
__STATIC_INLINE void | ll_dma_set_destination_address (dma_regs_t *DMAx, uint32_t channel, uint32_t address)
| Set the Destination address. More...
__STATIC_INLINE uint32_t | ll_dma_get_source_address (dma_regs_t *DMAx, uint32_t channel)
| Get Source address. More...
__STATIC_INLINE uint32_t | ll_dma_get_destination_address (dma_regs_t *DMAx, uint32_t channel)
| Get Destination address. More...
__STATIC_INLINE void | ll_dma_set_m2m_src_address (dma_regs_t *DMAx, uint32_t channel, uint32_t address)
| Set the Memory to Memory Source address. More...
__STATIC_INLINE void | ll_dma_set_m2m_dst_address (dma_regs_t *DMAx, uint32_t channel, uint32_t address)
| Set the Memory to Memory Destination address. More...
__STATIC_INLINE uint32_t | ll_dma_get_m2m_src_address (dma_regs_t *DMAx, uint32_t channel)
| Get the Memory to Memory Source address. More...
__STATIC_INLINE uint32_t | ll_dma_get_m2m_dst_address (dma_regs_t *DMAx, uint32_t channel)
| Get the Memory to Memory Destination address. More...
__STATIC_INLINE void | ll_dma_enable_src_stat_update (dma_regs_t *DMAx, uint32_t channel)
| Enable Source Status Update Enable for DMA instance on Channel x. More...
__STATIC_INLINE void | ll_dma_disable_src_stat_update (dma_regs_t *DMAx, uint32_t channel)
| Disable Source Status Update Enable for DMA instance on Channel x. More...
__STATIC_INLINE uint32_t | ll_dma_src_stat_update_is_enable (dma_regs_t *DMAx, uint32_t channel)
| Check if Source Status Update Enable. More...
__STATIC_INLINE void | ll_dma_enable_dst_stat_update (dma_regs_t *DMAx, uint32_t channel)
| Enable Destination Status Update Enable for DMA instance on Channel x. More...
__STATIC_INLINE void | ll_dma_disable_dst_stat_update (dma_regs_t *DMAx, uint32_t channel)
| Disable Destination Status Update Enable for DMA instance on Channel x. More...
__STATIC_INLINE uint32_t | ll_dma_dst_stat_update_is_enable (dma_regs_t *DMAx, uint32_t channel)
| Check if Destination Status Update Enable. More...
__STATIC_INLINE void | ll_dma_set_source_peripheral (dma_regs_t *DMAx, uint32_t channel, uint32_t peripheral)
| Set source peripheral for DMA instance on Channel x. More...
__STATIC_INLINE uint32_t | ll_dma_get_source_peripheral (dma_regs_t *DMAx, uint32_t channel)
| Get source peripheral for DMA instance on Channel x. More...
__STATIC_INLINE void | ll_dma_set_destination_peripheral (dma_regs_t *DMAx, uint32_t channel, uint32_t peripheral)
| Set destination peripheral for DMA instance on Channel x. More...
__STATIC_INLINE uint32_t | ll_dma_get_destination_peripheral (dma_regs_t *DMAx, uint32_t channel)
| Get destination peripheral for DMA instance on Channel x. More...
__STATIC_INLINE void | ll_dma_select_handshaking (dma_regs_t *DMAx, uint32_t channel, uint32_t src_handshaking, uint32_t dst_handshaking)
| Set source and destination source handshaking interface. More...
__STATIC_INLINE void | ll_dma_set_src_gather_sgi (dma_regs_t *DMAx, uint32_t channel, uint32_t src_gather_sgi)
| Set source gather interval. More...
__STATIC_INLINE uint32_t | ll_dma_get_src_gather_sgi (dma_regs_t *DMAx, uint32_t channel)
| Get source gather interval. More...
__STATIC_INLINE void | ll_dma_set_src_gather_sgc (dma_regs_t *DMAx, uint32_t channel, uint32_t src_gather_sgc)
| Set source gather count. More...
__STATIC_INLINE uint32_t | ll_dma_get_src_gather_sgc (dma_regs_t *DMAx, uint32_t channel)
| Get source gather count. More...
__STATIC_INLINE void | ll_dma_set_dst_scatter_dsi (dma_regs_t *DMAx, uint32_t channel, uint32_t dst_scatter_dsi)
| Set destination scatter interval. More...
__STATIC_INLINE uint32_t | ll_dma_get_dst_scatter_dsi (dma_regs_t *DMAx, uint32_t channel)
| Get Set destination scatter interval. More...
__STATIC_INLINE void | ll_dma_set_dst_scatter_dsc (dma_regs_t *DMAx, uint32_t channel, uint32_t dst_scatter_dsc)
| Set destination scatter count. More...
__STATIC_INLINE uint32_t | ll_dma_get_dst_scatter_dsc (dma_regs_t *DMAx, uint32_t channel)
| Get destination scatter count. More...
__STATIC_INLINE void | ll_dma_req_src_single_transaction (dma_regs_t *DMAx, uint32_t channel)
| Source Single Transaction Request. More...
__STATIC_INLINE void | ll_dma_req_src_burst_transaction (dma_regs_t *DMAx, uint32_t channel)
| Source Burst Transaction Request. More...
__STATIC_INLINE void | ll_dma_req_src_last_single_transaction (dma_regs_t *DMAx, uint32_t channel)
| Source Last Single Transaction Request. More...
__STATIC_INLINE void | ll_dma_req_src_last_burst_transaction (dma_regs_t *DMAx, uint32_t channel)
| Source Last Burst Transaction Request. More...
__STATIC_INLINE void | ll_dma_req_dst_single_transaction (dma_regs_t *DMAx, uint32_t channel)
| Destination Single Transaction Request. More...
__STATIC_INLINE void | ll_dma_req_dst_burst_transaction (dma_regs_t *DMAx, uint32_t channel)
| Destination Burst Transaction Request. More...
__STATIC_INLINE void | ll_dma_req_dst_last_single_transaction (dma_regs_t *DMAx, uint32_t channel)
| Destination Last Single Transaction Request. More...
__STATIC_INLINE void | ll_dma_req_dst_last_burst_transaction (dma_regs_t *DMAx, uint32_t channel)
| Destination Last Burst Transaction Request. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_gtfr (dma_regs_t *DMAx)
| Get DMA Module global transfer complete interrupt status. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_gblk (dma_regs_t *DMAx)
| Get DMA Module global block complete interrupt status. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_gsrct (dma_regs_t *DMAx)
| Get DMA Module global source transaction complete interrupt status. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_gdstt (dma_regs_t *DMAx)
| Get DMA Module global destination transaction complete interrupt status. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_gerr (dma_regs_t *DMAx)
| Get DMA Module global error interrupt status. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_rtfr (dma_regs_t *DMAx, uint32_t channel)
| Indicate the Raw Status of IntTfr Interrupt flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_rblk (dma_regs_t *DMAx, uint32_t channel)
| Indicate the Raw Status of IntBlock Interrupt flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_rsrct (dma_regs_t *DMAx, uint32_t channel)
| Indicate the Raw Status of IntSrcTran Interrupt flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_rdstt (dma_regs_t *DMAx, uint32_t channel)
| Indicate the Raw Status of IntDstTran Interrupt flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_rerr (dma_regs_t *DMAx, uint32_t channel)
| Indicate the Raw Status of IntErr Interrupt flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_tfr (dma_regs_t *DMAx, uint32_t channel)
| Indicate the status of DMA Channel transfer complete flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_tfr0 (dma_regs_t *DMAx)
| Indicate the status of Channel 0 transfer complete flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_tfr1 (dma_regs_t *DMAx)
| Indicate the status of Channel 1 transfer complete flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_tfr2 (dma_regs_t *DMAx)
| Indicate the status of Channel 2 transfer complete flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_tfr3 (dma_regs_t *DMAx)
| Indicate the status of Channel 3 transfer complete flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_tfr4 (dma_regs_t *DMAx)
| Indicate the status of Channel 4 transfer complete flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_tfr5 (dma_regs_t *DMAx)
| Indicate the status of Channel 5 transfer complete flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_tfr6 (dma_regs_t *DMAx)
| Indicate the status of Channel 6 transfer complete flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_tfr7 (dma_regs_t *DMAx)
| Indicate the status of Channel 7 transfer complete flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_blk (dma_regs_t *DMAx, uint32_t channel)
| Indicate the status of DMA Channel block complete flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_blk0 (dma_regs_t *DMAx)
| Indicate the status of Channel 0 block complete flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_blk1 (dma_regs_t *DMAx)
| Indicate the status of Channel 1 block complete flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_blk2 (dma_regs_t *DMAx)
| Indicate the status of Channel 2 block complete flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_blk3 (dma_regs_t *DMAx)
| Indicate the status of Channel 3 block complete flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_blk4 (dma_regs_t *DMAx)
| Indicate the status of Channel 4 block complete flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_blk5 (dma_regs_t *DMAx)
| Indicate the status of Channel 5 block complete flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_blk6 (dma_regs_t *DMAx)
| Indicate the status of Channel 6 block complete flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_blk7 (dma_regs_t *DMAx)
| Indicate the status of Channel 7 block complete flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_srct (dma_regs_t *DMAx, uint32_t channel)
| Indicate the status of DMA Channel source transaction complete flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_srct0 (dma_regs_t *DMAx)
| Indicate the status of Channel 0 source transaction complete flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_srct1 (dma_regs_t *DMAx)
| Indicate the status of Channel 1 source transaction complete flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_srct2 (dma_regs_t *DMAx)
| Indicate the status of Channel 2 source transaction complete flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_srct3 (dma_regs_t *DMAx)
| Indicate the status of Channel 3 source transaction complete flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_srct4 (dma_regs_t *DMAx)
| Indicate the status of Channel 4 source transaction complete flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_srct5 (dma_regs_t *DMAx)
| Indicate the status of Channel 5 source transaction complete flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_srct6 (dma_regs_t *DMAx)
| Indicate the status of Channel 6 source transaction complete flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_srct7 (dma_regs_t *DMAx)
| Indicate the status of Channel 7 source transaction complete flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_dstt (dma_regs_t *DMAx, uint32_t channel)
| Indicate the status of DMA Channel destination transaction complete flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_dstt0 (dma_regs_t *DMAx)
| Indicate the status of Channel 0 destination transaction complete flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_dstt1 (dma_regs_t *DMAx)
| Indicate the status of Channel 1 destination transaction complete flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_dstt2 (dma_regs_t *DMAx)
| Indicate the status of Channel 2 destination transaction complete flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_dstt3 (dma_regs_t *DMAx)
| Indicate the status of Channel 3 destination transaction complete flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_dstt4 (dma_regs_t *DMAx)
| Indicate the status of Channel 4 destination transaction complete flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_dstt5 (dma_regs_t *DMAx)
| Indicate the status of Channel 5 destination transaction complete flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_dstt6 (dma_regs_t *DMAx)
| Indicate the status of Channel 6 destination transaction complete flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_dstt7 (dma_regs_t *DMAx)
| Indicate the status of Channel 7 destination transaction complete flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_err (dma_regs_t *DMAx, uint32_t channel)
| Indicate the status of DMA Channel error flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_err0 (dma_regs_t *DMAx)
| Indicate the status of Channel 0 error flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_err1 (dma_regs_t *DMAx)
| Indicate the status of Channel 1 error flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_err2 (dma_regs_t *DMAx)
| Indicate the status of Channel 2 error flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_err3 (dma_regs_t *DMAx)
| Indicate the status of Channel 3 error flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_err4 (dma_regs_t *DMAx)
| Indicate the status of Channel 4 error flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_err5 (dma_regs_t *DMAx)
| Indicate the status of Channel 5 error flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_err6 (dma_regs_t *DMAx)
| Indicate the status of Channel 6 error flag. More...
__STATIC_INLINE uint32_t | ll_dma_is_active_flag_err7 (dma_regs_t *DMAx)
| Indicate the status of Channel 7 error flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_tfr (dma_regs_t *DMAx, uint32_t channel)
| Clear DMA Channel transfer complete flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_tfr0 (dma_regs_t *DMAx)
| Clear Channel 0 transfer complete flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_tfr1 (dma_regs_t *DMAx)
| Clear Channel 1 transfer complete flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_tfr2 (dma_regs_t *DMAx)
| Clear Channel 2 transfer complete flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_tfr3 (dma_regs_t *DMAx)
| Clear Channel 3 transfer complete flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_tfr4 (dma_regs_t *DMAx)
| Clear Channel 4 transfer complete flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_tfr5 (dma_regs_t *DMAx)
| Clear Channel 5 transfer complete flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_tfr6 (dma_regs_t *DMAx)
| Clear Channel 6 transfer complete flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_tfr7 (dma_regs_t *DMAx)
| Clear Channel 7 transfer complete flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_blk (dma_regs_t *DMAx, uint32_t channel)
| Clear DMA Channel block complete flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_blk0 (dma_regs_t *DMAx)
| Clear Channel 0 Block Complete flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_blk1 (dma_regs_t *DMAx)
| Clear Channel 1 Block Complete flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_blk2 (dma_regs_t *DMAx)
| Clear Channel 2 Block Complete flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_blk3 (dma_regs_t *DMAx)
| Clear Channel 3 Block Complete flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_blk4 (dma_regs_t *DMAx)
| Clear Channel 4 Block Complete flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_blk5 (dma_regs_t *DMAx)
| Clear Channel 5 Block Complete flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_blk6 (dma_regs_t *DMAx)
| Clear Channel 6 Block Cmplete flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_blk7 (dma_regs_t *DMAx)
| Clear Channel 7 Block Complete flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_srct (dma_regs_t *DMAx, uint32_t channel)
| Clear DMA Channel source transaction Complete flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_srct0 (dma_regs_t *DMAx)
| Clear Channel 0 source transaction Complete flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_srct1 (dma_regs_t *DMAx)
| Clear Channel 1 source transaction Complete flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_srct2 (dma_regs_t *DMAx)
| Clear Channel 2 source transaction Complete flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_srct3 (dma_regs_t *DMAx)
| Clear Channel 3 source transaction Complete flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_srct4 (dma_regs_t *DMAx)
| Clear Channel 4 source transaction Complete flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_srct5 (dma_regs_t *DMAx)
| Clear Channel 5 source transaction Complete flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_srct6 (dma_regs_t *DMAx)
| Clear Channel 6 source transaction Complete flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_srct7 (dma_regs_t *DMAx)
| Clear Channel 7 source transaction Complete flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_dstt (dma_regs_t *DMAx, uint32_t channel)
| Clear DMA Channel destination transaction Complete flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_dstt0 (dma_regs_t *DMAx)
| Clear Channel 0 destination transaction Complete status. More...
__STATIC_INLINE void | ll_dma_clear_flag_dstt1 (dma_regs_t *DMAx)
| Clear Channel 1 destination transaction Complete flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_dstt2 (dma_regs_t *DMAx)
| Clear Channel 2 destination transaction Complete flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_dstt3 (dma_regs_t *DMAx)
| Clear Channel 3 destination transaction Complete flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_dstt4 (dma_regs_t *DMAx)
| Clear Channel 4 destination transaction Complete flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_dstt5 (dma_regs_t *DMAx)
| Clear Channel 5 destination transaction Complete flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_dstt6 (dma_regs_t *DMAx)
| Clear Channel 6 destination transaction Complete flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_dstt7 (dma_regs_t *DMAx)
| Clear Channel 7 destination transaction Complete flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_err (dma_regs_t *DMAx, uint32_t channel)
| Clear DMA Channel error flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_err0 (dma_regs_t *DMAx)
| Clear Channel 0 error flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_err1 (dma_regs_t *DMAx)
| Clear Channel 1 error flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_err2 (dma_regs_t *DMAx)
| Clear Channel 2 error flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_err3 (dma_regs_t *DMAx)
| Clear Channel 3 error flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_err4 (dma_regs_t *DMAx)
| Clear Channel 4 error flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_err5 (dma_regs_t *DMAx)
| Clear Channel 5 error flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_err6 (dma_regs_t *DMAx)
| Clear Channel 6 error flag. More...
__STATIC_INLINE void | ll_dma_clear_flag_err7 (dma_regs_t *DMAx)
| Clear Channel 7 error flag. More...
__STATIC_INLINE void | ll_dma_enable_it_tfr (dma_regs_t *DMAx, uint32_t channel)
| Enable Transfer Complete interrupt. More...
__STATIC_INLINE void | ll_dma_enable_it_blk (dma_regs_t *DMAx, uint32_t channel)
| Enable Block Complete interrupt. More...
__STATIC_INLINE void | ll_dma_enable_it_srct (dma_regs_t *DMAx, uint32_t channel)
| Enable source transaction Complete interrupt. More...
__STATIC_INLINE void | ll_dma_enable_it_dstt (dma_regs_t *DMAx, uint32_t channel)
| Enable destination transaction Complete interrupt. More...
__STATIC_INLINE void | ll_dma_enable_it_err (dma_regs_t *DMAx, uint32_t channel)
| Enable error interrupt. More...
__STATIC_INLINE void | ll_dma_disable_it_tfr (dma_regs_t *DMAx, uint32_t channel)
| Disable Transfer Complete interrupt. More...
__STATIC_INLINE void | ll_dma_disable_it_blk (dma_regs_t *DMAx, uint32_t channel)
| Disable Block Complete interrupt. More...
__STATIC_INLINE void | ll_dma_disable_it_srct (dma_regs_t *DMAx, uint32_t channel)
| Disable source transaction Complete interrupt. More...
__STATIC_INLINE void | ll_dma_disable_it_dstt (dma_regs_t *DMAx, uint32_t channel)
| Disable destination transaction Complete interrupt. More...
__STATIC_INLINE void | ll_dma_disable_it_err (dma_regs_t *DMAx, uint32_t channel)
| Disable error interrupt. More...
__STATIC_INLINE uint32_t | ll_dma_is_enable_it_tfr (dma_regs_t *DMAx, uint32_t channel)
| Check if DMA Transfer interrupt is enabled or disabled. More...
__STATIC_INLINE uint32_t | ll_dma_is_enable_it_blk (dma_regs_t *DMAx, uint32_t channel)
| Check if DMA block interrupt is enabled or disabled. More...
__STATIC_INLINE uint32_t | ll_dma_is_enable_it_srct (dma_regs_t *DMAx, uint32_t channel)
| Check if DMA source transaction interrupt is enabled or disabled. More...
__STATIC_INLINE uint32_t | ll_dma_is_enable_it_dstt (dma_regs_t *DMAx, uint32_t channel)
| Check if DMA destination transaction interrupt is enabled or disabled. More...
__STATIC_INLINE uint32_t | ll_dma_is_enable_it_err (dma_regs_t *DMAx, uint32_t channel)
| Check if DMA error interrupt is enabled or disabled. More...
__STATIC_INLINE void | ll_dma_enable_it (dma_regs_t *DMAx, uint32_t channel)
| Enable DMA channel interrupt. More...
__STATIC_INLINE void | ll_dma_disable_it (dma_regs_t *DMAx, uint32_t channel)
| Disable DMA channel interrupt. More...
__STATIC_INLINE uint32_t | ll_dma_is_enable_it (dma_regs_t *DMAx, uint32_t channel)
| Check if DMA interrupt is enabled or disabled. More...
error_status_t | ll_dma_deinit (dma_regs_t *DMAx, uint32_t channel)
| De-initialize the DMA registers to their default reset values. More...
error_status_t | ll_dma_init (dma_regs_t *DMAx, uint32_t channel, ll_dma_init_t *p_dma_init)
| Initialize the DMA registers according to the specified parameters in p_dma_init. More...
void | ll_dma_struct_init (ll_dma_init_t *p_dma_init)
| Set each field of a ll_dma_init_t type structure to default value. More...
error_status_t | ll_dma_hs_choice (dma_regs_t *DMAx, uint32_t src_peripheral, uint32_t dst_peripheral)
| Initialize the DMA HS choice according to the specified parameters. More...

## Detailed Description

Header file containing functions prototypes of DMA LL library.

Author
  BLE Driver Team

Attention

  ##### Copyright (c) 2019 GOODIX

All rights reserved.

Redistribution and use in source and binary forms, with or without modification, are permitted provided that the following conditions are met: Redistributions of source code must retain the above copyright notice, this list of conditions and the following disclaimer. Redistributions in binary form must reproduce the above copyright notice, this list of conditions and the following disclaimer in the documentation and/or other materials provided with the distribution. Neither the name of GOODIX nor the names of its contributors may be used to endorse or promote products derived from this software without specific prior written permission.

THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL COPYRIGHT HOLDERS AND CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.

Definition in file gr55xx_ll_dma.h.