Public Attributes | List of all members
iso_set_data_path_trigger_t Struct Reference
BLE » Core Isochronous Channels » Structures

The parameter for set iso data path trigger. More...

`#include <ble_iso.h>`

## Public Attributes
uint16_t | conn_hdl
| Connection handle of CIS/BIS. More...
uint8_t | direction
| Specifies the data transport path, see iso_data_path_direction_t. More...
uint8_t | enable_flag
| 0x00: disable, 0x01: enable. More...
int32_t | trigger_offset
| Trigger offset in microseconds. More...

## Detailed Description

The parameter for set iso data path trigger.

Definition at line 425 of file ble_iso.h.

## Member Data Documentation

## ◆ conn_hdl

uint16_t iso_set_data_path_trigger_t::conn_hdl

Connection handle of CIS/BIS.

Definition at line 427 of file ble_iso.h.

## ◆ direction

uint8_t iso_set_data_path_trigger_t::direction

Specifies the data transport path, see iso_data_path_direction_t.

Definition at line 428 of file ble_iso.h.

## ◆ enable_flag

uint8_t iso_set_data_path_trigger_t::enable_flag

0x00: disable, 0x01: enable.

Definition at line 429 of file ble_iso.h.

## ◆ trigger_offset

int32_t iso_set_data_path_trigger_t::trigger_offset

Trigger offset in microseconds.

Definition at line 430 of file ble_iso.h.

The documentation for this struct was generated from the following file:

- ble_iso.h