Modules | Macros
Defines
Peripheral Driver » HAL Driver » UART
Collaboration diagram for Defines:

## Modules
| UART Exported Constants
| UART Exported Macros
| UART Private Macros

## Macros
#define | UART_DEFAULT_CONFIG
| Default configuartion for initializing structure. More...

## Detailed Description

## Macro Definition Documentation

## ◆ UART_DEFAULT_CONFIG

#define UART_DEFAULT_CONFIG

Value:
{ \
.baud_rate = 9600, \
.data_bits = UART_DATABITS_8, \
.stop_bits = UART_STOPBITS_1, \
.parity = UART_PARITY_NONE, \
.hw_flow_ctrl = UART_HWCONTROL_NONE, \
.rx_timeout_mode = UART_RECEIVER_TIMEOUT_DISABLE, \
}

Default configuartion for initializing structure.

Definition at line 452 of file gr55xx_hal_uart.h.

UART_DATABITS_8
#define UART_DATABITS_8
UART frame with 8 data bits.
Definition: gr55xx_hal_uart.h:258
UART_HWCONTROL_NONE
#define UART_HWCONTROL_NONE
No hardware control
Definition: gr55xx_hal_uart.h:282
UART_PARITY_NONE
#define UART_PARITY_NONE
No parity
Definition: gr55xx_hal_uart.h:272
UART_RECEIVER_TIMEOUT_DISABLE
#define UART_RECEIVER_TIMEOUT_DISABLE
UART receiver timeout disable.
Definition: gr55xx_hal_uart.h:289
UART_STOPBITS_1
#define UART_STOPBITS_1
UART frame with 1 stop bit
Definition: gr55xx_hal_uart.h:264