Functions
IO operation functions
Peripheral Driver » HAL Driver » WDT » Functions

IO operation functions. More...

Collaboration diagram for IO operation functions:

## Functions
hal_status_t | hal_wdt_refresh (wdt_handle_t *p_wdt)
| Refresh the WDT. More...

## Detailed Description

IO operation functions.

      ==============================================================================
                          ##### IO operation functions #####
      ==============================================================================
      [..]
        This section provides functions allowing to:
        (+) Refresh the WDT.

## Function Documentation

## ◆ hal_wdt_refresh()

hal_status_t hal_wdt_refresh | ( | wdt_handle_t * | p_wdt | ) |

Refresh the WDT.

Parameters

  [in] | p_wdt | Pointer to a WDT handle which contains the configuration information for the specified WDT module.

Return values

  HAL_OK | Operation is OK.
  HAL_ERROR | Parameter error or operation not supported.
  HAL_BUSY | Driver is busy.
  HAL_TIMEOUT | Timeout occurred.