Functions
gr55xx_ll_aon_rf.h File Reference

Header file containing functions prototypes of AON RF LL library. More...

`#include "gr55xx_hal.h"`
Include dependency graph for gr55xx_ll_aon_rf.h:
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Functions
__STATIC_INLINE void | ll_aon_rf_enable_test_mux (void)
| Enable the test mux 0 tri state. More...
__STATIC_INLINE void | ll_aon_rf_disable_test_mux (void)
| Disable the test mux 0 tri state. More...
__STATIC_INLINE void | ll_aon_rf_enable_cpll_cp_reset (void)
| Enable the cpll reset. More...
__STATIC_INLINE void | ll_aon_rf_disable_cpll_cp_reset (void)
| Disable the cpll reset. More...
__STATIC_INLINE void | ll_aon_rf_enable_cpll_drift_detection (void)
| Enable the cpll drift detection. More...
__STATIC_INLINE void | ll_aon_rf_disable_cpll_drift_detection (void)
| Disable the cpll drift detection. More...
__STATIC_INLINE void | ll_aon_rf_set_cpll_m_div (uint32_t value)
| Set the cpll m div,Pre division before CP (00- no division / 11 divide by 16). More...
__STATIC_INLINE void | ll_aon_rf_set_threshold (uint32_t l_threshold, uint32_t h_threshold)
| Set the cpll drift detection. More...
__STATIC_INLINE void | ll_aon_rf_set_cpll_kvco_ctrl (uint32_t code)
| Set the cpll drift CPLL VCO KVCO control. More...
__STATIC_INLINE void | ll_aon_rf_set_xo_ibias (uint32_t hi_value, uint32_t lo_value)
| Set XO core current programmability. More...
__STATIC_INLINE void | ll_aon_rf_set_rf_reg9 (uint32_t value)
| Set the RF_REG9. More...
__STATIC_INLINE uint32_t | ll_aon_rf_get_rf_reg9 (void)
| Get the RF_REG9. More...
__STATIC_INLINE void | ll_aon_rf_set_xo_cap (uint32_t hi_value, uint32_t lo_value)
| Set the xo cap value,cload programmability from 50fF to 26pF on each side. More...
__STATIC_INLINE uint32_t | ll_aon_rf_get_cpll_crscde (void)
| Get the cpll crscde. More...
__STATIC_INLINE void | ll_aon_rf_set_su_enable (void)
| Set SU enable. More...
__STATIC_INLINE void | ll_mcu_set_cpll_drift_irq_enable (void)
| Set cpll drift irq enable. More...
__STATIC_INLINE void | ll_mcu_set_cpll_drift_irq_disable (void)
| Set cpll drift irq disable. More...
__STATIC_INLINE void | ll_mcu_clear_cpll_drift_irq (void)
| clear cpll drift irq. More...

## Detailed Description

Header file containing functions prototypes of AON RF LL library.

Author
  BLE Driver Team

Attention

  ##### Copyright (c) 2019 GOODIX

All rights reserved.

Redistribution and use in source and binary forms, with or without modification, are permitted provided that the following conditions are met: Redistributions of source code must retain the above copyright notice, this list of conditions and the following disclaimer. Redistributions in binary form must reproduce the above copyright notice, this list of conditions and the following disclaimer in the documentation and/or other materials provided with the distribution. Neither the name of GOODIX nor the names of its contributors may be used to endorse or promote products derived from this software without specific prior written permission.

THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL COPYRIGHT HOLDERS AND CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.

Definition in file gr55xx_ll_aon_rf.h.